DCMTK Version 3.7.0 OFFIS DICOM Toolkit

Public Member Functions | Protected Member Functions | Private Attributes | List of all members
DRTImageIOD Class Reference

Interface class for RTImageIOD. More...

Inheritance diagram for DRTImageIOD:

## Public Member Functions
| DRTImageIOD ()
| default constructor
| DRTImageIOD (const DRTImageIOD &copy)
| copy constructor More...
virtual | ~DRTImageIOD ()
| destructor
DRTImageIOD & | operator= (const DRTImageIOD &copy)
| assignment operator More...
virtual void | clear ()
| clear all internal member variables
virtual OFBool | isValid ()
| check whether the current internal state is valid More...
virtual OFCondition | read (DcmItem &dataset)
| read object from dataset More...
virtual OFCondition | readPatientData (DcmItem &dataset)
| read PatientData from dataset More...
virtual OFCondition | readStudyData (DcmItem &dataset)
| read StudyData from dataset. More...
virtual OFCondition | readSeriesData (DcmItem &dataset)
| read SeriesData from dataset. More...
virtual OFCondition | write (DcmItem &dataset)
| write object to dataset More...
virtual OFBool | isClinicalTrialSubjectModulePresent (const OFBool complete=OFFalse)
| check whether ClinicalTrialSubjectModule (U) is present. More...
virtual OFBool | isPatientStudyModulePresent (const OFBool complete=OFFalse)
| check whether PatientStudyModule (U) is present. More...
virtual OFBool | isClinicalTrialStudyModulePresent (const OFBool complete=OFFalse)
| check whether ClinicalTrialStudyModule (U) is present. More...
virtual OFBool | isClinicalTrialSeriesModulePresent (const OFBool complete=OFFalse)
| check whether ClinicalTrialSeriesModule (U) is present. More...
virtual OFBool | isFrameOfReferenceModulePresent (const OFBool complete=OFFalse)
| check whether FrameOfReferenceModule (U) is present. More...
virtual OFBool | isGeneralReferenceModulePresent (const OFBool complete=OFFalse)
| check whether GeneralReferenceModule (U) is present. More...
virtual OFBool | isContrastBolusModulePresent (const OFBool complete=OFFalse)
| check whether ContrastBolusModule (C) is present. More...
virtual OFBool | isCineModulePresent (const OFBool complete=OFFalse)
| check whether CineModule (C) is present. More...
virtual OFBool | isMultiFrameModulePresent (const OFBool complete=OFFalse)
| check whether MultiFrameModule (C) is present. More...
virtual OFBool | isDeviceModulePresent (const OFBool complete=OFFalse)
| check whether DeviceModule (U) is present. More...
virtual OFBool | isModalityLUTModulePresent (const OFBool complete=OFFalse)
| check whether ModalityLUTModule (U) is present. More...
virtual OFBool | isVOILUTModulePresent (const OFBool complete=OFFalse)
| check whether VOILUTModule (U) is present. More...
virtual OFBool | isApprovalModulePresent (const OFBool complete=OFFalse)
| check whether ApprovalModule (U) is present. More...
virtual OFBool | isCommonInstanceReferenceModulePresent (const OFBool complete=OFFalse)
| check whether CommonInstanceReferenceModule (U) is present. More...
virtual OFBool | isFrameExtractionModulePresent (const OFBool complete=OFFalse)
| check whether FrameExtractionModule (C) is present. More...
virtual OFCondition | getAccessionNumber (OFString &value, const signed long pos=0) const
| get AccessionNumber (0008,0050) More...
virtual OFCondition | getAcquisitionDate (OFString &value, const signed long pos=0) const
| get AcquisitionDate (0008,0022) More...
virtual OFCondition | getAcquisitionDateTime (OFString &value, const signed long pos=0) const
| get AcquisitionDateTime (0008,002a) More...
virtual OFCondition | getAcquisitionDuration (Float64 &value, const unsigned long pos=0) const
| get AcquisitionDuration (0018,9073) More...
virtual OFCondition | getAcquisitionNumber (OFString &value, const signed long pos=0) const
| get AcquisitionNumber (0020,0012) More...
virtual OFCondition | getAcquisitionNumber (Sint32 &value, const unsigned long pos=0) const
| get AcquisitionNumber (0020,0012) More...
virtual OFCondition | getAcquisitionTime (OFString &value, const signed long pos=0) const
| get AcquisitionTime (0008,0032) More...
virtual OFCondition | getAcquisitionUID (OFString &value, const signed long pos=0) const
| get AcquisitionUID (0008,0017) More...
virtual OFCondition | getActualFrameDuration (OFString &value, const signed long pos=0) const
| get ActualFrameDuration (0018,1242) More...
virtual OFCondition | getActualFrameDuration (Sint32 &value, const unsigned long pos=0) const
| get ActualFrameDuration (0018,1242) More...
virtual OFCondition | getAdditionalPatientHistory (OFString &value, const signed long pos=0) const
| get AdditionalPatientHistory (0010,21b0) More...
virtual OFCondition | getAdmissionID (OFString &value, const signed long pos=0) const
| get AdmissionID (0038,0010) More...
virtual OFCondition | getAdmittingDiagnosesDescription (OFString &value, const signed long pos=0) const
| get AdmittingDiagnosesDescription (0008,1080) More...
virtual OFCondition | getAllergies (OFString &value, const signed long pos=0) const
| get Allergies (0010,2110) More...
virtual OFCondition | getApprovalStatus (OFString &value, const signed long pos=0) const
| get ApprovalStatus (300e,0002) More...
virtual OFCondition | getAuthorizationEquipmentCertificationNumber (OFString &value, const signed long pos=0) const
| get AuthorizationEquipmentCertificationNumber (0100,0426) More...
virtual OFCondition | getBarcodeValue (OFString &value, const signed long pos=0) const
| get BarcodeValue (2200,0005) More...
virtual OFCondition | getBeamLimitingDeviceAngle (OFString &value, const signed long pos=0) const
| get BeamLimitingDeviceAngle (300a,0120) More...
virtual OFCondition | getBeamLimitingDeviceAngle (Float64 &value, const unsigned long pos=0) const
| get BeamLimitingDeviceAngle (300a,0120) More...
virtual OFCondition | getBitsAllocated (Uint16 &value, const unsigned long pos=0) const
| get BitsAllocated (0028,0100) More...
virtual OFCondition | getBitsStored (Uint16 &value, const unsigned long pos=0) const
| get BitsStored (0028,0101) More...
virtual OFCondition | getBluePaletteColorLookupTableData (Uint16 *&value, unsigned long *count=NULL) const
| get BluePaletteColorLookupTableData (0028,1203) More...
virtual OFCondition | getBluePaletteColorLookupTableDescriptor (Uint16 &value, const unsigned long pos=0) const
| get BluePaletteColorLookupTableDescriptor (0028,1103) More...
virtual OFCondition | getBurnedInAnnotation (OFString &value, const signed long pos=0) const
| get BurnedInAnnotation (0028,0301) More...
virtual OFCondition | getCineRate (OFString &value, const signed long pos=0) const
| get CineRate (0018,0040) More...
virtual OFCondition | getCineRate (Sint32 &value, const unsigned long pos=0) const
| get CineRate (0018,0040) More...
virtual OFCondition | getClinicalTrialCoordinatingCenterName (OFString &value, const signed long pos=0) const
| get ClinicalTrialCoordinatingCenterName (0012,0060) More...
virtual OFCondition | getClinicalTrialProtocolEthicsCommitteeApprovalNumber (OFString &value, const signed long pos=0) const
| get ClinicalTrialProtocolEthicsCommitteeApprovalNumber (0012,0082) More...
virtual OFCondition | getClinicalTrialProtocolEthicsCommitteeName (OFString &value, const signed long pos=0) const
| get ClinicalTrialProtocolEthicsCommitteeName (0012,0081) More...
virtual OFCondition | getClinicalTrialProtocolID (OFString &value, const signed long pos=0) const
| get ClinicalTrialProtocolID (0012,0020) More...
virtual OFCondition | getClinicalTrialProtocolName (OFString &value, const signed long pos=0) const
| get ClinicalTrialProtocolName (0012,0021) More...
virtual OFCondition | getClinicalTrialSeriesDescription (OFString &value, const signed long pos=0) const
| get ClinicalTrialSeriesDescription (0012,0072) More...
virtual OFCondition | getClinicalTrialSeriesID (OFString &value, const signed long pos=0) const
| get ClinicalTrialSeriesID (0012,0071) More...
virtual OFCondition | getClinicalTrialSiteID (OFString &value, const signed long pos=0) const
| get ClinicalTrialSiteID (0012,0030) More...
virtual OFCondition | getClinicalTrialSiteName (OFString &value, const signed long pos=0) const
| get ClinicalTrialSiteName (0012,0031) More...
virtual OFCondition | getClinicalTrialSponsorName (OFString &value, const signed long pos=0) const
| get ClinicalTrialSponsorName (0012,0010) More...
virtual OFCondition | getClinicalTrialSubjectID (OFString &value, const signed long pos=0) const
| get ClinicalTrialSubjectID (0012,0040) More...
virtual OFCondition | getClinicalTrialSubjectReadingID (OFString &value, const signed long pos=0) const
| get ClinicalTrialSubjectReadingID (0012,0042) More...
virtual OFCondition | getClinicalTrialTimePointDescription (OFString &value, const signed long pos=0) const
| get ClinicalTrialTimePointDescription (0012,0051) More...
virtual OFCondition | getClinicalTrialTimePointID (OFString &value, const signed long pos=0) const
| get ClinicalTrialTimePointID (0012,0050) More...
virtual OFCondition | getColorSpace (OFString &value, const signed long pos=0) const
| get ColorSpace (0028,2002) More...
virtual OFCondition | getColumns (Uint16 &value, const unsigned long pos=0) const
| get Columns (0028,0011) More...
virtual OFCondition | getCommentsOnThePerformedProcedureStep (OFString &value, const signed long pos=0) const
| get CommentsOnThePerformedProcedureStep (0040,0280) More...
virtual OFCondition | getConsultingPhysicianName (OFString &value, const signed long pos=0) const
| get ConsultingPhysicianName (0008,009c) More...
virtual OFCondition | getContentDate (OFString &value, const signed long pos=0) const
| get ContentDate (0008,0023) More...
virtual OFCondition | getContentQualification (OFString &value, const signed long pos=0) const
| get ContentQualification (0018,9004) More...
virtual OFCondition | getContentTime (OFString &value, const signed long pos=0) const
| get ContentTime (0008,0033) More...
virtual OFCondition | getContrastBolusAgent (OFString &value, const signed long pos=0) const
| get ContrastBolusAgent (0018,0010) More...
virtual OFCondition | getContrastBolusIngredient (OFString &value, const signed long pos=0) const
| get ContrastBolusIngredient (0018,1048) More...
virtual OFCondition | getContrastBolusIngredientConcentration (OFString &value, const signed long pos=0) const
| get ContrastBolusIngredientConcentration (0018,1049) More...
virtual OFCondition | getContrastBolusIngredientConcentration (Float64 &value, const unsigned long pos=0) const
| get ContrastBolusIngredientConcentration (0018,1049) More...
virtual OFCondition | getContrastBolusRoute (OFString &value, const signed long pos=0) const
| get ContrastBolusRoute (0018,1040) More...
virtual OFCondition | getContrastBolusStartTime (OFString &value, const signed long pos=0) const
| get ContrastBolusStartTime (0018,1042) More...
virtual OFCondition | getContrastBolusStopTime (OFString &value, const signed long pos=0) const
| get ContrastBolusStopTime (0018,1043) More...
virtual OFCondition | getContrastBolusTotalDose (OFString &value, const signed long pos=0) const
| get ContrastBolusTotalDose (0018,1044) More...
virtual OFCondition | getContrastBolusTotalDose (Float64 &value, const unsigned long pos=0) const
| get ContrastBolusTotalDose (0018,1044) More...
virtual OFCondition | getContrastBolusVolume (OFString &value, const signed long pos=0) const
| get ContrastBolusVolume (0018,1041) More...
virtual OFCondition | getContrastBolusVolume (Float64 &value, const unsigned long pos=0) const
| get ContrastBolusVolume (0018,1041) More...
virtual OFCondition | getContrastFlowDuration (OFString &value, const signed long pos=0) const
| get ContrastFlowDuration (0018,1047) More...
virtual OFCondition | getContrastFlowDuration (Float64 &value, const unsigned long pos=0) const
| get ContrastFlowDuration (0018,1047) More...
virtual OFCondition | getContrastFlowDuration (OFVector< Float64 > &value) const
| get ContrastFlowDuration (0018,1047) More...
virtual OFCondition | getContrastFlowRate (OFString &value, const signed long pos=0) const
| get ContrastFlowRate (0018,1046) More...
virtual OFCondition | getContrastFlowRate (Float64 &value, const unsigned long pos=0) const
| get ContrastFlowRate (0018,1046) More...
virtual OFCondition | getContrastFlowRate (OFVector< Float64 > &value) const
| get ContrastFlowRate (0018,1046) More...
virtual OFCondition | getConversionType (OFString &value, const signed long pos=0) const
| get ConversionType (0008,0064) More...
virtual OFCondition | getDateOfLastCalibration (OFString &value, const signed long pos=0) const
| get DateOfLastCalibration (0018,1200) More...
virtual OFCondition | getDeidentificationMethod (OFString &value, const signed long pos=0) const
| get DeidentificationMethod (0012,0063) More...
virtual OFCondition | getDerivationDescription (OFString &value, const signed long pos=0) const
| get DerivationDescription (0008,2111) More...
virtual OFCondition | getDeviceSerialNumber (OFString &value, const signed long pos=0) const
| get DeviceSerialNumber (0018,1000) More...
virtual OFCondition | getDeviceUID (OFString &value, const signed long pos=0) const
| get DeviceUID (0018,1002) More...
virtual OFCondition | getEffectiveDuration (OFString &value, const signed long pos=0) const
| get EffectiveDuration (0018,0072) More...
virtual OFCondition | getEffectiveDuration (Float64 &value, const unsigned long pos=0) const
| get EffectiveDuration (0018,0072) More...
virtual OFCondition | getEncapsulatedPixelDataValueTotalLength (Uint64 &value, const unsigned long pos=0) const
| get EncapsulatedPixelDataValueTotalLength (7fe0,0003) More...
virtual OFCondition | getEndCumulativeMetersetWeight (OFString &value, const signed long pos=0) const
| get EndCumulativeMetersetWeight (300c,0009) More...
virtual OFCondition | getEndCumulativeMetersetWeight (Float64 &value, const unsigned long pos=0) const
| get EndCumulativeMetersetWeight (300c,0009) More...
virtual OFCondition | getEnhancedRTBeamLimitingDeviceDefinitionFlag (OFString &value, const signed long pos=0) const
| get EnhancedRTBeamLimitingDeviceDefinitionFlag (3008,00a3) More...
virtual OFCondition | getEthnicGroup (OFString &value, const signed long pos=0) const
| get EthnicGroup (0010,2160) More...
virtual OFCondition | getExposureTime (OFString &value, const signed long pos=0) const
| get ExposureTime (0018,1150) More...
virtual OFCondition | getExposureTime (Sint32 &value, const unsigned long pos=0) const
| get ExposureTime (0018,1150) More...
virtual OFCondition | getExposureTimeInms (Float64 &value, const unsigned long pos=0) const
| get ExposureTimeInms (0018,9328) More...
virtual OFCondition | getExtendedOffsetTable (Uint64 *&value, unsigned long *count=NULL) const
| get ExtendedOffsetTable (7fe0,0001) More...
virtual OFCondition | getExtendedOffsetTableLengths (Uint64 *&value, unsigned long *count=NULL) const
| get ExtendedOffsetTableLengths (7fe0,0002) More...
virtual OFCondition | getFractionNumber (OFString &value, const signed long pos=0) const
| get FractionNumber (3002,0029) More...
virtual OFCondition | getFractionNumber (Sint32 &value, const unsigned long pos=0) const
| get FractionNumber (3002,0029) More...
virtual OFCondition | getFrameDelay (OFString &value, const signed long pos=0) const
| get FrameDelay (0018,1066) More...
virtual OFCondition | getFrameDelay (Float64 &value, const unsigned long pos=0) const
| get FrameDelay (0018,1066) More...
virtual OFCondition | getFrameIncrementPointer (OFString &value, const signed long pos=0) const
| get FrameIncrementPointer (0028,0009) More...
virtual OFCondition | getFrameOfReferenceUID (OFString &value, const signed long pos=0) const
| get FrameOfReferenceUID (0020,0052) More...
virtual OFCondition | getFrameTime (OFString &value, const signed long pos=0) const
| get FrameTime (0018,1063) More...
virtual OFCondition | getFrameTime (Float64 &value, const unsigned long pos=0) const
| get FrameTime (0018,1063) More...
virtual OFCondition | getFrameTimeVector (OFString &value, const signed long pos=0) const
| get FrameTimeVector (0018,1065) More...
virtual OFCondition | getFrameTimeVector (Float64 &value, const unsigned long pos=0) const
| get FrameTimeVector (0018,1065) More...
virtual OFCondition | getFrameTimeVector (OFVector< Float64 > &value) const
| get FrameTimeVector (0018,1065) More...
virtual OFCondition | getGantryAngle (OFString &value, const signed long pos=0) const
| get GantryAngle (300a,011e) More...
virtual OFCondition | getGantryAngle (Float64 &value, const unsigned long pos=0) const
| get GantryAngle (300a,011e) More...
virtual OFCondition | getGantryID (OFString &value, const signed long pos=0) const
| get GantryID (0018,1008) More...
virtual OFCondition | getGantryPitchAngle (Float32 &value, const unsigned long pos=0) const
| get GantryPitchAngle (300a,014a) More...
virtual OFCondition | getGreenPaletteColorLookupTableData (Uint16 *&value, unsigned long *count=NULL) const
| get GreenPaletteColorLookupTableData (0028,1202) More...
virtual OFCondition | getGreenPaletteColorLookupTableDescriptor (Uint16 &value, const unsigned long pos=0) const
| get GreenPaletteColorLookupTableDescriptor (0028,1102) More...
virtual OFCondition | getHighBit (Uint16 &value, const unsigned long pos=0) const
| get HighBit (0028,0102) More...
virtual OFCondition | getICCProfile (Uint8 *&value, unsigned long *count=NULL) const
| get ICCProfile (0028,2000) More...
virtual OFCondition | getImageComments (OFString &value, const signed long pos=0) const
| get ImageComments (0020,4000) More...
virtual OFCondition | getImageLaterality (OFString &value, const signed long pos=0) const
| get ImageLaterality (0020,0062) More...
virtual OFCondition | getImagePlanePixelSpacing (OFString &value, const signed long pos=0) const
| get ImagePlanePixelSpacing (3002,0011) More...
virtual OFCondition | getImagePlanePixelSpacing (Float64 &value, const unsigned long pos=0) const
| get ImagePlanePixelSpacing (3002,0011) More...
virtual OFCondition | getImagePlanePixelSpacing (OFVector< Float64 > &value) const
| get ImagePlanePixelSpacing (3002,0011) More...
virtual OFCondition | getImageTriggerDelay (OFString &value, const signed long pos=0) const
| get ImageTriggerDelay (0018,1067) More...
virtual OFCondition | getImageTriggerDelay (Float64 &value, const unsigned long pos=0) const
| get ImageTriggerDelay (0018,1067) More...
virtual OFCondition | getImageType (OFString &value, const signed long pos=0) const
| get ImageType (0008,0008) More...
virtual OFCondition | getImagesInAcquisition (OFString &value, const signed long pos=0) const
| get ImagesInAcquisition (0020,1002) More...
virtual OFCondition | getImagesInAcquisition (Sint32 &value, const unsigned long pos=0) const
| get ImagesInAcquisition (0020,1002) More...
virtual OFCondition | getInstanceCoercionDateTime (OFString &value, const signed long pos=0) const
| get InstanceCoercionDateTime (0008,0015) More...
virtual OFCondition | getInstanceCreationDate (OFString &value, const signed long pos=0) const
| get InstanceCreationDate (0008,0012) More...
virtual OFCondition | getInstanceCreationTime (OFString &value, const signed long pos=0) const
| get InstanceCreationTime (0008,0013) More...
virtual OFCondition | getInstanceCreatorUID (OFString &value, const signed long pos=0) const
| get InstanceCreatorUID (0008,0014) More...
virtual OFCondition | getInstanceNumber (OFString &value, const signed long pos=0) const
| get InstanceNumber (0020,0013) More...
virtual OFCondition | getInstanceNumber (Sint32 &value, const unsigned long pos=0) const
| get InstanceNumber (0020,0013) More...
virtual OFCondition | getInstanceOriginStatus (OFString &value, const signed long pos=0) const
| get InstanceOriginStatus (0400,0600) More...
virtual OFCondition | getInstitutionAddress (OFString &value, const signed long pos=0) const
| get InstitutionAddress (0008,0081) More...
virtual OFCondition | getInstitutionName (OFString &value, const signed long pos=0) const
| get InstitutionName (0008,0080) More...
virtual OFCondition | getInstitutionalDepartmentName (OFString &value, const signed long pos=0) const
| get InstitutionalDepartmentName (0008,1040) More...
virtual OFCondition | getIrradiationEventUID (OFString &value, const signed long pos=0) const
| get IrradiationEventUID (0008,3010) More...
virtual OFCondition | getIsocenterPosition (OFString &value, const signed long pos=0) const
| get IsocenterPosition (300a,012c) More...
virtual OFCondition | getIsocenterPosition (Float64 &value, const unsigned long pos=0) const
| get IsocenterPosition (300a,012c) More...
virtual OFCondition | getIsocenterPosition (OFVector< Float64 > &value) const
| get IsocenterPosition (300a,012c) More...
virtual OFCondition | getIssuerOfPatientID (OFString &value, const signed long pos=0) const
| get IssuerOfPatientID (0010,0021) More...
virtual OFCondition | getLargestImagePixelValue (Uint16 &value, const unsigned long pos=0) const
| get LargestImagePixelValue (0028,0107) More...
virtual OFCondition | getLastMenstrualDate (OFString &value, const signed long pos=0) const
| get LastMenstrualDate (0010,21d0) More...
virtual OFCondition | getLongitudinalTemporalEventType (OFString &value, const signed long pos=0) const
| get LongitudinalTemporalEventType (0012,0053) More...
virtual OFCondition | getLongitudinalTemporalInformationModified (OFString &value, const signed long pos=0) const
| get LongitudinalTemporalInformationModified (0028,0303) More...
virtual OFCondition | getLongitudinalTemporalOffsetFromEvent (Float64 &value, const unsigned long pos=0) const
| get LongitudinalTemporalOffsetFromEvent (0012,0052) More...
virtual OFCondition | getLossyImageCompression (OFString &value, const signed long pos=0) const
| get LossyImageCompression (0028,2110) More...
virtual OFCondition | getLossyImageCompressionMethod (OFString &value, const signed long pos=0) const
| get LossyImageCompressionMethod (0028,2114) More...
virtual OFCondition | getLossyImageCompressionRatio (OFString &value, const signed long pos=0) const
| get LossyImageCompressionRatio (0028,2112) More...
virtual OFCondition | getLossyImageCompressionRatio (Float64 &value, const unsigned long pos=0) const
| get LossyImageCompressionRatio (0028,2112) More...
virtual OFCondition | getLossyImageCompressionRatio (OFVector< Float64 > &value) const
| get LossyImageCompressionRatio (0028,2112) More...
virtual OFCondition | getManufacturer (OFString &value, const signed long pos=0) const
| get Manufacturer (0008,0070) More...
virtual OFCondition | getManufacturerDeviceClassUID (OFString &value, const signed long pos=0) const
| get ManufacturerDeviceClassUID (0018,100b) More...
virtual OFCondition | getManufacturerModelName (OFString &value, const signed long pos=0) const
| get ManufacturerModelName (0008,1090) More...
virtual OFCondition | getMeasuredAPDimension (OFString &value, const signed long pos=0) const
| get MeasuredAPDimension (0010,1023) More...
virtual OFCondition | getMeasuredAPDimension (Float64 &value, const unsigned long pos=0) const
| get MeasuredAPDimension (0010,1023) More...
virtual OFCondition | getMeasuredLateralDimension (OFString &value, const signed long pos=0) const
| get MeasuredLateralDimension (0010,1024) More...
virtual OFCondition | getMeasuredLateralDimension (Float64 &value, const unsigned long pos=0) const
| get MeasuredLateralDimension (0010,1024) More...
virtual OFCondition | getMedicalAlerts (OFString &value, const signed long pos=0) const
| get MedicalAlerts (0010,2000) More...
virtual OFCondition | getMetersetExposure (OFString &value, const signed long pos=0) const
| get MetersetExposure (3002,0032) More...
virtual OFCondition | getMetersetExposure (Float64 &value, const unsigned long pos=0) const
| get MetersetExposure (3002,0032) More...
virtual OFCondition | getModality (OFString &value, const signed long pos=0) const
| get Modality (0008,0060) More...
virtual OFCondition | getNameOfPhysiciansReadingStudy (OFString &value, const signed long pos=0) const
| get NameOfPhysiciansReadingStudy (0008,1060) More...
virtual OFCondition | getNumberOfFrames (OFString &value, const signed long pos=0) const
| get NumberOfFrames (0028,0008) More...
virtual OFCondition | getNumberOfFrames (Sint32 &value, const unsigned long pos=0) const
| get NumberOfFrames (0028,0008) More...
virtual OFCondition | getOccupation (OFString &value, const signed long pos=0) const
| get Occupation (0010,2180) More...
virtual OFCondition | getOperatorsName (OFString &value, const signed long pos=0) const
| get OperatorsName (0008,1070) More...
virtual OFCondition | getOriginalSpecializedSOPClassUID (OFString &value, const signed long pos=0) const
| get OriginalSpecializedSOPClassUID (0008,001b) More...
virtual OFCondition | getOtherPatientNames (OFString &value, const signed long pos=0) const
| get OtherPatientNames (0010,1001) More...
virtual OFCondition | getPatientAge (OFString &value, const signed long pos=0) const
| get PatientAge (0010,1010) More...
virtual OFCondition | getPatientAlternativeCalendar (OFString &value, const signed long pos=0) const
| get PatientAlternativeCalendar (0010,0035) More...
virtual OFCondition | getPatientBirthDate (OFString &value, const signed long pos=0) const
| get PatientBirthDate (0010,0030) More...
virtual OFCondition | getPatientBirthDateInAlternativeCalendar (OFString &value, const signed long pos=0) const
| get PatientBirthDateInAlternativeCalendar (0010,0033) More...
virtual OFCondition | getPatientBirthTime (OFString &value, const signed long pos=0) const
| get PatientBirthTime (0010,0032) More...
virtual OFCondition | getPatientBodyMassIndex (OFString &value, const signed long pos=0) const
| get PatientBodyMassIndex (0010,1022) More...
virtual OFCondition | getPatientBodyMassIndex (Float64 &value, const unsigned long pos=0) const
| get PatientBodyMassIndex (0010,1022) More...
virtual OFCondition | getPatientBreedDescription (OFString &value, const signed long pos=0) const
| get PatientBreedDescription (0010,2292) More...
virtual OFCondition | getPatientComments (OFString &value, const signed long pos=0) const
| get PatientComments (0010,4000) More...
virtual OFCondition | getPatientDeathDateInAlternativeCalendar (OFString &value, const signed long pos=0) const
| get PatientDeathDateInAlternativeCalendar (0010,0034) More...
virtual OFCondition | getPatientID (OFString &value, const signed long pos=0) const
| get PatientID (0010,0020) More...
virtual OFCondition | getPatientIdentityRemoved (OFString &value, const signed long pos=0) const
| get PatientIdentityRemoved (0012,0062) More...
virtual OFCondition | getPatientName (OFString &value, const signed long pos=0) const
| get PatientName (0010,0010) More...
virtual OFCondition | getPatientOrientation (OFString &value, const signed long pos=0) const
| get PatientOrientation (0020,0020) More...
virtual OFCondition | getPatientPosition (OFString &value, const signed long pos=0) const
| get PatientPosition (0018,5100) More...
virtual OFCondition | getPatientSex (OFString &value, const signed long pos=0) const
| get PatientSex (0010,0040) More...
virtual OFCondition | getPatientSexNeutered (OFString &value, const signed long pos=0) const
| get PatientSexNeutered (0010,2203) More...
virtual OFCondition | getPatientSize (OFString &value, const signed long pos=0) const
| get PatientSize (0010,1020) More...
virtual OFCondition | getPatientSize (Float64 &value, const unsigned long pos=0) const
| get PatientSize (0010,1020) More...
virtual OFCondition | getPatientSpeciesDescription (OFString &value, const signed long pos=0) const
| get PatientSpeciesDescription (0010,2201) More...
virtual OFCondition | getPatientState (OFString &value, const signed long pos=0) const
| get PatientState (0038,0500) More...
virtual OFCondition | getPatientSupportAngle (OFString &value, const signed long pos=0) const
| get PatientSupportAngle (300a,0122) More...
virtual OFCondition | getPatientSupportAngle (Float64 &value, const unsigned long pos=0) const
| get PatientSupportAngle (300a,0122) More...
virtual OFCondition | getPatientWeight (OFString &value, const signed long pos=0) const
| get PatientWeight (0010,1030) More...
virtual OFCondition | getPatientWeight (Float64 &value, const unsigned long pos=0) const
| get PatientWeight (0010,1030) More...
virtual OFCondition | getPerformedProcedureStepDescription (OFString &value, const signed long pos=0) const
| get PerformedProcedureStepDescription (0040,0254) More...
virtual OFCondition | getPerformedProcedureStepEndDate (OFString &value, const signed long pos=0) const
| get PerformedProcedureStepEndDate (0040,0250) More...
virtual OFCondition | getPerformedProcedureStepEndTime (OFString &value, const signed long pos=0) const
| get PerformedProcedureStepEndTime (0040,0251) More...
virtual OFCondition | getPerformedProcedureStepID (OFString &value, const signed long pos=0) const
| get PerformedProcedureStepID (0040,0253) More...
virtual OFCondition | getPerformedProcedureStepStartDate (OFString &value, const signed long pos=0) const
| get PerformedProcedureStepStartDate (0040,0244) More...
virtual OFCondition | getPerformedProcedureStepStartTime (OFString &value, const signed long pos=0) const
| get PerformedProcedureStepStartTime (0040,0245) More...
virtual OFCondition | getPhotometricInterpretation (OFString &value, const signed long pos=0) const
| get PhotometricInterpretation (0028,0004) More...
virtual OFCondition | getPhysiciansOfRecord (OFString &value, const signed long pos=0) const
| get PhysiciansOfRecord (0008,1048) More...
virtual OFCondition | getPixelAspectRatio (OFString &value, const signed long pos=0) const
| get PixelAspectRatio (0028,0034) More...
virtual OFCondition | getPixelAspectRatio (Sint32 &value, const unsigned long pos=0) const
| get PixelAspectRatio (0028,0034) More...
virtual OFCondition | getPixelDataProviderURL (OFString &value, const signed long pos=0) const
| get PixelDataProviderURL (0028,7fe0) More...
virtual OFCondition | getPixelIntensityRelationship (OFString &value, const signed long pos=0) const
| get PixelIntensityRelationship (0028,1040) More...
virtual OFCondition | getPixelIntensityRelationshipSign (Sint16 &value, const unsigned long pos=0) const
| get PixelIntensityRelationshipSign (0028,1041) More...
virtual OFCondition | getPixelPaddingRangeLimit (Uint16 &value, const unsigned long pos=0) const
| get PixelPaddingRangeLimit (0028,0121) More...
virtual OFCondition | getPixelPaddingValue (Uint16 &value, const unsigned long pos=0) const
| get PixelPaddingValue (0028,0120) More...
virtual OFCondition | getPixelRepresentation (Uint16 &value, const unsigned long pos=0) const
| get PixelRepresentation (0028,0103) More...
virtual OFCondition | getPlanarConfiguration (Uint16 &value, const unsigned long pos=0) const
| get PlanarConfiguration (0028,0006) More...
virtual OFCondition | getPositionReferenceIndicator (OFString &value, const signed long pos=0) const
| get PositionReferenceIndicator (0020,1040) More...
virtual OFCondition | getPreferredPlaybackSequencing (Uint16 &value, const unsigned long pos=0) const
| get PreferredPlaybackSequencing (0018,1244) More...
virtual OFCondition | getPregnancyStatus (Uint16 &value, const unsigned long pos=0) const
| get PregnancyStatus (0010,21c0) More...
virtual OFCondition | getPresentationLUTShape (OFString &value, const signed long pos=0) const
| get PresentationLUTShape (2050,0020) More...
virtual OFCondition | getPrimaryDosimeterUnit (OFString &value, const signed long pos=0) const
| get PrimaryDosimeterUnit (300a,00b3) More...
virtual OFCondition | getQualityControlImage (OFString &value, const signed long pos=0) const
| get QualityControlImage (0028,0300) More...
virtual OFCondition | getQualityControlSubject (OFString &value, const signed long pos=0) const
| get QualityControlSubject (0010,0200) More...
virtual OFCondition | getQueryRetrieveView (OFString &value, const signed long pos=0) const
| get QueryRetrieveView (0008,0053) More...
virtual OFCondition | getRTImageDescription (OFString &value, const signed long pos=0) const
| get RTImageDescription (3002,0004) More...
virtual OFCondition | getRTImageLabel (OFString &value, const signed long pos=0) const
| get RTImageLabel (3002,0002) More...
virtual OFCondition | getRTImageName (OFString &value, const signed long pos=0) const
| get RTImageName (3002,0003) More...
virtual OFCondition | getRTImageOrientation (OFString &value, const signed long pos=0) const
| get RTImageOrientation (3002,0010) More...
virtual OFCondition | getRTImageOrientation (Float64 &value, const unsigned long pos=0) const
| get RTImageOrientation (3002,0010) More...
virtual OFCondition | getRTImageOrientation (OFVector< Float64 > &value) const
| get RTImageOrientation (3002,0010) More...
virtual OFCondition | getRTImagePlane (OFString &value, const signed long pos=0) const
| get RTImagePlane (3002,000c) More...
virtual OFCondition | getRTImagePosition (OFString &value, const signed long pos=0) const
| get RTImagePosition (3002,0012) More...
virtual OFCondition | getRTImagePosition (Float64 &value, const unsigned long pos=0) const
| get RTImagePosition (3002,0012) More...
virtual OFCondition | getRTImagePosition (OFVector< Float64 > &value) const
| get RTImagePosition (3002,0012) More...
virtual OFCondition | getRTImageSID (OFString &value, const signed long pos=0) const
| get RTImageSID (3002,0026) More...
virtual OFCondition | getRTImageSID (Float64 &value, const unsigned long pos=0) const
| get RTImageSID (3002,0026) More...
virtual OFCondition | getRadiationMachineName (OFString &value, const signed long pos=0) const
| get RadiationMachineName (3002,0020) More...
virtual OFCondition | getRadiationMachineSAD (OFString &value, const signed long pos=0) const
| get RadiationMachineSAD (3002,0022) More...
virtual OFCondition | getRadiationMachineSAD (Float64 &value, const unsigned long pos=0) const
| get RadiationMachineSAD (3002,0022) More...
virtual OFCondition | getRadiationMachineSSD (OFString &value, const signed long pos=0) const
| get RadiationMachineSSD (3002,0024) More...
virtual OFCondition | getRadiationMachineSSD (Float64 &value, const unsigned long pos=0) const
| get RadiationMachineSSD (3002,0024) More...
virtual OFCondition | getReasonForVisit (OFString &value, const signed long pos=0) const
| get ReasonForVisit (0032,1066) More...
virtual OFCondition | getRecognizableVisualFeatures (OFString &value, const signed long pos=0) const
| get RecognizableVisualFeatures (0028,0302) More...
virtual OFCondition | getRecommendedDisplayFrameRate (OFString &value, const signed long pos=0) const
| get RecommendedDisplayFrameRate (0008,2144) More...
virtual OFCondition | getRecommendedDisplayFrameRate (Sint32 &value, const unsigned long pos=0) const
| get RecommendedDisplayFrameRate (0008,2144) More...
virtual OFCondition | getRedPaletteColorLookupTableData (Uint16 *&value, unsigned long *count=NULL) const
| get RedPaletteColorLookupTableData (0028,1201) More...
virtual OFCondition | getRedPaletteColorLookupTableDescriptor (Uint16 &value, const unsigned long pos=0) const
| get RedPaletteColorLookupTableDescriptor (0028,1101) More...
virtual OFCondition | getReferencedBeamNumber (OFString &value, const signed long pos=0) const
| get ReferencedBeamNumber (300c,0006) More...
virtual OFCondition | getReferencedBeamNumber (Sint32 &value, const unsigned long pos=0) const
| get ReferencedBeamNumber (300c,0006) More...
virtual OFCondition | getReferencedFractionGroupNumber (OFString &value, const signed long pos=0) const
| get ReferencedFractionGroupNumber (300c,0022) More...
virtual OFCondition | getReferencedFractionGroupNumber (Sint32 &value, const unsigned long pos=0) const
| get ReferencedFractionGroupNumber (300c,0022) More...
virtual OFCondition | getReferringPhysicianName (OFString &value, const signed long pos=0) const
| get ReferringPhysicianName (0008,0090) More...
virtual OFCondition | getRelatedGeneralSOPClassUID (OFString &value, const signed long pos=0) const
| get RelatedGeneralSOPClassUID (0008,001a) More...
virtual OFCondition | getReportedValuesOrigin (OFString &value, const signed long pos=0) const
| get ReportedValuesOrigin (3002,000a) More...
virtual OFCondition | getRequestingService (OFString &value, const signed long pos=0) const
| get RequestingService (0032,1033) More...
virtual OFCondition | getRescaleIntercept (OFString &value, const signed long pos=0) const
| get RescaleIntercept (0028,1052) More...
virtual OFCondition | getRescaleIntercept (Float64 &value, const unsigned long pos=0) const
| get RescaleIntercept (0028,1052) More...
virtual OFCondition | getRescaleSlope (OFString &value, const signed long pos=0) const
| get RescaleSlope (0028,1053) More...
virtual OFCondition | getRescaleSlope (Float64 &value, const unsigned long pos=0) const
| get RescaleSlope (0028,1053) More...
virtual OFCondition | getRescaleType (OFString &value, const signed long pos=0) const
| get RescaleType (0028,1054) More...
virtual OFCondition | getResponsibleOrganization (OFString &value, const signed long pos=0) const
| get ResponsibleOrganization (0010,2299) More...
virtual OFCondition | getResponsiblePerson (OFString &value, const signed long pos=0) const
| get ResponsiblePerson (0010,2297) More...
virtual OFCondition | getResponsiblePersonRole (OFString &value, const signed long pos=0) const
| get ResponsiblePersonRole (0010,2298) More...
virtual OFCondition | getReviewDate (OFString &value, const signed long pos=0) const
| get ReviewDate (300e,0004) More...
virtual OFCondition | getReviewTime (OFString &value, const signed long pos=0) const
| get ReviewTime (300e,0005) More...
virtual OFCondition | getReviewerName (OFString &value, const signed long pos=0) const
| get ReviewerName (300e,0008) More...
virtual OFCondition | getRows (Uint16 &value, const unsigned long pos=0) const
| get Rows (0028,0010) More...
virtual OFCondition | getSOPAuthorizationComment (OFString &value, const signed long pos=0) const
| get SOPAuthorizationComment (0100,0424) More...
virtual OFCondition | getSOPAuthorizationDateTime (OFString &value, const signed long pos=0) const
| get SOPAuthorizationDateTime (0100,0420) More...
virtual OFCondition | getSOPClassUID (OFString &value, const signed long pos=0) const
| get SOPClassUID (0008,0016) More...
virtual OFCondition | getSOPInstanceStatus (OFString &value, const signed long pos=0) const
| get SOPInstanceStatus (0100,0410) More...
virtual OFCondition | getSOPInstanceUID (OFString &value, const signed long pos=0) const
| get SOPInstanceUID (0008,0018) More...
virtual OFCondition | getSamplesPerPixel (Uint16 &value, const unsigned long pos=0) const
| get SamplesPerPixel (0028,0002) More...
virtual OFCondition | getSeriesDate (OFString &value, const signed long pos=0) const
| get SeriesDate (0008,0021) More...
virtual OFCondition | getSeriesDescription (OFString &value, const signed long pos=0) const
| get SeriesDescription (0008,103e) More...
virtual OFCondition | getSeriesInstanceUID (OFString &value, const signed long pos=0) const
| get SeriesInstanceUID (0020,000e) More...
virtual OFCondition | getSeriesNumber (OFString &value, const signed long pos=0) const
| get SeriesNumber (0020,0011) More...
virtual OFCondition | getSeriesNumber (Sint32 &value, const unsigned long pos=0) const
| get SeriesNumber (0020,0011) More...
virtual OFCondition | getSeriesTime (OFString &value, const signed long pos=0) const
| get SeriesTime (0008,0031) More...
virtual OFCondition | getServiceEpisodeDescription (OFString &value, const signed long pos=0) const
| get ServiceEpisodeDescription (0038,0062) More...
virtual OFCondition | getServiceEpisodeID (OFString &value, const signed long pos=0) const
| get ServiceEpisodeID (0038,0060) More...
virtual OFCondition | getSmallestImagePixelValue (Uint16 &value, const unsigned long pos=0) const
| get SmallestImagePixelValue (0028,0106) More...
virtual OFCondition | getSmokingStatus (OFString &value, const signed long pos=0) const
| get SmokingStatus (0010,21a0) More...
virtual OFCondition | getSoftwareVersions (OFString &value, const signed long pos=0) const
| get SoftwareVersions (0018,1020) More...
virtual OFCondition | getSourceToReferenceObjectDistance (OFString &value, const signed long pos=0) const
| get SourceToReferenceObjectDistance (3002,0028) More...
virtual OFCondition | getSourceToReferenceObjectDistance (Float64 &value, const unsigned long pos=0) const
| get SourceToReferenceObjectDistance (3002,0028) More...
virtual OFCondition | getSpatialResolution (OFString &value, const signed long pos=0) const
| get SpatialResolution (0018,1050) More...
virtual OFCondition | getSpatialResolution (Float64 &value, const unsigned long pos=0) const
| get SpatialResolution (0018,1050) More...
virtual OFCondition | getSpecificCharacterSet (OFString &value, const signed long pos=0) const
| get SpecificCharacterSet (0008,0005) More...
virtual OFCondition | getStartCumulativeMetersetWeight (OFString &value, const signed long pos=0) const
| get StartCumulativeMetersetWeight (300c,0008) More...
virtual OFCondition | getStartCumulativeMetersetWeight (Float64 &value, const unsigned long pos=0) const
| get StartCumulativeMetersetWeight (300c,0008) More...
virtual OFCondition | getStartTrim (OFString &value, const signed long pos=0) const
| get StartTrim (0008,2142) More...
virtual OFCondition | getStartTrim (Sint32 &value, const unsigned long pos=0) const
| get StartTrim (0008,2142) More...
virtual OFCondition | getStationName (OFString &value, const signed long pos=0) const
| get StationName (0008,1010) More...
virtual OFCondition | getStereoPairsPresent (OFString &value, const signed long pos=0) const
| get StereoPairsPresent (0022,0028) More...
virtual OFCondition | getStopTrim (OFString &value, const signed long pos=0) const
| get StopTrim (0008,2143) More...
virtual OFCondition | getStopTrim (Sint32 &value, const unsigned long pos=0) const
| get StopTrim (0008,2143) More...
virtual OFCondition | getStrainAdditionalInformation (OFString &value, const signed long pos=0) const
| get StrainAdditionalInformation (0010,0218) More...
virtual OFCondition | getStrainDescription (OFString &value, const signed long pos=0) const
| get StrainDescription (0010,0212) More...
virtual OFCondition | getStrainNomenclature (OFString &value, const signed long pos=0) const
| get StrainNomenclature (0010,0213) More...
virtual OFCondition | getStudyDate (OFString &value, const signed long pos=0) const
| get StudyDate (0008,0020) More...
virtual OFCondition | getStudyDescription (OFString &value, const signed long pos=0) const
| get StudyDescription (0008,1030) More...
virtual OFCondition | getStudyID (OFString &value, const signed long pos=0) const
| get StudyID (0020,0010) More...
virtual OFCondition | getStudyInstanceUID (OFString &value, const signed long pos=0) const
| get StudyInstanceUID (0020,000d) More...
virtual OFCondition | getStudyTime (OFString &value, const signed long pos=0) const
| get StudyTime (0008,0030) More...
virtual OFCondition | getTableTopEccentricAngle (OFString &value, const signed long pos=0) const
| get TableTopEccentricAngle (300a,0125) More...
virtual OFCondition | getTableTopEccentricAngle (Float64 &value, const unsigned long pos=0) const
| get TableTopEccentricAngle (300a,0125) More...
virtual OFCondition | getTableTopEccentricAxisDistance (OFString &value, const signed long pos=0) const
| get TableTopEccentricAxisDistance (300a,0124) More...
virtual OFCondition | getTableTopEccentricAxisDistance (Float64 &value, const unsigned long pos=0) const
| get TableTopEccentricAxisDistance (300a,0124) More...
virtual OFCondition | getTableTopLateralPosition (OFString &value, const signed long pos=0) const
| get TableTopLateralPosition (300a,012a) More...
virtual OFCondition | getTableTopLateralPosition (Float64 &value, const unsigned long pos=0) const
| get TableTopLateralPosition (300a,012a) More...
virtual OFCondition | getTableTopLongitudinalPosition (OFString &value, const signed long pos=0) const
| get TableTopLongitudinalPosition (300a,0129) More...
virtual OFCondition | getTableTopLongitudinalPosition (Float64 &value, const unsigned long pos=0) const
| get TableTopLongitudinalPosition (300a,0129) More...
virtual OFCondition | getTableTopPitchAngle (Float32 &value, const unsigned long pos=0) const
| get TableTopPitchAngle (300a,0140) More...
virtual OFCondition | getTableTopRollAngle (Float32 &value, const unsigned long pos=0) const
| get TableTopRollAngle (300a,0144) More...
virtual OFCondition | getTableTopVerticalPosition (OFString &value, const signed long pos=0) const
| get TableTopVerticalPosition (300a,0128) More...
virtual OFCondition | getTableTopVerticalPosition (Float64 &value, const unsigned long pos=0) const
| get TableTopVerticalPosition (300a,0128) More...
virtual OFCondition | getTimeOfLastCalibration (OFString &value, const signed long pos=0) const
| get TimeOfLastCalibration (0018,1201) More...
virtual OFCondition | getTimezoneOffsetFromUTC (OFString &value, const signed long pos=0) const
| get TimezoneOffsetFromUTC (0008,0201) More...
virtual OFCondition | getTreatmentSessionUID (OFString &value, const signed long pos=0) const
| get TreatmentSessionUID (300a,0700) More...
virtual OFCondition | getTypeOfPatientID (OFString &value, const signed long pos=0) const
| get TypeOfPatientID (0010,0022) More...
virtual OFCondition | getVOILUTFunction (OFString &value, const signed long pos=0) const
| get VOILUTFunction (0028,1056) More...
virtual OFCondition | getWindowCenter (OFString &value, const signed long pos=0) const
| get WindowCenter (0028,1050) More...
virtual OFCondition | getWindowCenter (Float64 &value, const unsigned long pos=0) const
| get WindowCenter (0028,1050) More...
virtual OFCondition | getWindowCenter (OFVector< Float64 > &value) const
| get WindowCenter (0028,1050) More...
virtual OFCondition | getWindowCenterWidthExplanation (OFString &value, const signed long pos=0) const
| get WindowCenterWidthExplanation (0028,1055) More...
virtual OFCondition | getWindowWidth (OFString &value, const signed long pos=0) const
| get WindowWidth (0028,1051) More...
virtual OFCondition | getWindowWidth (Float64 &value, const unsigned long pos=0) const
| get WindowWidth (0028,1051) More...
virtual OFCondition | getWindowWidth (OFVector< Float64 > &value) const
| get WindowWidth (0028,1051) More...
virtual OFCondition | getXRayImageReceptorAngle (OFString &value, const signed long pos=0) const
| get XRayImageReceptorAngle (3002,000e) More...
virtual OFCondition | getXRayImageReceptorAngle (Float64 &value, const unsigned long pos=0) const
| get XRayImageReceptorAngle (3002,000e) More...
virtual OFCondition | getXRayImageReceptorTranslation (OFString &value, const signed long pos=0) const
| get XRayImageReceptorTranslation (3002,000d) More...
virtual OFCondition | getXRayImageReceptorTranslation (Float64 &value, const unsigned long pos=0) const
| get XRayImageReceptorTranslation (3002,000d) More...
virtual OFCondition | getXRayImageReceptorTranslation (OFVector< Float64 > &value) const
| get XRayImageReceptorTranslation (3002,000d) More...
DcmPixelData & | getPixelData ()
| get PixelData (7fe0,0010) More...
const DcmPixelData & | getPixelData () const
| get PixelData (7fe0,0010) More...
DRTAdmittingDiagnosesCodeSequence & | getAdmittingDiagnosesCodeSequence ()
| get AdmittingDiagnosesCodeSequence (0008,1084) More...
const DRTAdmittingDiagnosesCodeSequence & | getAdmittingDiagnosesCodeSequence () const
| get AdmittingDiagnosesCodeSequence (0008,1084) More...
DRTAnatomicRegionSequence & | getAnatomicRegionSequence ()
| get AnatomicRegionSequence (0008,2218) More...
const DRTAnatomicRegionSequence & | getAnatomicRegionSequence () const
| get AnatomicRegionSequence (0008,2218) More...
DRTBreedRegistrationSequence & | getBreedRegistrationSequence ()
| get BreedRegistrationSequence (0010,2294) More...
const DRTBreedRegistrationSequence & | getBreedRegistrationSequence () const
| get BreedRegistrationSequence (0010,2294) More...
DRTClinicalTrialTimePointTypeCodeSequence & | getClinicalTrialTimePointTypeCodeSequence ()
| get ClinicalTrialTimePointTypeCodeSequence (0012,0054) More...
const DRTClinicalTrialTimePointTypeCodeSequence & | getClinicalTrialTimePointTypeCodeSequence () const
| get ClinicalTrialTimePointTypeCodeSequence (0012,0054) More...
DRTCodingSchemeIdentificationSequence & | getCodingSchemeIdentificationSequence ()
| get CodingSchemeIdentificationSequence (0008,0110) More...
const DRTCodingSchemeIdentificationSequence & | getCodingSchemeIdentificationSequence () const
| get CodingSchemeIdentificationSequence (0008,0110) More...
DRTConsentForClinicalTrialUseSequence & | getConsentForClinicalTrialUseSequence ()
| get ConsentForClinicalTrialUseSequence (0012,0083) More...
const DRTConsentForClinicalTrialUseSequence & | getConsentForClinicalTrialUseSequence () const
| get ConsentForClinicalTrialUseSequence (0012,0083) More...
DRTConsultingPhysicianIdentificationSequence & | getConsultingPhysicianIdentificationSequence ()
| get ConsultingPhysicianIdentificationSequence (0008,009d) More...
const DRTConsultingPhysicianIdentificationSequence & | getConsultingPhysicianIdentificationSequence () const
| get ConsultingPhysicianIdentificationSequence (0008,009d) More...
DRTContextGroupIdentificationSequence & | getContextGroupIdentificationSequence ()
| get ContextGroupIdentificationSequence (0008,0123) More...
const DRTContextGroupIdentificationSequence & | getContextGroupIdentificationSequence () const
| get ContextGroupIdentificationSequence (0008,0123) More...
DRTContrastBolusAdministrationRouteSequence & | getContrastBolusAdministrationRouteSequence ()
| get ContrastBolusAdministrationRouteSequence (0018,0014) More...
const DRTContrastBolusAdministrationRouteSequence & | getContrastBolusAdministrationRouteSequence () const
| get ContrastBolusAdministrationRouteSequence (0018,0014) More...
DRTContrastBolusAgentSequence & | getContrastBolusAgentSequence ()
| get ContrastBolusAgentSequence (0018,0012) More...
const DRTContrastBolusAgentSequence & | getContrastBolusAgentSequence () const
| get ContrastBolusAgentSequence (0018,0012) More...
DRTContributingEquipmentSequence & | getContributingEquipmentSequence ()
| get ContributingEquipmentSequence (0018,a001) More...
const DRTContributingEquipmentSequence & | getContributingEquipmentSequence () const
| get ContributingEquipmentSequence (0018,a001) More...
DRTConversionSourceAttributesSequence & | getConversionSourceAttributesSequence ()
| get ConversionSourceAttributesSequence (0020,9172) More...
const DRTConversionSourceAttributesSequence & | getConversionSourceAttributesSequence () const
| get ConversionSourceAttributesSequence (0020,9172) More...
DRTDeidentificationMethodCodeSequence & | getDeidentificationMethodCodeSequence ()
| get DeidentificationMethodCodeSequence (0012,0064) More...
const DRTDeidentificationMethodCodeSequence & | getDeidentificationMethodCodeSequence () const
| get DeidentificationMethodCodeSequence (0012,0064) More...
DRTDerivationCodeSequence & | getDerivationCodeSequence ()
| get DerivationCodeSequence (0008,9215) More...
const DRTDerivationCodeSequence & | getDerivationCodeSequence () const
| get DerivationCodeSequence (0008,9215) More...
DRTDeviceSequence & | getDeviceSequence ()
| get DeviceSequence (0050,0010) More...
const DRTDeviceSequence & | getDeviceSequence () const
| get DeviceSequence (0050,0010) More...
DRTDigitalSignaturesSequence & | getDigitalSignaturesSequence ()
| get DigitalSignaturesSequence (fffa,fffa) More...
const DRTDigitalSignaturesSequence & | getDigitalSignaturesSequence () const
| get DigitalSignaturesSequence (fffa,fffa) More...
DRTEncryptedAttributesSequence & | getEncryptedAttributesSequence ()
| get EncryptedAttributesSequence (0400,0500) More...
const DRTEncryptedAttributesSequence & | getEncryptedAttributesSequence () const
| get EncryptedAttributesSequence (0400,0500) More...
DRTEnhancedRTBeamLimitingDeviceSequence & | getEnhancedRTBeamLimitingDeviceSequence ()
| get EnhancedRTBeamLimitingDeviceSequence (3008,00a1) More...
const DRTEnhancedRTBeamLimitingDeviceSequence & | getEnhancedRTBeamLimitingDeviceSequence () const
| get EnhancedRTBeamLimitingDeviceSequence (3008,00a1) More...
DRTExposureSequence & | getExposureSequence ()
| get ExposureSequence (3002,0030) More...
const DRTExposureSequence & | getExposureSequence () const
| get ExposureSequence (3002,0030) More...
DRTFluenceMapSequence & | getFluenceMapSequence ()
| get FluenceMapSequence (3002,0040) More...
const DRTFluenceMapSequence & | getFluenceMapSequence () const
| get FluenceMapSequence (3002,0040) More...
DRTFrameExtractionSequence & | getFrameExtractionSequence ()
| get FrameExtractionSequence (0008,1164) More...
const DRTFrameExtractionSequence & | getFrameExtractionSequence () const
| get FrameExtractionSequence (0008,1164) More...
DRTGeneticModificationsSequence & | getGeneticModificationsSequence ()
| get GeneticModificationsSequence (0010,0221) More...
const DRTGeneticModificationsSequence & | getGeneticModificationsSequence () const
| get GeneticModificationsSequence (0010,0221) More...
DRTGroupOfPatientsIdentificationSequence & | getGroupOfPatientsIdentificationSequence ()
| get GroupOfPatientsIdentificationSequence (0010,0027) More...
const DRTGroupOfPatientsIdentificationSequence & | getGroupOfPatientsIdentificationSequence () const
| get GroupOfPatientsIdentificationSequence (0010,0027) More...
DRTHL7StructuredDocumentReferenceSequence & | getHL7StructuredDocumentReferenceSequence ()
| get HL7StructuredDocumentReferenceSequence (0040,a390) More...
const DRTHL7StructuredDocumentReferenceSequence & | getHL7StructuredDocumentReferenceSequence () const
| get HL7StructuredDocumentReferenceSequence (0040,a390) More...
DRTIconImageSequence & | getIconImageSequence ()
| get IconImageSequence (0088,0200) More...
const DRTIconImageSequence & | getIconImageSequence () const
| get IconImageSequence (0088,0200) More...
DRTInstitutionalDepartmentTypeCodeSequence & | getInstitutionalDepartmentTypeCodeSequence ()
| get InstitutionalDepartmentTypeCodeSequence (0008,1041) More...
const DRTInstitutionalDepartmentTypeCodeSequence & | getInstitutionalDepartmentTypeCodeSequence () const
| get InstitutionalDepartmentTypeCodeSequence (0008,1041) More...
DRTIssuerOfAccessionNumberSequence & | getIssuerOfAccessionNumberSequence ()
| get IssuerOfAccessionNumberSequence (0008,0051) More...
const DRTIssuerOfAccessionNumberSequence & | getIssuerOfAccessionNumberSequence () const
| get IssuerOfAccessionNumberSequence (0008,0051) More...
DRTIssuerOfAdmissionIDSequence & | getIssuerOfAdmissionIDSequence ()
| get IssuerOfAdmissionIDSequence (0038,0014) More...
const DRTIssuerOfAdmissionIDSequence & | getIssuerOfAdmissionIDSequence () const
| get IssuerOfAdmissionIDSequence (0038,0014) More...
DRTIssuerOfPatientIDQualifiersSequence & | getIssuerOfPatientIDQualifiersSequence ()
| get IssuerOfPatientIDQualifiersSequence (0010,0024) More...
const DRTIssuerOfPatientIDQualifiersSequence & | getIssuerOfPatientIDQualifiersSequence () const
| get IssuerOfPatientIDQualifiersSequence (0010,0024) More...
DRTIssuerOfServiceEpisodeIDSequence & | getIssuerOfServiceEpisodeIDSequence ()
| get IssuerOfServiceEpisodeIDSequence (0038,0064) More...
const DRTIssuerOfServiceEpisodeIDSequence & | getIssuerOfServiceEpisodeIDSequence () const
| get IssuerOfServiceEpisodeIDSequence (0038,0064) More...
DRTMACParametersSequence & | getMACParametersSequence ()
| get MACParametersSequence (4ffe,0001) More...
const DRTMACParametersSequence & | getMACParametersSequence () const
| get MACParametersSequence (4ffe,0001) More...
DRTMappingResourceIdentificationSequence & | getMappingResourceIdentificationSequence ()
| get MappingResourceIdentificationSequence (0008,0124) More...
const DRTMappingResourceIdentificationSequence & | getMappingResourceIdentificationSequence () const
| get MappingResourceIdentificationSequence (0008,0124) More...
DRTModalityLUTSequence & | getModalityLUTSequence ()
| get ModalityLUTSequence (0028,3000) More...
const DRTModalityLUTSequence & | getModalityLUTSequence () const
| get ModalityLUTSequence (0028,3000) More...
DRTMultiplexedAudioChannelsDescriptionCodeSequence & | getMultiplexedAudioChannelsDescriptionCodeSequence ()
| get MultiplexedAudioChannelsDescriptionCodeSequence (003a,0300) More...
const DRTMultiplexedAudioChannelsDescriptionCodeSequence & | getMultiplexedAudioChannelsDescriptionCodeSequence () const
| get MultiplexedAudioChannelsDescriptionCodeSequence (003a,0300) More...
DRTOperatorIdentificationSequence & | getOperatorIdentificationSequence ()
| get OperatorIdentificationSequence (0008,1072) More...
const DRTOperatorIdentificationSequence & | getOperatorIdentificationSequence () const
| get OperatorIdentificationSequence (0008,1072) More...
DRTOriginalAttributesSequence & | getOriginalAttributesSequence ()
| get OriginalAttributesSequence (0400,0561) More...
const DRTOriginalAttributesSequence & | getOriginalAttributesSequence () const
| get OriginalAttributesSequence (0400,0561) More...
DRTOtherPatientIDsSequence & | getOtherPatientIDsSequence ()
| get OtherPatientIDsSequence (0010,1002) More...
const DRTOtherPatientIDsSequence & | getOtherPatientIDsSequence () const
| get OtherPatientIDsSequence (0010,1002) More...
DRTPatientBreedCodeSequence & | getPatientBreedCodeSequence ()
| get PatientBreedCodeSequence (0010,2293) More...
const DRTPatientBreedCodeSequence & | getPatientBreedCodeSequence () const
| get PatientBreedCodeSequence (0010,2293) More...
DRTPatientSizeCodeSequence & | getPatientSizeCodeSequence ()
| get PatientSizeCodeSequence (0010,1021) More...
const DRTPatientSizeCodeSequence & | getPatientSizeCodeSequence () const
| get PatientSizeCodeSequence (0010,1021) More...
DRTPatientSpeciesCodeSequence & | getPatientSpeciesCodeSequence ()
| get PatientSpeciesCodeSequence (0010,2202) More...
const DRTPatientSpeciesCodeSequence & | getPatientSpeciesCodeSequence () const
| get PatientSpeciesCodeSequence (0010,2202) More...
DRTPerformedProtocolCodeSequence & | getPerformedProtocolCodeSequence ()
| get PerformedProtocolCodeSequence (0040,0260) More...
const DRTPerformedProtocolCodeSequence & | getPerformedProtocolCodeSequence () const
| get PerformedProtocolCodeSequence (0040,0260) More...
DRTPhysiciansOfRecordIdentificationSequence & | getPhysiciansOfRecordIdentificationSequence ()
| get PhysiciansOfRecordIdentificationSequence (0008,1049) More...
const DRTPhysiciansOfRecordIdentificationSequence & | getPhysiciansOfRecordIdentificationSequence () const
| get PhysiciansOfRecordIdentificationSequence (0008,1049) More...
DRTPhysiciansReadingStudyIdentificationSequence & | getPhysiciansReadingStudyIdentificationSequence ()
| get PhysiciansReadingStudyIdentificationSequence (0008,1062) More...
const DRTPhysiciansReadingStudyIdentificationSequence & | getPhysiciansReadingStudyIdentificationSequence () const
| get PhysiciansReadingStudyIdentificationSequence (0008,1062) More...
DRTPrimaryAnatomicStructureSequence & | getPrimaryAnatomicStructureSequence ()
| get PrimaryAnatomicStructureSequence (0008,2228) More...
const DRTPrimaryAnatomicStructureSequence & | getPrimaryAnatomicStructureSequence () const
| get PrimaryAnatomicStructureSequence (0008,2228) More...
DRTPrivateDataElementCharacteristicsSequence & | getPrivateDataElementCharacteristicsSequence ()
| get PrivateDataElementCharacteristicsSequence (0008,0300) More...
const DRTPrivateDataElementCharacteristicsSequence & | getPrivateDataElementCharacteristicsSequence () const
| get PrivateDataElementCharacteristicsSequence (0008,0300) More...
DRTProcedureCodeSequence & | getProcedureCodeSequence ()
| get ProcedureCodeSequence (0008,1032) More...
const DRTProcedureCodeSequence & | getProcedureCodeSequence () const
| get ProcedureCodeSequence (0008,1032) More...
DRTRealWorldValueMappingSequence & | getRealWorldValueMappingSequence ()
| get RealWorldValueMappingSequence (0040,9096) More...
const DRTRealWorldValueMappingSequence & | getRealWorldValueMappingSequence () const
| get RealWorldValueMappingSequence (0040,9096) More...
DRTReasonForPerformedProcedureCodeSequence & | getReasonForPerformedProcedureCodeSequence ()
| get ReasonForPerformedProcedureCodeSequence (0040,1012) More...
const DRTReasonForPerformedProcedureCodeSequence & | getReasonForPerformedProcedureCodeSequence () const
| get ReasonForPerformedProcedureCodeSequence (0040,1012) More...
DRTReasonForVisitCodeSequence & | getReasonForVisitCodeSequence ()
| get ReasonForVisitCodeSequence (0032,1067) More...
const DRTReasonForVisitCodeSequence & | getReasonForVisitCodeSequence () const
| get ReasonForVisitCodeSequence (0032,1067) More...
DRTReferencedDefinedProtocolSequence & | getReferencedDefinedProtocolSequence ()
| get ReferencedDefinedProtocolSequence (0018,990c) More...
const DRTReferencedDefinedProtocolSequence & | getReferencedDefinedProtocolSequence () const
| get ReferencedDefinedProtocolSequence (0018,990c) More...
DRTReferencedImageSequence & | getReferencedImageSequence ()
| get ReferencedImageSequence (0008,1140) More...
const DRTReferencedImageSequence & | getReferencedImageSequence () const
| get ReferencedImageSequence (0008,1140) More...
DRTReferencedInstanceSequence & | getReferencedInstanceSequence ()
| get ReferencedInstanceSequence (0008,114a) More...
const DRTReferencedInstanceSequence & | getReferencedInstanceSequence () const
| get ReferencedInstanceSequence (0008,114a) More...
DRTReferencedPatientPhotoSequence & | getReferencedPatientPhotoSequence ()
| get ReferencedPatientPhotoSequence (0010,1100) More...
const DRTReferencedPatientPhotoSequence & | getReferencedPatientPhotoSequence () const
| get ReferencedPatientPhotoSequence (0010,1100) More...
DRTReferencedPatientSequence & | getReferencedPatientSequence ()
| get ReferencedPatientSequence (0008,1120) More...
const DRTReferencedPatientSequence & | getReferencedPatientSequence () const
| get ReferencedPatientSequence (0008,1120) More...
DRTReferencedPerformedProcedureStepSequence & | getReferencedPerformedProcedureStepSequence ()
| get ReferencedPerformedProcedureStepSequence (0008,1111) More...
const DRTReferencedPerformedProcedureStepSequence & | getReferencedPerformedProcedureStepSequence () const
| get ReferencedPerformedProcedureStepSequence (0008,1111) More...
DRTReferencedPerformedProtocolSequence & | getReferencedPerformedProtocolSequence ()
| get ReferencedPerformedProtocolSequence (0018,990d) More...
const DRTReferencedPerformedProtocolSequence & | getReferencedPerformedProtocolSequence () const
| get ReferencedPerformedProtocolSequence (0018,990d) More...
DRTReferencedRTPlanSequenceInRTImageModule & | getReferencedRTPlanSequence ()
| get ReferencedRTPlanSequence (300c,0002) More...
const DRTReferencedRTPlanSequenceInRTImageModule & | getReferencedRTPlanSequence () const
| get ReferencedRTPlanSequence (300c,0002) More...
DRTReferencedSeriesSequence & | getReferencedSeriesSequence ()
| get ReferencedSeriesSequence (0008,1115) More...
const DRTReferencedSeriesSequence & | getReferencedSeriesSequence () const
| get ReferencedSeriesSequence (0008,1115) More...
DRTReferencedStudySequence & | getReferencedStudySequence ()
| get ReferencedStudySequence (0008,1110) More...
const DRTReferencedStudySequence & | getReferencedStudySequence () const
| get ReferencedStudySequence (0008,1110) More...
DRTReferringPhysicianIdentificationSequence & | getReferringPhysicianIdentificationSequence ()
| get ReferringPhysicianIdentificationSequence (0008,0096) More...
const DRTReferringPhysicianIdentificationSequence & | getReferringPhysicianIdentificationSequence () const
| get ReferringPhysicianIdentificationSequence (0008,0096) More...
DRTRequestAttributesSequence & | getRequestAttributesSequence ()
| get RequestAttributesSequence (0040,0275) More...
const DRTRequestAttributesSequence & | getRequestAttributesSequence () const
| get RequestAttributesSequence (0040,0275) More...
DRTRequestingServiceCodeSequence & | getRequestingServiceCodeSequence ()
| get RequestingServiceCodeSequence (0032,1034) More...
const DRTRequestingServiceCodeSequence & | getRequestingServiceCodeSequence () const
| get RequestingServiceCodeSequence (0032,1034) More...
DRTSeriesDescriptionCodeSequence & | getSeriesDescriptionCodeSequence ()
| get SeriesDescriptionCodeSequence (0008,103f) More...
const DRTSeriesDescriptionCodeSequence & | getSeriesDescriptionCodeSequence () const
| get SeriesDescriptionCodeSequence (0008,103f) More...
DRTSourceImageSequence & | getSourceImageSequence ()
| get SourceImageSequence (0008,2112) More...
const DRTSourceImageSequence & | getSourceImageSequence () const
| get SourceImageSequence (0008,2112) More...
DRTSourceInstanceSequence & | getSourceInstanceSequence ()
| get SourceInstanceSequence (0042,0013) More...
const DRTSourceInstanceSequence & | getSourceInstanceSequence () const
| get SourceInstanceSequence (0042,0013) More...
DRTSourcePatientGroupIdentificationSequence & | getSourcePatientGroupIdentificationSequence ()
| get SourcePatientGroupIdentificationSequence (0010,0026) More...
const DRTSourcePatientGroupIdentificationSequence & | getSourcePatientGroupIdentificationSequence () const
| get SourcePatientGroupIdentificationSequence (0010,0026) More...
DRTStrainCodeSequence & | getStrainCodeSequence ()
| get StrainCodeSequence (0010,0219) More...
const DRTStrainCodeSequence & | getStrainCodeSequence () const
| get StrainCodeSequence (0010,0219) More...
DRTStrainStockSequence & | getStrainStockSequence ()
| get StrainStockSequence (0010,0216) More...
const DRTStrainStockSequence & | getStrainStockSequence () const
| get StrainStockSequence (0010,0216) More...
DRTStudiesContainingOtherReferencedInstancesSequence & | getStudiesContainingOtherReferencedInstancesSequence ()
| get StudiesContainingOtherReferencedInstancesSequence (0008,1200) More...
const DRTStudiesContainingOtherReferencedInstancesSequence & | getStudiesContainingOtherReferencedInstancesSequence () const
| get StudiesContainingOtherReferencedInstancesSequence (0008,1200) More...
DRTUDISequence & | getUDISequence ()
| get UDISequence (0018,100a) More...
const DRTUDISequence & | getUDISequence () const
| get UDISequence (0018,100a) More...
DRTVOILUTSequence & | getVOILUTSequence ()
| get VOILUTSequence (0028,3010) More...
const DRTVOILUTSequence & | getVOILUTSequence () const
| get VOILUTSequence (0028,3010) More...
virtual OFCondition | setAccessionNumber (const OFString &value, const OFBool check=OFTrue)
| set AccessionNumber (0008,0050) More...
virtual OFCondition | setAcquisitionDate (const OFString &value, const OFBool check=OFTrue)
| set AcquisitionDate (0008,0022) More...
virtual OFCondition | setAcquisitionDateTime (const OFString &value, const OFBool check=OFTrue)
| set AcquisitionDateTime (0008,002a) More...
virtual OFCondition | setAcquisitionDuration (const Float64 value, const unsigned long pos=0)
| set AcquisitionDuration (0018,9073) More...
virtual OFCondition | setAcquisitionNumber (const OFString &value, const OFBool check=OFTrue)
| set AcquisitionNumber (0020,0012) More...
virtual OFCondition | setAcquisitionTime (const OFString &value, const OFBool check=OFTrue)
| set AcquisitionTime (0008,0032) More...
virtual OFCondition | setAcquisitionUID (const OFString &value, const OFBool check=OFTrue)
| set AcquisitionUID (0008,0017) More...
virtual OFCondition | setActualFrameDuration (const OFString &value, const OFBool check=OFTrue)
| set ActualFrameDuration (0018,1242) More...
virtual OFCondition | setAdditionalPatientHistory (const OFString &value, const OFBool check=OFTrue)
| set AdditionalPatientHistory (0010,21b0) More...
virtual OFCondition | setAdmissionID (const OFString &value, const OFBool check=OFTrue)
| set AdmissionID (0038,0010) More...
virtual OFCondition | setAdmittingDiagnosesDescription (const OFString &value, const OFBool check=OFTrue)
| set AdmittingDiagnosesDescription (0008,1080) More...
virtual OFCondition | setAllergies (const OFString &value, const OFBool check=OFTrue)
| set Allergies (0010,2110) More...
virtual OFCondition | setApprovalStatus (const OFString &value, const OFBool check=OFTrue)
| set ApprovalStatus (300e,0002) More...
virtual OFCondition | setAuthorizationEquipmentCertificationNumber (const OFString &value, const OFBool check=OFTrue)
| set AuthorizationEquipmentCertificationNumber (0100,0426) More...
virtual OFCondition | setBarcodeValue (const OFString &value, const OFBool check=OFTrue)
| set BarcodeValue (2200,0005) More...
virtual OFCondition | setBeamLimitingDeviceAngle (const OFString &value, const OFBool check=OFTrue)
| set BeamLimitingDeviceAngle (300a,0120) More...
virtual OFCondition | setBitsAllocated (const Uint16 value, const unsigned long pos=0)
| set BitsAllocated (0028,0100) More...
virtual OFCondition | setBitsStored (const Uint16 value, const unsigned long pos=0)
| set BitsStored (0028,0101) More...
virtual OFCondition | setBluePaletteColorLookupTableData (const Uint16 *value, const unsigned long count)
| set BluePaletteColorLookupTableData (0028,1203) More...
virtual OFCondition | setBluePaletteColorLookupTableDescriptor (const Uint16 value, const unsigned long pos=0)
| set BluePaletteColorLookupTableDescriptor (0028,1103) More...
virtual OFCondition | setBurnedInAnnotation (const OFString &value, const OFBool check=OFTrue)
| set BurnedInAnnotation (0028,0301) More...
virtual OFCondition | setCineRate (const OFString &value, const OFBool check=OFTrue)
| set CineRate (0018,0040) More...
virtual OFCondition | setClinicalTrialCoordinatingCenterName (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialCoordinatingCenterName (0012,0060) More...
virtual OFCondition | setClinicalTrialProtocolEthicsCommitteeApprovalNumber (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialProtocolEthicsCommitteeApprovalNumber (0012,0082) More...
virtual OFCondition | setClinicalTrialProtocolEthicsCommitteeName (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialProtocolEthicsCommitteeName (0012,0081) More...
virtual OFCondition | setClinicalTrialProtocolID (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialProtocolID (0012,0020) More...
virtual OFCondition | setClinicalTrialProtocolName (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialProtocolName (0012,0021) More...
virtual OFCondition | setClinicalTrialSeriesDescription (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialSeriesDescription (0012,0072) More...
virtual OFCondition | setClinicalTrialSeriesID (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialSeriesID (0012,0071) More...
virtual OFCondition | setClinicalTrialSiteID (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialSiteID (0012,0030) More...
virtual OFCondition | setClinicalTrialSiteName (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialSiteName (0012,0031) More...
virtual OFCondition | setClinicalTrialSponsorName (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialSponsorName (0012,0010) More...
virtual OFCondition | setClinicalTrialSubjectID (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialSubjectID (0012,0040) More...
virtual OFCondition | setClinicalTrialSubjectReadingID (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialSubjectReadingID (0012,0042) More...
virtual OFCondition | setClinicalTrialTimePointDescription (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialTimePointDescription (0012,0051) More...
virtual OFCondition | setClinicalTrialTimePointID (const OFString &value, const OFBool check=OFTrue)
| set ClinicalTrialTimePointID (0012,0050) More...
virtual OFCondition | setColorSpace (const OFString &value, const OFBool check=OFTrue)
| set ColorSpace (0028,2002) More...
virtual OFCondition | setColumns (const Uint16 value, const unsigned long pos=0)
| set Columns (0028,0011) More...
virtual OFCondition | setCommentsOnThePerformedProcedureStep (const OFString &value, const OFBool check=OFTrue)
| set CommentsOnThePerformedProcedureStep (0040,0280) More...
virtual OFCondition | setConsultingPhysicianName (const OFString &value, const OFBool check=OFTrue)
| set ConsultingPhysicianName (0008,009c) More...
virtual OFCondition | setContentDate (const OFString &value, const OFBool check=OFTrue)
| set ContentDate (0008,0023) More...
virtual OFCondition | setContentQualification (const OFString &value, const OFBool check=OFTrue)
| set ContentQualification (0018,9004) More...
virtual OFCondition | setContentTime (const OFString &value, const OFBool check=OFTrue)
| set ContentTime (0008,0033) More...
virtual OFCondition | setContrastBolusAgent (const OFString &value, const OFBool check=OFTrue)
| set ContrastBolusAgent (0018,0010) More...
virtual OFCondition | setContrastBolusIngredient (const OFString &value, const OFBool check=OFTrue)
| set ContrastBolusIngredient (0018,1048) More...
virtual OFCondition | setContrastBolusIngredientConcentration (const OFString &value, const OFBool check=OFTrue)
| set ContrastBolusIngredientConcentration (0018,1049) More...
virtual OFCondition | setContrastBolusRoute (const OFString &value, const OFBool check=OFTrue)
| set ContrastBolusRoute (0018,1040) More...
virtual OFCondition | setContrastBolusStartTime (const OFString &value, const OFBool check=OFTrue)
| set ContrastBolusStartTime (0018,1042) More...
virtual OFCondition | setContrastBolusStopTime (const OFString &value, const OFBool check=OFTrue)
| set ContrastBolusStopTime (0018,1043) More...
virtual OFCondition | setContrastBolusTotalDose (const OFString &value, const OFBool check=OFTrue)
| set ContrastBolusTotalDose (0018,1044) More...
virtual OFCondition | setContrastBolusVolume (const OFString &value, const OFBool check=OFTrue)
| set ContrastBolusVolume (0018,1041) More...
virtual OFCondition | setContrastFlowDuration (const OFString &value, const OFBool check=OFTrue)
| set ContrastFlowDuration (0018,1047) More...
virtual OFCondition | setContrastFlowRate (const OFString &value, const OFBool check=OFTrue)
| set ContrastFlowRate (0018,1046) More...
virtual OFCondition | setConversionType (const OFString &value, const OFBool check=OFTrue)
| set ConversionType (0008,0064) More...
virtual OFCondition | setDateOfLastCalibration (const OFString &value, const OFBool check=OFTrue)
| set DateOfLastCalibration (0018,1200) More...
virtual OFCondition | setDeidentificationMethod (const OFString &value, const OFBool check=OFTrue)
| set DeidentificationMethod (0012,0063) More...
virtual OFCondition | setDerivationDescription (const OFString &value, const OFBool check=OFTrue)
| set DerivationDescription (0008,2111) More...
virtual OFCondition | setDeviceSerialNumber (const OFString &value, const OFBool check=OFTrue)
| set DeviceSerialNumber (0018,1000) More...
virtual OFCondition | setDeviceUID (const OFString &value, const OFBool check=OFTrue)
| set DeviceUID (0018,1002) More...
virtual OFCondition | setEffectiveDuration (const OFString &value, const OFBool check=OFTrue)
| set EffectiveDuration (0018,0072) More...
virtual OFCondition | setEncapsulatedPixelDataValueTotalLength (const Uint64 value, const unsigned long pos=0)
| set EncapsulatedPixelDataValueTotalLength (7fe0,0003) More...
virtual OFCondition | setEndCumulativeMetersetWeight (const OFString &value, const OFBool check=OFTrue)
| set EndCumulativeMetersetWeight (300c,0009) More...
virtual OFCondition | setEnhancedRTBeamLimitingDeviceDefinitionFlag (const OFString &value, const OFBool check=OFTrue)
| set EnhancedRTBeamLimitingDeviceDefinitionFlag (3008,00a3) More...
virtual OFCondition | setEthnicGroup (const OFString &value, const OFBool check=OFTrue)
| set EthnicGroup (0010,2160) More...
virtual OFCondition | setExposureTime (const OFString &value, const OFBool check=OFTrue)
| set ExposureTime (0018,1150) More...
virtual OFCondition | setExposureTimeInms (const Float64 value, const unsigned long pos=0)
| set ExposureTimeInms (0018,9328) More...
virtual OFCondition | setExtendedOffsetTable (const Uint64 *value, const unsigned long count)
| set ExtendedOffsetTable (7fe0,0001) More...
virtual OFCondition | setExtendedOffsetTableLengths (const Uint64 *value, const unsigned long count)
| set ExtendedOffsetTableLengths (7fe0,0002) More...
virtual OFCondition | setFractionNumber (const OFString &value, const OFBool check=OFTrue)
| set FractionNumber (3002,0029) More...
virtual OFCondition | setFrameDelay (const OFString &value, const OFBool check=OFTrue)
| set FrameDelay (0018,1066) More...
virtual OFCondition | setFrameIncrementPointer (const OFString &value, const OFBool check=OFTrue)
| set FrameIncrementPointer (0028,0009) More...
virtual OFCondition | setFrameOfReferenceUID (const OFString &value, const OFBool check=OFTrue)
| set FrameOfReferenceUID (0020,0052) More...
virtual OFCondition | setFrameTime (const OFString &value, const OFBool check=OFTrue)
| set FrameTime (0018,1063) More...
virtual OFCondition | setFrameTimeVector (const OFString &value, const OFBool check=OFTrue)
| set FrameTimeVector (0018,1065) More...
virtual OFCondition | setGantryAngle (const OFString &value, const OFBool check=OFTrue)
| set GantryAngle (300a,011e) More...
virtual OFCondition | setGantryID (const OFString &value, const OFBool check=OFTrue)
| set GantryID (0018,1008) More...
virtual OFCondition | setGantryPitchAngle (const Float32 value, const unsigned long pos=0)
| set GantryPitchAngle (300a,014a) More...
virtual OFCondition | setGreenPaletteColorLookupTableData (const Uint16 *value, const unsigned long count)
| set GreenPaletteColorLookupTableData (0028,1202) More...
virtual OFCondition | setGreenPaletteColorLookupTableDescriptor (const Uint16 value, const unsigned long pos=0)
| set GreenPaletteColorLookupTableDescriptor (0028,1102) More...
virtual OFCondition | setHighBit (const Uint16 value, const unsigned long pos=0)
| set HighBit (0028,0102) More...
virtual OFCondition | setICCProfile (const Uint8 *value, const unsigned long count)
| set ICCProfile (0028,2000) More...
virtual OFCondition | setImageComments (const OFString &value, const OFBool check=OFTrue)
| set ImageComments (0020,4000) More...
virtual OFCondition | setImageLaterality (const OFString &value, const OFBool check=OFTrue)
| set ImageLaterality (0020,0062) More...
virtual OFCondition | setImagePlanePixelSpacing (const OFString &value, const OFBool check=OFTrue)
| set ImagePlanePixelSpacing (3002,0011) More...
virtual OFCondition | setImageTriggerDelay (const OFString &value, const OFBool check=OFTrue)
| set ImageTriggerDelay (0018,1067) More...
virtual OFCondition | setImageType (const OFString &value, const OFBool check=OFTrue)
| set ImageType (0008,0008) More...
virtual OFCondition | setImagesInAcquisition (const OFString &value, const OFBool check=OFTrue)
| set ImagesInAcquisition (0020,1002) More...
virtual OFCondition | setInstanceCoercionDateTime (const OFString &value, const OFBool check=OFTrue)
| set InstanceCoercionDateTime (0008,0015) More...
virtual OFCondition | setInstanceCreationDate (const OFString &value, const OFBool check=OFTrue)
| set InstanceCreationDate (0008,0012) More...
virtual OFCondition | setInstanceCreationTime (const OFString &value, const OFBool check=OFTrue)
| set InstanceCreationTime (0008,0013) More...
virtual OFCondition | setInstanceCreatorUID (const OFString &value, const OFBool check=OFTrue)
| set InstanceCreatorUID (0008,0014) More...
virtual OFCondition | setInstanceNumber (const OFString &value, const OFBool check=OFTrue)
| set InstanceNumber (0020,0013) More...
virtual OFCondition | setInstanceOriginStatus (const OFString &value, const OFBool check=OFTrue)
| set InstanceOriginStatus (0400,0600) More...
virtual OFCondition | setInstitutionAddress (const OFString &value, const OFBool check=OFTrue)
| set InstitutionAddress (0008,0081) More...
virtual OFCondition | setInstitutionName (const OFString &value, const OFBool check=OFTrue)
| set InstitutionName (0008,0080) More...
virtual OFCondition | setInstitutionalDepartmentName (const OFString &value, const OFBool check=OFTrue)
| set InstitutionalDepartmentName (0008,1040) More...
virtual OFCondition | setIrradiationEventUID (const OFString &value, const OFBool check=OFTrue)
| set IrradiationEventUID (0008,3010) More...
virtual OFCondition | setIsocenterPosition (const OFString &value, const OFBool check=OFTrue)
| set IsocenterPosition (300a,012c) More...
virtual OFCondition | setIssuerOfPatientID (const OFString &value, const OFBool check=OFTrue)
| set IssuerOfPatientID (0010,0021) More...
virtual OFCondition | setLargestImagePixelValue (const Uint16 value, const unsigned long pos=0)
| set LargestImagePixelValue (0028,0107) More...
virtual OFCondition | setLastMenstrualDate (const OFString &value, const OFBool check=OFTrue)
| set LastMenstrualDate (0010,21d0) More...
virtual OFCondition | setLongitudinalTemporalEventType (const OFString &value, const OFBool check=OFTrue)
| set LongitudinalTemporalEventType (0012,0053) More...
virtual OFCondition | setLongitudinalTemporalInformationModified (const OFString &value, const OFBool check=OFTrue)
| set LongitudinalTemporalInformationModified (0028,0303) More...
virtual OFCondition | setLongitudinalTemporalOffsetFromEvent (const Float64 value, const unsigned long pos=0)
| set LongitudinalTemporalOffsetFromEvent (0012,0052) More...
virtual OFCondition | setLossyImageCompression (const OFString &value, const OFBool check=OFTrue)
| set LossyImageCompression (0028,2110) More...
virtual OFCondition | setLossyImageCompressionMethod (const OFString &value, const OFBool check=OFTrue)
| set LossyImageCompressionMethod (0028,2114) More...
virtual OFCondition | setLossyImageCompressionRatio (const OFString &value, const OFBool check=OFTrue)
| set LossyImageCompressionRatio (0028,2112) More...
virtual OFCondition | setManufacturer (const OFString &value, const OFBool check=OFTrue)
| set Manufacturer (0008,0070) More...
virtual OFCondition | setManufacturerDeviceClassUID (const OFString &value, const OFBool check=OFTrue)
| set ManufacturerDeviceClassUID (0018,100b) More...
virtual OFCondition | setManufacturerModelName (const OFString &value, const OFBool check=OFTrue)
| set ManufacturerModelName (0008,1090) More...
virtual OFCondition | setMeasuredAPDimension (const OFString &value, const OFBool check=OFTrue)
| set MeasuredAPDimension (0010,1023) More...
virtual OFCondition | setMeasuredLateralDimension (const OFString &value, const OFBool check=OFTrue)
| set MeasuredLateralDimension (0010,1024) More...
virtual OFCondition | setMedicalAlerts (const OFString &value, const OFBool check=OFTrue)
| set MedicalAlerts (0010,2000) More...
virtual OFCondition | setMetersetExposure (const OFString &value, const OFBool check=OFTrue)
| set MetersetExposure (3002,0032) More...
virtual OFCondition | setModality (const OFString &value, const OFBool check=OFTrue)
| set Modality (0008,0060) More...
virtual OFCondition | setNameOfPhysiciansReadingStudy (const OFString &value, const OFBool check=OFTrue)
| set NameOfPhysiciansReadingStudy (0008,1060) More...
virtual OFCondition | setNumberOfFrames (const OFString &value, const OFBool check=OFTrue)
| set NumberOfFrames (0028,0008) More...
virtual OFCondition | setOccupation (const OFString &value, const OFBool check=OFTrue)
| set Occupation (0010,2180) More...
virtual OFCondition | setOperatorsName (const OFString &value, const OFBool check=OFTrue)
| set OperatorsName (0008,1070) More...
virtual OFCondition | setOriginalSpecializedSOPClassUID (const OFString &value, const OFBool check=OFTrue)
| set OriginalSpecializedSOPClassUID (0008,001b) More...
virtual OFCondition | setOtherPatientNames (const OFString &value, const OFBool check=OFTrue)
| set OtherPatientNames (0010,1001) More...
virtual OFCondition | setPatientAge (const OFString &value, const OFBool check=OFTrue)
| set PatientAge (0010,1010) More...
virtual OFCondition | setPatientAlternativeCalendar (const OFString &value, const OFBool check=OFTrue)
| set PatientAlternativeCalendar (0010,0035) More...
virtual OFCondition | setPatientBirthDate (const OFString &value, const OFBool check=OFTrue)
| set PatientBirthDate (0010,0030) More...
virtual OFCondition | setPatientBirthDateInAlternativeCalendar (const OFString &value, const OFBool check=OFTrue)
| set PatientBirthDateInAlternativeCalendar (0010,0033) More...
virtual OFCondition | setPatientBirthTime (const OFString &value, const OFBool check=OFTrue)
| set PatientBirthTime (0010,0032) More...
virtual OFCondition | setPatientBodyMassIndex (const OFString &value, const OFBool check=OFTrue)
| set PatientBodyMassIndex (0010,1022) More...
virtual OFCondition | setPatientBreedDescription (const OFString &value, const OFBool check=OFTrue)
| set PatientBreedDescription (0010,2292) More...
virtual OFCondition | setPatientComments (const OFString &value, const OFBool check=OFTrue)
| set PatientComments (0010,4000) More...
virtual OFCondition | setPatientDeathDateInAlternativeCalendar (const OFString &value, const OFBool check=OFTrue)
| set PatientDeathDateInAlternativeCalendar (0010,0034) More...
virtual OFCondition | setPatientID (const OFString &value, const OFBool check=OFTrue)
| set PatientID (0010,0020) More...
virtual OFCondition | setPatientIdentityRemoved (const OFString &value, const OFBool check=OFTrue)
| set PatientIdentityRemoved (0012,0062) More...
virtual OFCondition | setPatientName (const OFString &value, const OFBool check=OFTrue)
| set PatientName (0010,0010) More...
virtual OFCondition | setPatientOrientation (const OFString &value, const OFBool check=OFTrue)
| set PatientOrientation (0020,0020) More...
virtual OFCondition | setPatientPosition (const OFString &value, const OFBool check=OFTrue)
| set PatientPosition (0018,5100) More...
virtual OFCondition | setPatientSex (const OFString &value, const OFBool check=OFTrue)
| set PatientSex (0010,0040) More...
virtual OFCondition | setPatientSexNeutered (const OFString &value, const OFBool check=OFTrue)
| set PatientSexNeutered (0010,2203) More...
virtual OFCondition | setPatientSize (const OFString &value, const OFBool check=OFTrue)
| set PatientSize (0010,1020) More...
virtual OFCondition | setPatientSpeciesDescription (const OFString &value, const OFBool check=OFTrue)
| set PatientSpeciesDescription (0010,2201) More...
virtual OFCondition | setPatientState (const OFString &value, const OFBool check=OFTrue)
| set PatientState (0038,0500) More...
virtual OFCondition | setPatientSupportAngle (const OFString &value, const OFBool check=OFTrue)
| set PatientSupportAngle (300a,0122) More...
virtual OFCondition | setPatientWeight (const OFString &value, const OFBool check=OFTrue)
| set PatientWeight (0010,1030) More...
virtual OFCondition | setPerformedProcedureStepDescription (const OFString &value, const OFBool check=OFTrue)
| set PerformedProcedureStepDescription (0040,0254) More...
virtual OFCondition | setPerformedProcedureStepEndDate (const OFString &value, const OFBool check=OFTrue)
| set PerformedProcedureStepEndDate (0040,0250) More...
virtual OFCondition | setPerformedProcedureStepEndTime (const OFString &value, const OFBool check=OFTrue)
| set PerformedProcedureStepEndTime (0040,0251) More...
virtual OFCondition | setPerformedProcedureStepID (const OFString &value, const OFBool check=OFTrue)
| set PerformedProcedureStepID (0040,0253) More...
virtual OFCondition | setPerformedProcedureStepStartDate (const OFString &value, const OFBool check=OFTrue)
| set PerformedProcedureStepStartDate (0040,0244) More...
virtual OFCondition | setPerformedProcedureStepStartTime (const OFString &value, const OFBool check=OFTrue)
| set PerformedProcedureStepStartTime (0040,0245) More...
virtual OFCondition | setPhotometricInterpretation (const OFString &value, const OFBool check=OFTrue)
| set PhotometricInterpretation (0028,0004) More...
virtual OFCondition | setPhysiciansOfRecord (const OFString &value, const OFBool check=OFTrue)
| set PhysiciansOfRecord (0008,1048) More...
virtual OFCondition | setPixelAspectRatio (const OFString &value, const OFBool check=OFTrue)
| set PixelAspectRatio (0028,0034) More...
virtual OFCondition | setPixelDataProviderURL (const OFString &value, const OFBool check=OFTrue)
| set PixelDataProviderURL (0028,7fe0) More...
virtual OFCondition | setPixelIntensityRelationship (const OFString &value, const OFBool check=OFTrue)
| set PixelIntensityRelationship (0028,1040) More...
virtual OFCondition | setPixelIntensityRelationshipSign (const Sint16 value, const unsigned long pos=0)
| set PixelIntensityRelationshipSign (0028,1041) More...
virtual OFCondition | setPixelPaddingRangeLimit (const Uint16 value, const unsigned long pos=0)
| set PixelPaddingRangeLimit (0028,0121) More...
virtual OFCondition | setPixelPaddingValue (const Uint16 value, const unsigned long pos=0)
| set PixelPaddingValue (0028,0120) More...
virtual OFCondition | setPixelRepresentation (const Uint16 value, const unsigned long pos=0)
| set PixelRepresentation (0028,0103) More...
virtual OFCondition | setPlanarConfiguration (const Uint16 value, const unsigned long pos=0)
| set PlanarConfiguration (0028,0006) More...
virtual OFCondition | setPositionReferenceIndicator (const OFString &value, const OFBool check=OFTrue)
| set PositionReferenceIndicator (0020,1040) More...
virtual OFCondition | setPreferredPlaybackSequencing (const Uint16 value, const unsigned long pos=0)
| set PreferredPlaybackSequencing (0018,1244) More...
virtual OFCondition | setPregnancyStatus (const Uint16 value, const unsigned long pos=0)
| set PregnancyStatus (0010,21c0) More...
virtual OFCondition | setPresentationLUTShape (const OFString &value, const OFBool check=OFTrue)
| set PresentationLUTShape (2050,0020) More...
virtual OFCondition | setPrimaryDosimeterUnit (const OFString &value, const OFBool check=OFTrue)
| set PrimaryDosimeterUnit (300a,00b3) More...
virtual OFCondition | setQualityControlImage (const OFString &value, const OFBool check=OFTrue)
| set QualityControlImage (0028,0300) More...
virtual OFCondition | setQualityControlSubject (const OFString &value, const OFBool check=OFTrue)
| set QualityControlSubject (0010,0200) More...
virtual OFCondition | setQueryRetrieveView (const OFString &value, const OFBool check=OFTrue)
| set QueryRetrieveView (0008,0053) More...
virtual OFCondition | setRTImageDescription (const OFString &value, const OFBool check=OFTrue)
| set RTImageDescription (3002,0004) More...
virtual OFCondition | setRTImageLabel (const OFString &value, const OFBool check=OFTrue)
| set RTImageLabel (3002,0002) More...
virtual OFCondition | setRTImageName (const OFString &value, const OFBool check=OFTrue)
| set RTImageName (3002,0003) More...
virtual OFCondition | setRTImageOrientation (const OFString &value, const OFBool check=OFTrue)
| set RTImageOrientation (3002,0010) More...
virtual OFCondition | setRTImagePlane (const OFString &value, const OFBool check=OFTrue)
| set RTImagePlane (3002,000c) More...
virtual OFCondition | setRTImagePosition (const OFString &value, const OFBool check=OFTrue)
| set RTImagePosition (3002,0012) More...
virtual OFCondition | setRTImageSID (const OFString &value, const OFBool check=OFTrue)
| set RTImageSID (3002,0026) More...
virtual OFCondition | setRadiationMachineName (const OFString &value, const OFBool check=OFTrue)
| set RadiationMachineName (3002,0020) More...
virtual OFCondition | setRadiationMachineSAD (const OFString &value, const OFBool check=OFTrue)
| set RadiationMachineSAD (3002,0022) More...
virtual OFCondition | setRadiationMachineSSD (const OFString &value, const OFBool check=OFTrue)
| set RadiationMachineSSD (3002,0024) More...
virtual OFCondition | setReasonForVisit (const OFString &value, const OFBool check=OFTrue)
| set ReasonForVisit (0032,1066) More...
virtual OFCondition | setRecognizableVisualFeatures (const OFString &value, const OFBool check=OFTrue)
| set RecognizableVisualFeatures (0028,0302) More...
virtual OFCondition | setRecommendedDisplayFrameRate (const OFString &value, const OFBool check=OFTrue)
| set RecommendedDisplayFrameRate (0008,2144) More...
virtual OFCondition | setRedPaletteColorLookupTableData (const Uint16 *value, const unsigned long count)
| set RedPaletteColorLookupTableData (0028,1201) More...
virtual OFCondition | setRedPaletteColorLookupTableDescriptor (const Uint16 value, const unsigned long pos=0)
| set RedPaletteColorLookupTableDescriptor (0028,1101) More...
virtual OFCondition | setReferencedBeamNumber (const OFString &value, const OFBool check=OFTrue)
| set ReferencedBeamNumber (300c,0006) More...
virtual OFCondition | setReferencedFractionGroupNumber (const OFString &value, const OFBool check=OFTrue)
| set ReferencedFractionGroupNumber (300c,0022) More...
virtual OFCondition | setReferringPhysicianName (const OFString &value, const OFBool check=OFTrue)
| set ReferringPhysicianName (0008,0090) More...
virtual OFCondition | setRelatedGeneralSOPClassUID (const OFString &value, const OFBool check=OFTrue)
| set RelatedGeneralSOPClassUID (0008,001a) More...
virtual OFCondition | setReportedValuesOrigin (const OFString &value, const OFBool check=OFTrue)
| set ReportedValuesOrigin (3002,000a) More...
virtual OFCondition | setRequestingService (const OFString &value, const OFBool check=OFTrue)
| set RequestingService (0032,1033) More...
virtual OFCondition | setRescaleIntercept (const OFString &value, const OFBool check=OFTrue)
| set RescaleIntercept (0028,1052) More...
virtual OFCondition | setRescaleSlope (const OFString &value, const OFBool check=OFTrue)
| set RescaleSlope (0028,1053) More...
virtual OFCondition | setRescaleType (const OFString &value, const OFBool check=OFTrue)
| set RescaleType (0028,1054) More...
virtual OFCondition | setResponsibleOrganization (const OFString &value, const OFBool check=OFTrue)
| set ResponsibleOrganization (0010,2299) More...
virtual OFCondition | setResponsiblePerson (const OFString &value, const OFBool check=OFTrue)
| set ResponsiblePerson (0010,2297) More...
virtual OFCondition | setResponsiblePersonRole (const OFString &value, const OFBool check=OFTrue)
| set ResponsiblePersonRole (0010,2298) More...
virtual OFCondition | setReviewDate (const OFString &value, const OFBool check=OFTrue)
| set ReviewDate (300e,0004) More...
virtual OFCondition | setReviewTime (const OFString &value, const OFBool check=OFTrue)
| set ReviewTime (300e,0005) More...
virtual OFCondition | setReviewerName (const OFString &value, const OFBool check=OFTrue)
| set ReviewerName (300e,0008) More...
virtual OFCondition | setRows (const Uint16 value, const unsigned long pos=0)
| set Rows (0028,0010) More...
virtual OFCondition | setSOPAuthorizationComment (const OFString &value, const OFBool check=OFTrue)
| set SOPAuthorizationComment (0100,0424) More...
virtual OFCondition | setSOPAuthorizationDateTime (const OFString &value, const OFBool check=OFTrue)
| set SOPAuthorizationDateTime (0100,0420) More...
virtual OFCondition | setSOPClassUID (const OFString &value, const OFBool check=OFTrue)
| set SOPClassUID (0008,0016) More...
virtual OFCondition | setSOPInstanceStatus (const OFString &value, const OFBool check=OFTrue)
| set SOPInstanceStatus (0100,0410) More...
virtual OFCondition | setSOPInstanceUID (const OFString &value, const OFBool check=OFTrue)
| set SOPInstanceUID (0008,0018) More...
virtual OFCondition | setSamplesPerPixel (const Uint16 value, const unsigned long pos=0)
| set SamplesPerPixel (0028,0002) More...
virtual OFCondition | setSeriesDate (const OFString &value, const OFBool check=OFTrue)
| set SeriesDate (0008,0021) More...
virtual OFCondition | setSeriesDescription (const OFString &value, const OFBool check=OFTrue)
| set SeriesDescription (0008,103e) More...
virtual OFCondition | setSeriesInstanceUID (const OFString &value, const OFBool check=OFTrue)
| set SeriesInstanceUID (0020,000e) More...
virtual OFCondition | setSeriesNumber (const OFString &value, const OFBool check=OFTrue)
| set SeriesNumber (0020,0011) More...
virtual OFCondition | setSeriesTime (const OFString &value, const OFBool check=OFTrue)
| set SeriesTime (0008,0031) More...
virtual OFCondition | setServiceEpisodeDescription (const OFString &value, const OFBool check=OFTrue)
| set ServiceEpisodeDescription (0038,0062) More...
virtual OFCondition | setServiceEpisodeID (const OFString &value, const OFBool check=OFTrue)
| set ServiceEpisodeID (0038,0060) More...
virtual OFCondition | setSmallestImagePixelValue (const Uint16 value, const unsigned long pos=0)
| set SmallestImagePixelValue (0028,0106) More...
virtual OFCondition | setSmokingStatus (const OFString &value, const OFBool check=OFTrue)
| set SmokingStatus (0010,21a0) More...
virtual OFCondition | setSoftwareVersions (const OFString &value, const OFBool check=OFTrue)
| set SoftwareVersions (0018,1020) More...
virtual OFCondition | setSourceToReferenceObjectDistance (const OFString &value, const OFBool check=OFTrue)
| set SourceToReferenceObjectDistance (3002,0028) More...
virtual OFCondition | setSpatialResolution (const OFString &value, const OFBool check=OFTrue)
| set SpatialResolution (0018,1050) More...
virtual OFCondition | setSpecificCharacterSet (const OFString &value, const OFBool check=OFTrue)
| set SpecificCharacterSet (0008,0005) More...
virtual OFCondition | setStartCumulativeMetersetWeight (const OFString &value, const OFBool check=OFTrue)
| set StartCumulativeMetersetWeight (300c,0008) More...
virtual OFCondition | setStartTrim (const OFString &value, const OFBool check=OFTrue)
| set StartTrim (0008,2142) More...
virtual OFCondition | setStationName (const OFString &value, const OFBool check=OFTrue)
| set StationName (0008,1010) More...
virtual OFCondition | setStereoPairsPresent (const OFString &value, const OFBool check=OFTrue)
| set StereoPairsPresent (0022,0028) More...
virtual OFCondition | setStopTrim (const OFString &value, const OFBool check=OFTrue)
| set StopTrim (0008,2143) More...
virtual OFCondition | setStrainAdditionalInformation (const OFString &value, const OFBool check=OFTrue)
| set StrainAdditionalInformation (0010,0218) More...
virtual OFCondition | setStrainDescription (const OFString &value, const OFBool check=OFTrue)
| set StrainDescription (0010,0212) More...
virtual OFCondition | setStrainNomenclature (const OFString &value, const OFBool check=OFTrue)
| set StrainNomenclature (0010,0213) More...
virtual OFCondition | setStudyDate (const OFString &value, const OFBool check=OFTrue)
| set StudyDate (0008,0020) More...
virtual OFCondition | setStudyDescription (const OFString &value, const OFBool check=OFTrue)
| set StudyDescription (0008,1030) More...
virtual OFCondition | setStudyID (const OFString &value, const OFBool check=OFTrue)
| set StudyID (0020,0010) More...
virtual OFCondition | setStudyInstanceUID (const OFString &value, const OFBool check=OFTrue)
| set StudyInstanceUID (0020,000d) More...
virtual OFCondition | setStudyTime (const OFString &value, const OFBool check=OFTrue)
| set StudyTime (0008,0030) More...
virtual OFCondition | setTableTopEccentricAngle (const OFString &value, const OFBool check=OFTrue)
| set TableTopEccentricAngle (300a,0125) More...
virtual OFCondition | setTableTopEccentricAxisDistance (const OFString &value, const OFBool check=OFTrue)
| set TableTopEccentricAxisDistance (300a,0124) More...
virtual OFCondition | setTableTopLateralPosition (const OFString &value, const OFBool check=OFTrue)
| set TableTopLateralPosition (300a,012a) More...
virtual OFCondition | setTableTopLongitudinalPosition (const OFString &value, const OFBool check=OFTrue)
| set TableTopLongitudinalPosition (300a,0129) More...
virtual OFCondition | setTableTopPitchAngle (const Float32 value, const unsigned long pos=0)
| set TableTopPitchAngle (300a,0140) More...
virtual OFCondition | setTableTopRollAngle (const Float32 value, const unsigned long pos=0)
| set TableTopRollAngle (300a,0144) More...
virtual OFCondition | setTableTopVerticalPosition (const OFString &value, const OFBool check=OFTrue)
| set TableTopVerticalPosition (300a,0128) More...
virtual OFCondition | setTimeOfLastCalibration (const OFString &value, const OFBool check=OFTrue)
| set TimeOfLastCalibration (0018,1201) More...
virtual OFCondition | setTimezoneOffsetFromUTC (const OFString &value, const OFBool check=OFTrue)
| set TimezoneOffsetFromUTC (0008,0201) More...
virtual OFCondition | setTreatmentSessionUID (const OFString &value, const OFBool check=OFTrue)
| set TreatmentSessionUID (300a,0700) More...
virtual OFCondition | setTypeOfPatientID (const OFString &value, const OFBool check=OFTrue)
| set TypeOfPatientID (0010,0022) More...
virtual OFCondition | setVOILUTFunction (const OFString &value, const OFBool check=OFTrue)
| set VOILUTFunction (0028,1056) More...
virtual OFCondition | setWindowCenter (const OFString &value, const OFBool check=OFTrue)
| set WindowCenter (0028,1050) More...
virtual OFCondition | setWindowCenterWidthExplanation (const OFString &value, const OFBool check=OFTrue)
| set WindowCenterWidthExplanation (0028,1055) More...
virtual OFCondition | setWindowWidth (const OFString &value, const OFBool check=OFTrue)
| set WindowWidth (0028,1051) More...
virtual OFCondition | setXRayImageReceptorAngle (const OFString &value, const OFBool check=OFTrue)
| set XRayImageReceptorAngle (3002,000e) More...
virtual OFCondition | setXRayImageReceptorTranslation (const OFString &value, const OFBool check=OFTrue)
| set XRayImageReceptorTranslation (3002,000d) More...

## Protected Member Functions
OFCondition | checkDatasetForReading (DcmItem &dataset)
| check the given dataset before reading. More...
void | updateAttributes ()
| update various DICOM attributes
Protected Member Functions inherited from DRTTypes
virtual | ~DRTTypes ()
| destructor. More...

## Private Attributes
DcmPersonName | PatientName
| PatientName (0010,0010) vr=PN, vm=1, type=2.
DcmLongString | PatientID
| PatientID (0010,0020) vr=LO, vm=1, type=2.
DcmLongString | IssuerOfPatientID
| IssuerOfPatientID (0010,0021) vr=LO, vm=1, type=3.
DRTIssuerOfPatientIDQualifiersSequence | IssuerOfPatientIDQualifiersSequence
| IssuerOfPatientIDQualifiersSequence (0010,0024) vr=SQ, vm=1, type=3.
DcmCodeString | TypeOfPatientID
| TypeOfPatientID (0010,0022) vr=CS, vm=1, type=3.
DcmDate | PatientBirthDate
| PatientBirthDate (0010,0030) vr=DA, vm=1, type=2.
DcmLongString | PatientBirthDateInAlternativeCalendar
| PatientBirthDateInAlternativeCalendar (0010,0033) vr=LO, vm=1, type=3.
DcmLongString | PatientDeathDateInAlternativeCalendar
| PatientDeathDateInAlternativeCalendar (0010,0034) vr=LO, vm=1, type=3.
DcmCodeString | PatientAlternativeCalendar
| PatientAlternativeCalendar (0010,0035) vr=CS, vm=1, type=1C.
DcmCodeString | PatientSex
| PatientSex (0010,0040) vr=CS, vm=1, type=2.
DRTReferencedPatientPhotoSequence | ReferencedPatientPhotoSequence
| ReferencedPatientPhotoSequence (0010,1100) vr=SQ, vm=1, type=3.
DcmCodeString | QualityControlSubject
| QualityControlSubject (0010,0200) vr=CS, vm=1, type=3.
DRTReferencedPatientSequence | ReferencedPatientSequence
| ReferencedPatientSequence (0008,1120) vr=SQ, vm=1, type=3.
DcmTime | PatientBirthTime
| PatientBirthTime (0010,0032) vr=TM, vm=1, type=3.
DRTOtherPatientIDsSequence | OtherPatientIDsSequence
| OtherPatientIDsSequence (0010,1002) vr=SQ, vm=1, type=3.
DcmPersonName | OtherPatientNames
| OtherPatientNames (0010,1001) vr=PN, vm=1-n, type=3.
DcmShortString | EthnicGroup
| EthnicGroup (0010,2160) vr=SH, vm=1, type=3.
DcmLongText | PatientComments
| PatientComments (0010,4000) vr=LT, vm=1, type=3.
DcmLongString | PatientSpeciesDescription
| PatientSpeciesDescription (0010,2201) vr=LO, vm=1, type=1C.
DRTPatientSpeciesCodeSequence | PatientSpeciesCodeSequence
| PatientSpeciesCodeSequence (0010,2202) vr=SQ, vm=1, type=1C.
DcmLongString | PatientBreedDescription
| PatientBreedDescription (0010,2292) vr=LO, vm=1, type=2C.
DRTPatientBreedCodeSequence | PatientBreedCodeSequence
| PatientBreedCodeSequence (0010,2293) vr=SQ, vm=1, type=2C.
DRTBreedRegistrationSequence | BreedRegistrationSequence
| BreedRegistrationSequence (0010,2294) vr=SQ, vm=1, type=2C.
DcmUnlimitedCharacters | StrainDescription
| StrainDescription (0010,0212) vr=UC, vm=1, type=3.
DcmLongString | StrainNomenclature
| StrainNomenclature (0010,0213) vr=LO, vm=1, type=3.
DRTStrainCodeSequence | StrainCodeSequence
| StrainCodeSequence (0010,0219) vr=SQ, vm=1, type=3.
DcmUnlimitedText | StrainAdditionalInformation
| StrainAdditionalInformation (0010,0218) vr=UT, vm=1, type=3.
DRTStrainStockSequence | StrainStockSequence
| StrainStockSequence (0010,0216) vr=SQ, vm=1, type=3.
DRTGeneticModificationsSequence | GeneticModificationsSequence
| GeneticModificationsSequence (0010,0221) vr=SQ, vm=1, type=3.
DcmPersonName | ResponsiblePerson
| ResponsiblePerson (0010,2297) vr=PN, vm=1, type=2C.
DcmCodeString | ResponsiblePersonRole
| ResponsiblePersonRole (0010,2298) vr=CS, vm=1, type=1C.
DcmLongString | ResponsibleOrganization
| ResponsibleOrganization (0010,2299) vr=LO, vm=1, type=2C.
DcmCodeString | PatientIdentityRemoved
| PatientIdentityRemoved (0012,0062) vr=CS, vm=1, type=3.
DcmLongString | DeidentificationMethod
| DeidentificationMethod (0012,0063) vr=LO, vm=1-n, type=1C.
DRTDeidentificationMethodCodeSequence | DeidentificationMethodCodeSequence
| DeidentificationMethodCodeSequence (0012,0064) vr=SQ, vm=1, type=1C.
DRTSourcePatientGroupIdentificationSequence | SourcePatientGroupIdentificationSequence
| SourcePatientGroupIdentificationSequence (0010,0026) vr=SQ, vm=1, type=3.
DRTGroupOfPatientsIdentificationSequence | GroupOfPatientsIdentificationSequence
| GroupOfPatientsIdentificationSequence (0010,0027) vr=SQ, vm=1, type=3.
DcmLongString | ClinicalTrialSponsorName
| ClinicalTrialSponsorName (0012,0010) vr=LO, vm=1, type=1.
DcmLongString | ClinicalTrialProtocolID
| ClinicalTrialProtocolID (0012,0020) vr=LO, vm=1, type=1.
DcmLongString | ClinicalTrialProtocolName
| ClinicalTrialProtocolName (0012,0021) vr=LO, vm=1, type=2.
DcmLongString | ClinicalTrialSiteID
| ClinicalTrialSiteID (0012,0030) vr=LO, vm=1, type=2.
DcmLongString | ClinicalTrialSiteName
| ClinicalTrialSiteName (0012,0031) vr=LO, vm=1, type=2.
DcmLongString | ClinicalTrialSubjectID
| ClinicalTrialSubjectID (0012,0040) vr=LO, vm=1, type=1C.
DcmLongString | ClinicalTrialSubjectReadingID
| ClinicalTrialSubjectReadingID (0012,0042) vr=LO, vm=1, type=1C.
DcmLongString | ClinicalTrialProtocolEthicsCommitteeName
| ClinicalTrialProtocolEthicsCommitteeName (0012,0081) vr=LO, vm=1, type=1C.
DcmLongString | ClinicalTrialProtocolEthicsCommitteeApprovalNumber
| ClinicalTrialProtocolEthicsCommitteeApprovalNumber (0012,0082) vr=LO, vm=1, type=3.
DcmUniqueIdentifier | StudyInstanceUID
| StudyInstanceUID (0020,000d) vr=UI, vm=1, type=1.
DcmDate | StudyDate
| StudyDate (0008,0020) vr=DA, vm=1, type=2.
DcmTime | StudyTime
| StudyTime (0008,0030) vr=TM, vm=1, type=2.
DcmPersonName | ReferringPhysicianName
| ReferringPhysicianName (0008,0090) vr=PN, vm=1, type=2.
DRTReferringPhysicianIdentificationSequence | ReferringPhysicianIdentificationSequence
| ReferringPhysicianIdentificationSequence (0008,0096) vr=SQ, vm=1, type=3.
DcmPersonName | ConsultingPhysicianName
| ConsultingPhysicianName (0008,009c) vr=PN, vm=1-n, type=3.
DRTConsultingPhysicianIdentificationSequence | ConsultingPhysicianIdentificationSequence
| ConsultingPhysicianIdentificationSequence (0008,009d) vr=SQ, vm=1, type=3.
DcmShortString | StudyID
| StudyID (0020,0010) vr=SH, vm=1, type=2.
DcmShortString | AccessionNumber
| AccessionNumber (0008,0050) vr=SH, vm=1, type=2.
DRTIssuerOfAccessionNumberSequence | IssuerOfAccessionNumberSequence
| IssuerOfAccessionNumberSequence (0008,0051) vr=SQ, vm=1, type=3.
DcmLongString | StudyDescription
| StudyDescription (0008,1030) vr=LO, vm=1, type=3.
DcmPersonName | PhysiciansOfRecord
| PhysiciansOfRecord (0008,1048) vr=PN, vm=1-n, type=3.
DRTPhysiciansOfRecordIdentificationSequence | PhysiciansOfRecordIdentificationSequence
| PhysiciansOfRecordIdentificationSequence (0008,1049) vr=SQ, vm=1, type=3.
DcmPersonName | NameOfPhysiciansReadingStudy
| NameOfPhysiciansReadingStudy (0008,1060) vr=PN, vm=1-n, type=3.
DRTPhysiciansReadingStudyIdentificationSequence | PhysiciansReadingStudyIdentificationSequence
| PhysiciansReadingStudyIdentificationSequence (0008,1062) vr=SQ, vm=1, type=3.
DcmLongString | RequestingService
| RequestingService (0032,1033) vr=LO, vm=1, type=3.
DRTRequestingServiceCodeSequence | RequestingServiceCodeSequence
| RequestingServiceCodeSequence (0032,1034) vr=SQ, vm=1, type=3.
DRTReferencedStudySequence | ReferencedStudySequence
| ReferencedStudySequence (0008,1110) vr=SQ, vm=1, type=3.
DRTProcedureCodeSequence | ProcedureCodeSequence
| ProcedureCodeSequence (0008,1032) vr=SQ, vm=1, type=3.
DRTReasonForPerformedProcedureCodeSequence | ReasonForPerformedProcedureCodeSequence
| ReasonForPerformedProcedureCodeSequence (0040,1012) vr=SQ, vm=1, type=3.
DcmLongString | AdmittingDiagnosesDescription
| AdmittingDiagnosesDescription (0008,1080) vr=LO, vm=1-n, type=3.
DRTAdmittingDiagnosesCodeSequence | AdmittingDiagnosesCodeSequence
| AdmittingDiagnosesCodeSequence (0008,1084) vr=SQ, vm=1, type=3.
DcmAgeString | PatientAge
| PatientAge (0010,1010) vr=AS, vm=1, type=3.
DcmDecimalString | PatientSize
| PatientSize (0010,1020) vr=DS, vm=1, type=3.
DcmDecimalString | PatientWeight
| PatientWeight (0010,1030) vr=DS, vm=1, type=3.
DcmDecimalString | PatientBodyMassIndex
| PatientBodyMassIndex (0010,1022) vr=DS, vm=1, type=3.
DcmDecimalString | MeasuredAPDimension
| MeasuredAPDimension (0010,1023) vr=DS, vm=1, type=3.
DcmDecimalString | MeasuredLateralDimension
| MeasuredLateralDimension (0010,1024) vr=DS, vm=1, type=3.
DRTPatientSizeCodeSequence | PatientSizeCodeSequence
| PatientSizeCodeSequence (0010,1021) vr=SQ, vm=1, type=3.
DcmLongString | MedicalAlerts
| MedicalAlerts (0010,2000) vr=LO, vm=1-n, type=3.
DcmLongString | Allergies
| Allergies (0010,2110) vr=LO, vm=1-n, type=3.
DcmCodeString | SmokingStatus
| SmokingStatus (0010,21a0) vr=CS, vm=1, type=3.
DcmUnsignedShort | PregnancyStatus
| PregnancyStatus (0010,21c0) vr=US, vm=1, type=3.
DcmDate | LastMenstrualDate
| LastMenstrualDate (0010,21d0) vr=DA, vm=1, type=3.
DcmLongString | PatientState
| PatientState (0038,0500) vr=LO, vm=1, type=3.
DcmShortString | Occupation
| Occupation (0010,2180) vr=SH, vm=1, type=3.
DcmLongText | AdditionalPatientHistory
| AdditionalPatientHistory (0010,21b0) vr=LT, vm=1, type=3.
DcmLongString | AdmissionID
| AdmissionID (0038,0010) vr=LO, vm=1, type=3.
DRTIssuerOfAdmissionIDSequence | IssuerOfAdmissionIDSequence
| IssuerOfAdmissionIDSequence (0038,0014) vr=SQ, vm=1, type=3.
DcmUnlimitedText | ReasonForVisit
| ReasonForVisit (0032,1066) vr=UT, vm=1, type=3.
DRTReasonForVisitCodeSequence | ReasonForVisitCodeSequence
| ReasonForVisitCodeSequence (0032,1067) vr=SQ, vm=1, type=3.
DcmLongString | ServiceEpisodeID
| ServiceEpisodeID (0038,0060) vr=LO, vm=1, type=3.
DRTIssuerOfServiceEpisodeIDSequence | IssuerOfServiceEpisodeIDSequence
| IssuerOfServiceEpisodeIDSequence (0038,0064) vr=SQ, vm=1, type=3.
DcmLongString | ServiceEpisodeDescription
| ServiceEpisodeDescription (0038,0062) vr=LO, vm=1, type=3.
DcmCodeString | PatientSexNeutered
| PatientSexNeutered (0010,2203) vr=CS, vm=1, type=2C.
DcmLongString | ClinicalTrialTimePointID
| ClinicalTrialTimePointID (0012,0050) vr=LO, vm=1, type=2.
DcmShortText | ClinicalTrialTimePointDescription
| ClinicalTrialTimePointDescription (0012,0051) vr=ST, vm=1, type=3.
DRTClinicalTrialTimePointTypeCodeSequence | ClinicalTrialTimePointTypeCodeSequence
| ClinicalTrialTimePointTypeCodeSequence (0012,0054) vr=SQ, vm=1, type=3.
DcmFloatingPointDouble | LongitudinalTemporalOffsetFromEvent
| LongitudinalTemporalOffsetFromEvent (0012,0052) vr=FD, vm=1, type=3.
DcmCodeString | LongitudinalTemporalEventType
| LongitudinalTemporalEventType (0012,0053) vr=CS, vm=1, type=1C.
DRTConsentForClinicalTrialUseSequence | ConsentForClinicalTrialUseSequence
| ConsentForClinicalTrialUseSequence (0012,0083) vr=SQ, vm=1, type=3.
DcmCodeString | Modality
| Modality (0008,0060) vr=CS, vm=1, type=1.
DcmUniqueIdentifier | SeriesInstanceUID
| SeriesInstanceUID (0020,000e) vr=UI, vm=1, type=1.
DcmIntegerString | SeriesNumber
| SeriesNumber (0020,0011) vr=IS, vm=1, type=2.
DcmDate | SeriesDate
| SeriesDate (0008,0021) vr=DA, vm=1, type=3.
DcmTime | SeriesTime
| SeriesTime (0008,0031) vr=TM, vm=1, type=3.
DcmLongString | SeriesDescription
| SeriesDescription (0008,103e) vr=LO, vm=1, type=3.
DRTSeriesDescriptionCodeSequence | SeriesDescriptionCodeSequence
| SeriesDescriptionCodeSequence (0008,103f) vr=SQ, vm=1, type=3.
DcmPersonName | OperatorsName
| OperatorsName (0008,1070) vr=PN, vm=1-n, type=2.
DRTOperatorIdentificationSequence | OperatorIdentificationSequence
| OperatorIdentificationSequence (0008,1072) vr=SQ, vm=1, type=3.
DRTReferencedPerformedProcedureStepSequence | ReferencedPerformedProcedureStepSequence
| ReferencedPerformedProcedureStepSequence (0008,1111) vr=SQ, vm=1, type=3.
DRTRequestAttributesSequence | RequestAttributesSequence
| RequestAttributesSequence (0040,0275) vr=SQ, vm=1, type=3.
DcmShortString | PerformedProcedureStepID
| PerformedProcedureStepID (0040,0253) vr=SH, vm=1, type=3.
DcmDate | PerformedProcedureStepStartDate
| PerformedProcedureStepStartDate (0040,0244) vr=DA, vm=1, type=3.
DcmTime | PerformedProcedureStepStartTime
| PerformedProcedureStepStartTime (0040,0245) vr=TM, vm=1, type=3.
DcmDate | PerformedProcedureStepEndDate
| PerformedProcedureStepEndDate (0040,0250) vr=DA, vm=1, type=3.
DcmTime | PerformedProcedureStepEndTime
| PerformedProcedureStepEndTime (0040,0251) vr=TM, vm=1, type=3.
DcmLongString | PerformedProcedureStepDescription
| PerformedProcedureStepDescription (0040,0254) vr=LO, vm=1, type=3.
DRTPerformedProtocolCodeSequence | PerformedProtocolCodeSequence
| PerformedProtocolCodeSequence (0040,0260) vr=SQ, vm=1, type=3.
DcmShortText | CommentsOnThePerformedProcedureStep
| CommentsOnThePerformedProcedureStep (0040,0280) vr=ST, vm=1, type=3.
DcmUniqueIdentifier | TreatmentSessionUID
| TreatmentSessionUID (300a,0700) vr=UI, vm=1, type=3.
DcmLongString | ClinicalTrialCoordinatingCenterName
| ClinicalTrialCoordinatingCenterName (0012,0060) vr=LO, vm=1, type=2.
DcmLongString | ClinicalTrialSeriesID
| ClinicalTrialSeriesID (0012,0071) vr=LO, vm=1, type=3.
DcmLongString | ClinicalTrialSeriesDescription
| ClinicalTrialSeriesDescription (0012,0072) vr=LO, vm=1, type=3.
DcmUniqueIdentifier | FrameOfReferenceUID
| FrameOfReferenceUID (0020,0052) vr=UI, vm=1, type=1.
DcmLongString | PositionReferenceIndicator
| PositionReferenceIndicator (0020,1040) vr=LO, vm=1, type=2.
DcmLongString | Manufacturer
| Manufacturer (0008,0070) vr=LO, vm=1, type=2.
DcmLongString | InstitutionName
| InstitutionName (0008,0080) vr=LO, vm=1, type=3.
DcmShortText | InstitutionAddress
| InstitutionAddress (0008,0081) vr=ST, vm=1, type=3.
DcmShortString | StationName
| StationName (0008,1010) vr=SH, vm=1, type=3.
DcmLongString | InstitutionalDepartmentName
| InstitutionalDepartmentName (0008,1040) vr=LO, vm=1, type=3.
DRTInstitutionalDepartmentTypeCodeSequence | InstitutionalDepartmentTypeCodeSequence
| InstitutionalDepartmentTypeCodeSequence (0008,1041) vr=SQ, vm=1, type=3.
DcmLongString | ManufacturerModelName
| ManufacturerModelName (0008,1090) vr=LO, vm=1, type=3.
DcmUniqueIdentifier | ManufacturerDeviceClassUID
| ManufacturerDeviceClassUID (0018,100b) vr=UI, vm=1-n, type=3.
DcmLongString | DeviceSerialNumber
| DeviceSerialNumber (0018,1000) vr=LO, vm=1, type=3.
DcmLongString | SoftwareVersions
| SoftwareVersions (0018,1020) vr=LO, vm=1-n, type=3.
DcmLongString | GantryID
| GantryID (0018,1008) vr=LO, vm=1, type=3.
DRTUDISequence | UDISequence
| UDISequence (0018,100a) vr=SQ, vm=1, type=3.
DcmUniqueIdentifier | DeviceUID
| DeviceUID (0018,1002) vr=UI, vm=1, type=3.
DcmDecimalString | SpatialResolution
| SpatialResolution (0018,1050) vr=DS, vm=1, type=3.
DcmDate | DateOfLastCalibration
| DateOfLastCalibration (0018,1200) vr=DA, vm=1-n, type=3.
DcmTime | TimeOfLastCalibration
| TimeOfLastCalibration (0018,1201) vr=TM, vm=1-n, type=3.
DcmUnsignedShort | PixelPaddingValue
| PixelPaddingValue (0028,0120) vr=US/SS, vm=1, type=1C.
DcmUniqueIdentifier | AcquisitionUID
| AcquisitionUID (0008,0017) vr=UI, vm=1, type=3.
DcmIntegerString | AcquisitionNumber
| AcquisitionNumber (0020,0012) vr=IS, vm=1, type=3.
DcmDate | AcquisitionDate
| AcquisitionDate (0008,0022) vr=DA, vm=1, type=3.
DcmTime | AcquisitionTime
| AcquisitionTime (0008,0032) vr=TM, vm=1, type=3.
DcmDateTime | AcquisitionDateTime
| AcquisitionDateTime (0008,002a) vr=DT, vm=1, type=3.
DcmFloatingPointDouble | AcquisitionDuration
| AcquisitionDuration (0018,9073) vr=FD, vm=1, type=3.
DcmIntegerString | ImagesInAcquisition
| ImagesInAcquisition (0020,1002) vr=IS, vm=1, type=3.
DcmUniqueIdentifier | IrradiationEventUID
| IrradiationEventUID (0008,3010) vr=UI, vm=1-n, type=3.
DcmIntegerString | InstanceNumber
| InstanceNumber (0020,0013) vr=IS, vm=1, type=2. More...
DcmCodeString | PatientOrientation
| PatientOrientation (0020,0020) vr=CS, vm=2, type=2C.
DcmDate | ContentDate
| ContentDate (0008,0023) vr=DA, vm=1, type=2C.
DcmTime | ContentTime
| ContentTime (0008,0033) vr=TM, vm=1, type=2C.
DcmLongText | ImageComments
| ImageComments (0020,4000) vr=LT, vm=1, type=3.
DcmCodeString | QualityControlImage
| QualityControlImage (0028,0300) vr=CS, vm=1, type=3.
DcmCodeString | BurnedInAnnotation
| BurnedInAnnotation (0028,0301) vr=CS, vm=1, type=3.
DcmCodeString | RecognizableVisualFeatures
| RecognizableVisualFeatures (0028,0302) vr=CS, vm=1, type=3.
DcmCodeString | LossyImageCompression
| LossyImageCompression (0028,2110) vr=CS, vm=1, type=3.
DcmDecimalString | LossyImageCompressionRatio
| LossyImageCompressionRatio (0028,2112) vr=DS, vm=1-n, type=3.
DcmCodeString | LossyImageCompressionMethod
| LossyImageCompressionMethod (0028,2114) vr=CS, vm=1-n, type=3.
DRTIconImageSequence | IconImageSequence
| IconImageSequence (0088,0200) vr=SQ, vm=1, type=3.
DcmCodeString | PresentationLUTShape
| PresentationLUTShape (2050,0020) vr=CS, vm=1, type=3.
DRTRealWorldValueMappingSequence | RealWorldValueMappingSequence
| RealWorldValueMappingSequence (0040,9096) vr=SQ, vm=1, type=3.
DcmCodeString | ImageLaterality
| ImageLaterality (0020,0062) vr=CS, vm=1, type=3.
DRTAnatomicRegionSequence | AnatomicRegionSequence
| AnatomicRegionSequence (0008,2218) vr=SQ, vm=1, type=3.
DRTPrimaryAnatomicStructureSequence | PrimaryAnatomicStructureSequence
| PrimaryAnatomicStructureSequence (0008,2228) vr=SQ, vm=1, type=3.
DRTReferencedImageSequence | ReferencedImageSequence
| ReferencedImageSequence (0008,1140) vr=SQ, vm=1, type=3.
DRTReferencedInstanceSequence | ReferencedInstanceSequence
| ReferencedInstanceSequence (0008,114a) vr=SQ, vm=1, type=3.
DcmShortText | DerivationDescription
| DerivationDescription (0008,2111) vr=ST, vm=1, type=3.
DRTDerivationCodeSequence | DerivationCodeSequence
| DerivationCodeSequence (0008,9215) vr=SQ, vm=1, type=3.
DRTSourceImageSequence | SourceImageSequence
| SourceImageSequence (0008,2112) vr=SQ, vm=1, type=3.
DRTSourceInstanceSequence | SourceInstanceSequence
| SourceInstanceSequence (0042,0013) vr=SQ, vm=1, type=3.
DcmUnsignedShort | Rows
| Rows (0028,0010) vr=US, vm=1, type=1.
DcmUnsignedShort | Columns
| Columns (0028,0011) vr=US, vm=1, type=1.
DcmUnsignedShort | PlanarConfiguration
| PlanarConfiguration (0028,0006) vr=US, vm=1, type=1C.
DcmIntegerString | PixelAspectRatio
| PixelAspectRatio (0028,0034) vr=IS, vm=2, type=1C.
DcmUnsignedShort | SmallestImagePixelValue
| SmallestImagePixelValue (0028,0106) vr=US/SS, vm=1, type=3.
DcmUnsignedShort | LargestImagePixelValue
| LargestImagePixelValue (0028,0107) vr=US/SS, vm=1, type=3.
DcmUnsignedShort | RedPaletteColorLookupTableDescriptor
| RedPaletteColorLookupTableDescriptor (0028,1101) vr=US/SS, vm=3, type=1C.
DcmUnsignedShort | GreenPaletteColorLookupTableDescriptor
| GreenPaletteColorLookupTableDescriptor (0028,1102) vr=US/SS, vm=3, type=1C.
DcmUnsignedShort | BluePaletteColorLookupTableDescriptor
| BluePaletteColorLookupTableDescriptor (0028,1103) vr=US/SS, vm=3, type=1C.
DcmOtherByteOtherWord | RedPaletteColorLookupTableData
| RedPaletteColorLookupTableData (0028,1201) vr=OW, vm=1, type=1C.
DcmOtherByteOtherWord | GreenPaletteColorLookupTableData
| GreenPaletteColorLookupTableData (0028,1202) vr=OW, vm=1, type=1C.
DcmOtherByteOtherWord | BluePaletteColorLookupTableData
| BluePaletteColorLookupTableData (0028,1203) vr=OW, vm=1, type=1C.
DcmOtherByteOtherWord | ICCProfile
| ICCProfile (0028,2000) vr=OB, vm=1, type=3.
DcmCodeString | ColorSpace
| ColorSpace (0028,2002) vr=CS, vm=1, type=3.
DcmPixelData | PixelData
| PixelData (7fe0,0010) vr=OB/OW, vm=1, type=1C.
DcmUniversalResourceIdentifierOrLocator | PixelDataProviderURL
| PixelDataProviderURL (0028,7fe0) vr=UR, vm=1, type=1C.
DcmUnsignedShort | PixelPaddingRangeLimit
| PixelPaddingRangeLimit (0028,0121) vr=US/SS, vm=1, type=1C.
DcmOther64bitVeryLong | ExtendedOffsetTable
| ExtendedOffsetTable (7fe0,0001) vr=OV, vm=1, type=3.
DcmOther64bitVeryLong | ExtendedOffsetTableLengths
| ExtendedOffsetTableLengths (7fe0,0002) vr=OV, vm=1, type=1C.
DcmLongString | ContrastBolusAgent
| ContrastBolusAgent (0018,0010) vr=LO, vm=1, type=2.
DRTContrastBolusAgentSequence | ContrastBolusAgentSequence
| ContrastBolusAgentSequence (0018,0012) vr=SQ, vm=1, type=3.
DcmLongString | ContrastBolusRoute
| ContrastBolusRoute (0018,1040) vr=LO, vm=1, type=3.
DRTContrastBolusAdministrationRouteSequence | ContrastBolusAdministrationRouteSequence
| ContrastBolusAdministrationRouteSequence (0018,0014) vr=SQ, vm=1, type=3.
DcmDecimalString | ContrastBolusVolume
| ContrastBolusVolume (0018,1041) vr=DS, vm=1, type=3.
DcmTime | ContrastBolusStartTime
| ContrastBolusStartTime (0018,1042) vr=TM, vm=1, type=3.
DcmTime | ContrastBolusStopTime
| ContrastBolusStopTime (0018,1043) vr=TM, vm=1, type=3.
DcmDecimalString | ContrastBolusTotalDose
| ContrastBolusTotalDose (0018,1044) vr=DS, vm=1, type=3.
DcmDecimalString | ContrastFlowRate
| ContrastFlowRate (0018,1046) vr=DS, vm=1-n, type=3.
DcmDecimalString | ContrastFlowDuration
| ContrastFlowDuration (0018,1047) vr=DS, vm=1-n, type=3.
DcmCodeString | ContrastBolusIngredient
| ContrastBolusIngredient (0018,1048) vr=CS, vm=1, type=3.
DcmDecimalString | ContrastBolusIngredientConcentration
| ContrastBolusIngredientConcentration (0018,1049) vr=DS, vm=1, type=3.
DcmUnsignedShort | PreferredPlaybackSequencing
| PreferredPlaybackSequencing (0018,1244) vr=US, vm=1, type=3.
DcmDecimalString | FrameTime
| FrameTime (0018,1063) vr=DS, vm=1, type=1C.
DcmDecimalString | FrameTimeVector
| FrameTimeVector (0018,1065) vr=DS, vm=1-n, type=1C.
DcmIntegerString | StartTrim
| StartTrim (0008,2142) vr=IS, vm=1, type=3.
DcmIntegerString | StopTrim
| StopTrim (0008,2143) vr=IS, vm=1, type=3.
DcmIntegerString | RecommendedDisplayFrameRate
| RecommendedDisplayFrameRate (0008,2144) vr=IS, vm=1, type=3.
DcmIntegerString | CineRate
| CineRate (0018,0040) vr=IS, vm=1, type=3.
DcmDecimalString | FrameDelay
| FrameDelay (0018,1066) vr=DS, vm=1, type=3.
DcmDecimalString | ImageTriggerDelay
| ImageTriggerDelay (0018,1067) vr=DS, vm=1, type=3.
DcmDecimalString | EffectiveDuration
| EffectiveDuration (0018,0072) vr=DS, vm=1, type=3.
DcmIntegerString | ActualFrameDuration
| ActualFrameDuration (0018,1242) vr=IS, vm=1, type=3.
DRTMultiplexedAudioChannelsDescriptionCodeSequence | MultiplexedAudioChannelsDescriptionCodeSequence
| MultiplexedAudioChannelsDescriptionCodeSequence (003a,0300) vr=SQ, vm=1, type=2C.
DcmIntegerString | NumberOfFrames
| NumberOfFrames (0028,0008) vr=IS, vm=1, type=1.
DcmAttributeTag | FrameIncrementPointer
| FrameIncrementPointer (0028,0009) vr=AT, vm=1-n, type=1.
DcmCodeString | StereoPairsPresent
| StereoPairsPresent (0022,0028) vr=CS, vm=1, type=3.
DcmUnsigned64bitVeryLong | EncapsulatedPixelDataValueTotalLength
| EncapsulatedPixelDataValueTotalLength (7fe0,0003) vr=UV, vm=1, type=3.
DRTDeviceSequence | DeviceSequence
| DeviceSequence (0050,0010) vr=SQ, vm=1, type=1.
DcmUnsignedShort | SamplesPerPixel
| SamplesPerPixel (0028,0002) vr=US, vm=1, type=1. More...
DcmCodeString | PhotometricInterpretation
| PhotometricInterpretation (0028,0004) vr=CS, vm=1, type=1. More...
DcmUnsignedShort | BitsAllocated
| BitsAllocated (0028,0100) vr=US, vm=1, type=1. More...
DcmUnsignedShort | BitsStored
| BitsStored (0028,0101) vr=US, vm=1, type=1. More...
DcmUnsignedShort | HighBit
| HighBit (0028,0102) vr=US, vm=1, type=1. More...
DcmUnsignedShort | PixelRepresentation
| PixelRepresentation (0028,0103) vr=US, vm=1, type=1. More...
DcmCodeString | PixelIntensityRelationship
| PixelIntensityRelationship (0028,1040) vr=CS, vm=1, type=3.
DcmSignedShort | PixelIntensityRelationshipSign
| PixelIntensityRelationshipSign (0028,1041) vr=SS, vm=1, type=1C.
DcmShortString | RTImageLabel
| RTImageLabel (3002,0002) vr=SH, vm=1, type=1.
DcmLongString | RTImageName
| RTImageName (3002,0003) vr=LO, vm=1, type=3.
DcmShortText | RTImageDescription
| RTImageDescription (3002,0004) vr=ST, vm=1, type=3.
DcmCodeString | ImageType
| ImageType (0008,0008) vr=CS, vm=2-n, type=1. More...
DcmCodeString | ConversionType
| ConversionType (0008,0064) vr=CS, vm=1, type=2.
DcmCodeString | ReportedValuesOrigin
| ReportedValuesOrigin (3002,000a) vr=CS, vm=1, type=2C.
DcmCodeString | RTImagePlane
| RTImagePlane (3002,000c) vr=CS, vm=1, type=1.
DcmDecimalString | XRayImageReceptorTranslation
| XRayImageReceptorTranslation (3002,000d) vr=DS, vm=3, type=3.
DcmDecimalString | XRayImageReceptorAngle
| XRayImageReceptorAngle (3002,000e) vr=DS, vm=1, type=2.
DcmDecimalString | RTImageOrientation
| RTImageOrientation (3002,0010) vr=DS, vm=6, type=2C.
DcmDecimalString | ImagePlanePixelSpacing
| ImagePlanePixelSpacing (3002,0011) vr=DS, vm=2, type=2.
DcmDecimalString | RTImagePosition
| RTImagePosition (3002,0012) vr=DS, vm=2, type=2.
DcmShortString | RadiationMachineName
| RadiationMachineName (3002,0020) vr=SH, vm=1, type=2.
DcmCodeString | PrimaryDosimeterUnit
| PrimaryDosimeterUnit (300a,00b3) vr=CS, vm=1, type=2.
DcmDecimalString | RadiationMachineSAD
| RadiationMachineSAD (3002,0022) vr=DS, vm=1, type=2.
DcmDecimalString | RadiationMachineSSD
| RadiationMachineSSD (3002,0024) vr=DS, vm=1, type=3.
DcmDecimalString | RTImageSID
| RTImageSID (3002,0026) vr=DS, vm=1, type=2.
DcmCodeString | EnhancedRTBeamLimitingDeviceDefinitionFlag
| EnhancedRTBeamLimitingDeviceDefinitionFlag (3008,00a3) vr=CS, vm=1, type=3.
DRTEnhancedRTBeamLimitingDeviceSequence | EnhancedRTBeamLimitingDeviceSequence
| EnhancedRTBeamLimitingDeviceSequence (3008,00a1) vr=SQ, vm=1, type=1C.
DcmDecimalString | SourceToReferenceObjectDistance
| SourceToReferenceObjectDistance (3002,0028) vr=DS, vm=1, type=3.
DRTReferencedRTPlanSequenceInRTImageModule | ReferencedRTPlanSequence
| ReferencedRTPlanSequence (300c,0002) vr=SQ, vm=1, type=3.
DcmIntegerString | ReferencedBeamNumber
| ReferencedBeamNumber (300c,0006) vr=IS, vm=1, type=3.
DcmIntegerString | ReferencedFractionGroupNumber
| ReferencedFractionGroupNumber (300c,0022) vr=IS, vm=1, type=3.
DcmIntegerString | FractionNumber
| FractionNumber (3002,0029) vr=IS, vm=1, type=3.
DcmDecimalString | StartCumulativeMetersetWeight
| StartCumulativeMetersetWeight (300c,0008) vr=DS, vm=1, type=3.
DcmDecimalString | EndCumulativeMetersetWeight
| EndCumulativeMetersetWeight (300c,0009) vr=DS, vm=1, type=3.
DRTExposureSequence | ExposureSequence
| ExposureSequence (3002,0030) vr=SQ, vm=1, type=3.
DRTFluenceMapSequence | FluenceMapSequence
| FluenceMapSequence (3002,0040) vr=SQ, vm=1, type=1C.
DcmDecimalString | GantryAngle
| GantryAngle (300a,011e) vr=DS, vm=1, type=3.
DcmFloatingPointSingle | GantryPitchAngle
| GantryPitchAngle (300a,014a) vr=FL, vm=1, type=3.
DcmDecimalString | BeamLimitingDeviceAngle
| BeamLimitingDeviceAngle (300a,0120) vr=DS, vm=1, type=3.
DcmDecimalString | PatientSupportAngle
| PatientSupportAngle (300a,0122) vr=DS, vm=1, type=3.
DcmDecimalString | TableTopEccentricAxisDistance
| TableTopEccentricAxisDistance (300a,0124) vr=DS, vm=1, type=3.
DcmDecimalString | TableTopEccentricAngle
| TableTopEccentricAngle (300a,0125) vr=DS, vm=1, type=3.
DcmFloatingPointSingle | TableTopPitchAngle
| TableTopPitchAngle (300a,0140) vr=FL, vm=1, type=3.
DcmFloatingPointSingle | TableTopRollAngle
| TableTopRollAngle (300a,0144) vr=FL, vm=1, type=3.
DcmDecimalString | TableTopVerticalPosition
| TableTopVerticalPosition (300a,0128) vr=DS, vm=1, type=3.
DcmDecimalString | TableTopLongitudinalPosition
| TableTopLongitudinalPosition (300a,0129) vr=DS, vm=1, type=3.
DcmDecimalString | TableTopLateralPosition
| TableTopLateralPosition (300a,012a) vr=DS, vm=1, type=3.
DcmDecimalString | IsocenterPosition
| IsocenterPosition (300a,012c) vr=DS, vm=3, type=3.
DcmCodeString | PatientPosition
| PatientPosition (0018,5100) vr=CS, vm=1, type=1C.
DcmIntegerString | ExposureTime
| ExposureTime (0018,1150) vr=IS, vm=1, type=3.
DcmFloatingPointDouble | ExposureTimeInms
| ExposureTimeInms (0018,9328) vr=FD, vm=1, type=3.
DcmDecimalString | MetersetExposure
| MetersetExposure (3002,0032) vr=DS, vm=1, type=3.
DRTModalityLUTSequence | ModalityLUTSequence
| ModalityLUTSequence (0028,3000) vr=SQ, vm=1, type=1C.
DcmDecimalString | RescaleIntercept
| RescaleIntercept (0028,1052) vr=DS, vm=1, type=1C.
DcmDecimalString | RescaleSlope
| RescaleSlope (0028,1053) vr=DS, vm=1, type=1C.
DcmLongString | RescaleType
| RescaleType (0028,1054) vr=LO, vm=1, type=1C.
DRTVOILUTSequence | VOILUTSequence
| VOILUTSequence (0028,3010) vr=SQ, vm=1, type=1C.
DcmDecimalString | WindowCenter
| WindowCenter (0028,1050) vr=DS, vm=1-n, type=1C.
DcmDecimalString | WindowWidth
| WindowWidth (0028,1051) vr=DS, vm=1-n, type=1C.
DcmLongString | WindowCenterWidthExplanation
| WindowCenterWidthExplanation (0028,1055) vr=LO, vm=1-n, type=3.
DcmCodeString | VOILUTFunction
| VOILUTFunction (0028,1056) vr=CS, vm=1, type=3.
DcmCodeString | ApprovalStatus
| ApprovalStatus (300e,0002) vr=CS, vm=1, type=1.
DcmDate | ReviewDate
| ReviewDate (300e,0004) vr=DA, vm=1, type=2C.
DcmTime | ReviewTime
| ReviewTime (300e,0005) vr=TM, vm=1, type=2C.
DcmPersonName | ReviewerName
| ReviewerName (300e,0008) vr=PN, vm=1, type=2C.
DcmUniqueIdentifier | SOPClassUID
| SOPClassUID (0008,0016) vr=UI, vm=1, type=1.
DcmUniqueIdentifier | SOPInstanceUID
| SOPInstanceUID (0008,0018) vr=UI, vm=1, type=1.
DcmCodeString | SpecificCharacterSet
| SpecificCharacterSet (0008,0005) vr=CS, vm=1-n, type=1C.
DcmDate | InstanceCreationDate
| InstanceCreationDate (0008,0012) vr=DA, vm=1, type=3.
DcmTime | InstanceCreationTime
| InstanceCreationTime (0008,0013) vr=TM, vm=1, type=3.
DcmDateTime | InstanceCoercionDateTime
| InstanceCoercionDateTime (0008,0015) vr=DT, vm=1, type=3.
DcmUniqueIdentifier | InstanceCreatorUID
| InstanceCreatorUID (0008,0014) vr=UI, vm=1, type=3.
DcmUniqueIdentifier | RelatedGeneralSOPClassUID
| RelatedGeneralSOPClassUID (0008,001a) vr=UI, vm=1-n, type=3.
DcmUniqueIdentifier | OriginalSpecializedSOPClassUID
| OriginalSpecializedSOPClassUID (0008,001b) vr=UI, vm=1, type=3.
DRTCodingSchemeIdentificationSequence | CodingSchemeIdentificationSequence
| CodingSchemeIdentificationSequence (0008,0110) vr=SQ, vm=1, type=3.
DRTContextGroupIdentificationSequence | ContextGroupIdentificationSequence
| ContextGroupIdentificationSequence (0008,0123) vr=SQ, vm=1, type=3.
DRTMappingResourceIdentificationSequence | MappingResourceIdentificationSequence
| MappingResourceIdentificationSequence (0008,0124) vr=SQ, vm=1, type=3.
DcmShortString | TimezoneOffsetFromUTC
| TimezoneOffsetFromUTC (0008,0201) vr=SH, vm=1, type=3.
DRTContributingEquipmentSequence | ContributingEquipmentSequence
| ContributingEquipmentSequence (0018,a001) vr=SQ, vm=1, type=3.
DcmCodeString | SOPInstanceStatus
| SOPInstanceStatus (0100,0410) vr=CS, vm=1, type=3.
DcmDateTime | SOPAuthorizationDateTime
| SOPAuthorizationDateTime (0100,0420) vr=DT, vm=1, type=3.
DcmLongText | SOPAuthorizationComment
| SOPAuthorizationComment (0100,0424) vr=LT, vm=1, type=3.
DcmLongString | AuthorizationEquipmentCertificationNumber
| AuthorizationEquipmentCertificationNumber (0100,0426) vr=LO, vm=1, type=3.
DRTMACParametersSequence | MACParametersSequence
| MACParametersSequence (4ffe,0001) vr=SQ, vm=1, type=3.
DRTDigitalSignaturesSequence | DigitalSignaturesSequence
| DigitalSignaturesSequence (fffa,fffa) vr=SQ, vm=1, type=3.
DRTEncryptedAttributesSequence | EncryptedAttributesSequence
| EncryptedAttributesSequence (0400,0500) vr=SQ, vm=1, type=1C.
DRTOriginalAttributesSequence | OriginalAttributesSequence
| OriginalAttributesSequence (0400,0561) vr=SQ, vm=1, type=3.
DRTHL7StructuredDocumentReferenceSequence | HL7StructuredDocumentReferenceSequence
| HL7StructuredDocumentReferenceSequence (0040,a390) vr=SQ, vm=1, type=1C.
DcmCodeString | LongitudinalTemporalInformationModified
| LongitudinalTemporalInformationModified (0028,0303) vr=CS, vm=1, type=3.
DcmCodeString | QueryRetrieveView
| QueryRetrieveView (0008,0053) vr=CS, vm=1, type=1C.
DRTConversionSourceAttributesSequence | ConversionSourceAttributesSequence
| ConversionSourceAttributesSequence (0020,9172) vr=SQ, vm=1, type=1C.
DcmCodeString | ContentQualification
| ContentQualification (0018,9004) vr=CS, vm=1, type=3.
DRTPrivateDataElementCharacteristicsSequence | PrivateDataElementCharacteristicsSequence
| PrivateDataElementCharacteristicsSequence (0008,0300) vr=SQ, vm=1, type=3.
DcmCodeString | InstanceOriginStatus
| InstanceOriginStatus (0400,0600) vr=CS, vm=1, type=3.
DcmLongText | BarcodeValue
| BarcodeValue (2200,0005) vr=LT, vm=1, type=3.
DRTReferencedDefinedProtocolSequence | ReferencedDefinedProtocolSequence
| ReferencedDefinedProtocolSequence (0018,990c) vr=SQ, vm=1, type=1C.
DRTReferencedPerformedProtocolSequence | ReferencedPerformedProtocolSequence
| ReferencedPerformedProtocolSequence (0018,990d) vr=SQ, vm=1, type=1C.
DRTReferencedSeriesSequence | ReferencedSeriesSequence
| ReferencedSeriesSequence (0008,1115) vr=SQ, vm=1, type=1C.
DRTStudiesContainingOtherReferencedInstancesSequence | StudiesContainingOtherReferencedInstancesSequence
| StudiesContainingOtherReferencedInstancesSequence (0008,1200) vr=SQ, vm=1, type=1C.
DRTFrameExtractionSequence | FrameExtractionSequence
| FrameExtractionSequence (0008,1164) vr=SQ, vm=1, type=1.

## Additional Inherited Members
Static Protected Member Functions inherited from DRTTypes
static OFCondition | addElementToDataset (OFCondition &result, DcmItem &dataset, DcmElement *element, const OFString &vm, const OFString &type, const char *moduleName=NULL)
| add given element to the dataset. More...
static OFCondition | getElementFromDataset (DcmItem &dataset, DcmElement &element)
| get element from dataset More...
static OFCondition | getStringValueFromElement (const DcmElement &element, OFString &stringValue, const signed long pos=0)
| get string value from element More...
static OFCondition | getStringValueFromDataset (DcmItem &dataset, const DcmTagKey &tagKey, OFString &stringValue)
| get string value from dataset More...
static OFCondition | putStringValueToDataset (DcmItem &dataset, const DcmTag &tag, const OFString &stringValue, const OFBool allowEmpty=OFTrue)
| put string value to dataset More...
static OFBool | checkElementValue (DcmElement &element, const OFString &vm, const OFString &type, const OFCondition &searchCond=EC_Normal, const char *moduleName=NULL)
| check element value for correct value multiplicity and type More...
static OFCondition | getAndCheckElementFromDataset (DcmItem &dataset, DcmElement &element, const OFString &vm, const OFString &type, const char *moduleName=NULL)
| get element from dataset and check it for correct value multiplicity and type. More...
static OFCondition | getAndCheckStringValueFromDataset (DcmItem &dataset, const DcmTagKey &tagKey, OFString &stringValue, const OFString &vm, const OFString &type, const char *moduleName=NULL)
| get string value from dataset and check it for correct value multiplicity and type. More...

## Detailed Description

Interface class for RTImageIOD.

Note
  Because of its many member variables, an instance of this class requires quite some memory. So be careful when creating automatic variables from this class (the stack size might be exceeded); it is probably better to use the heap space.

## Constructor & Destructor Documentation

## ◆ DRTImageIOD()

DRTImageIOD::DRTImageIOD | ( | const DRTImageIOD & | copy | ) |

copy constructor

Parameters

  copy | IOD object to be copied

## Member Function Documentation

## ◆ checkDatasetForReading()

OFCondition DRTImageIOD::checkDatasetForReading | ( | DcmItem & | dataset | ) |
| protected

check the given dataset before reading.

This methods checks whether the dataset contains at least the DICOM attribute SOPClassUID (0008,0016) with the expected value. Any incorrectness regarding this attribute is reported to the log stream (if enabled for error messages).

Parameters

  dataset | DICOM dataset to be checked

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAccessionNumber()

virtual OFCondition DRTImageIOD::getAccessionNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AccessionNumber (0008,0050)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAcquisitionDate()

virtual OFCondition DRTImageIOD::getAcquisitionDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AcquisitionDate (0008,0022)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAcquisitionDateTime()

virtual OFCondition DRTImageIOD::getAcquisitionDateTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AcquisitionDateTime (0008,002a)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAcquisitionDuration()

virtual OFCondition DRTImageIOD::getAcquisitionDuration | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get AcquisitionDuration (0018,9073)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAcquisitionNumber() [1/2]

virtual OFCondition DRTImageIOD::getAcquisitionNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AcquisitionNumber (0020,0012)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAcquisitionNumber() [2/2]

virtual OFCondition DRTImageIOD::getAcquisitionNumber | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get AcquisitionNumber (0020,0012)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAcquisitionTime()

virtual OFCondition DRTImageIOD::getAcquisitionTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AcquisitionTime (0008,0032)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAcquisitionUID()

virtual OFCondition DRTImageIOD::getAcquisitionUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AcquisitionUID (0008,0017)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getActualFrameDuration() [1/2]

virtual OFCondition DRTImageIOD::getActualFrameDuration | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ActualFrameDuration (0018,1242)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getActualFrameDuration() [2/2]

virtual OFCondition DRTImageIOD::getActualFrameDuration | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ActualFrameDuration (0018,1242)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAdditionalPatientHistory()

virtual OFCondition DRTImageIOD::getAdditionalPatientHistory | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AdditionalPatientHistory (0010,21b0)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAdmissionID()

virtual OFCondition DRTImageIOD::getAdmissionID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AdmissionID (0038,0010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAdmittingDiagnosesCodeSequence() [1/2]

DRTAdmittingDiagnosesCodeSequence& DRTImageIOD::getAdmittingDiagnosesCodeSequence | ( |  | ) |
| inline

get AdmittingDiagnosesCodeSequence (0008,1084)

Returns
  reference to sequence element

## ◆ getAdmittingDiagnosesCodeSequence() [2/2]

const DRTAdmittingDiagnosesCodeSequence& DRTImageIOD::getAdmittingDiagnosesCodeSequence | ( |  | ) | const
| inline

get AdmittingDiagnosesCodeSequence (0008,1084)

Returns
  const reference to sequence element

## ◆ getAdmittingDiagnosesDescription()

virtual OFCondition DRTImageIOD::getAdmittingDiagnosesDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AdmittingDiagnosesDescription (0008,1080)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAllergies()

virtual OFCondition DRTImageIOD::getAllergies | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get Allergies (0010,2110)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAnatomicRegionSequence() [1/2]

DRTAnatomicRegionSequence& DRTImageIOD::getAnatomicRegionSequence | ( |  | ) |
| inline

get AnatomicRegionSequence (0008,2218)

Returns
  reference to sequence element

## ◆ getAnatomicRegionSequence() [2/2]

const DRTAnatomicRegionSequence& DRTImageIOD::getAnatomicRegionSequence | ( |  | ) | const
| inline

get AnatomicRegionSequence (0008,2218)

Returns
  const reference to sequence element

## ◆ getApprovalStatus()

virtual OFCondition DRTImageIOD::getApprovalStatus | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ApprovalStatus (300e,0002)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getAuthorizationEquipmentCertificationNumber()

virtual OFCondition DRTImageIOD::getAuthorizationEquipmentCertificationNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get AuthorizationEquipmentCertificationNumber (0100,0426)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getBarcodeValue()

virtual OFCondition DRTImageIOD::getBarcodeValue | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get BarcodeValue (2200,0005)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getBeamLimitingDeviceAngle() [1/2]

virtual OFCondition DRTImageIOD::getBeamLimitingDeviceAngle | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get BeamLimitingDeviceAngle (300a,0120)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getBeamLimitingDeviceAngle() [2/2]

virtual OFCondition DRTImageIOD::getBeamLimitingDeviceAngle | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get BeamLimitingDeviceAngle (300a,0120)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getBitsAllocated()

virtual OFCondition DRTImageIOD::getBitsAllocated | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get BitsAllocated (0028,0100)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getBitsStored()

virtual OFCondition DRTImageIOD::getBitsStored | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get BitsStored (0028,0101)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getBluePaletteColorLookupTableData()

virtual OFCondition DRTImageIOD::getBluePaletteColorLookupTableData | ( | Uint16 *& | value,
|  | unsigned long * | count = `NULL`
| ) |  | const
| virtual

get BluePaletteColorLookupTableData (0028,1203)

Parameters

  value | reference to variable in which the value should be stored
  count | stores number of items in the result array (if not NULL)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getBluePaletteColorLookupTableDescriptor()

virtual OFCondition DRTImageIOD::getBluePaletteColorLookupTableDescriptor | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get BluePaletteColorLookupTableDescriptor (0028,1103)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getBreedRegistrationSequence() [1/2]

DRTBreedRegistrationSequence& DRTImageIOD::getBreedRegistrationSequence | ( |  | ) |
| inline

get BreedRegistrationSequence (0010,2294)

Returns
  reference to sequence element

## ◆ getBreedRegistrationSequence() [2/2]

const DRTBreedRegistrationSequence& DRTImageIOD::getBreedRegistrationSequence | ( |  | ) | const
| inline

get BreedRegistrationSequence (0010,2294)

Returns
  const reference to sequence element

## ◆ getBurnedInAnnotation()

virtual OFCondition DRTImageIOD::getBurnedInAnnotation | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get BurnedInAnnotation (0028,0301)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getCineRate() [1/2]

virtual OFCondition DRTImageIOD::getCineRate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get CineRate (0018,0040)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getCineRate() [2/2]

virtual OFCondition DRTImageIOD::getCineRate | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get CineRate (0018,0040)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialCoordinatingCenterName()

virtual OFCondition DRTImageIOD::getClinicalTrialCoordinatingCenterName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialCoordinatingCenterName (0012,0060)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialProtocolEthicsCommitteeApprovalNumber()

virtual OFCondition DRTImageIOD::getClinicalTrialProtocolEthicsCommitteeApprovalNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialProtocolEthicsCommitteeApprovalNumber (0012,0082)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialProtocolEthicsCommitteeName()

virtual OFCondition DRTImageIOD::getClinicalTrialProtocolEthicsCommitteeName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialProtocolEthicsCommitteeName (0012,0081)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialProtocolID()

virtual OFCondition DRTImageIOD::getClinicalTrialProtocolID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialProtocolID (0012,0020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialProtocolName()

virtual OFCondition DRTImageIOD::getClinicalTrialProtocolName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialProtocolName (0012,0021)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialSeriesDescription()

virtual OFCondition DRTImageIOD::getClinicalTrialSeriesDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialSeriesDescription (0012,0072)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialSeriesID()

virtual OFCondition DRTImageIOD::getClinicalTrialSeriesID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialSeriesID (0012,0071)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialSiteID()

virtual OFCondition DRTImageIOD::getClinicalTrialSiteID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialSiteID (0012,0030)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialSiteName()

virtual OFCondition DRTImageIOD::getClinicalTrialSiteName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialSiteName (0012,0031)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialSponsorName()

virtual OFCondition DRTImageIOD::getClinicalTrialSponsorName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialSponsorName (0012,0010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialSubjectID()

virtual OFCondition DRTImageIOD::getClinicalTrialSubjectID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialSubjectID (0012,0040)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialSubjectReadingID()

virtual OFCondition DRTImageIOD::getClinicalTrialSubjectReadingID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialSubjectReadingID (0012,0042)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialTimePointDescription()

virtual OFCondition DRTImageIOD::getClinicalTrialTimePointDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialTimePointDescription (0012,0051)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialTimePointID()

virtual OFCondition DRTImageIOD::getClinicalTrialTimePointID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ClinicalTrialTimePointID (0012,0050)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getClinicalTrialTimePointTypeCodeSequence() [1/2]

DRTClinicalTrialTimePointTypeCodeSequence& DRTImageIOD::getClinicalTrialTimePointTypeCodeSequence | ( |  | ) |
| inline

get ClinicalTrialTimePointTypeCodeSequence (0012,0054)

Returns
  reference to sequence element

## ◆ getClinicalTrialTimePointTypeCodeSequence() [2/2]

const DRTClinicalTrialTimePointTypeCodeSequence& DRTImageIOD::getClinicalTrialTimePointTypeCodeSequence | ( |  | ) | const
| inline

get ClinicalTrialTimePointTypeCodeSequence (0012,0054)

Returns
  const reference to sequence element

## ◆ getCodingSchemeIdentificationSequence() [1/2]

DRTCodingSchemeIdentificationSequence& DRTImageIOD::getCodingSchemeIdentificationSequence | ( |  | ) |
| inline

get CodingSchemeIdentificationSequence (0008,0110)

Returns
  reference to sequence element

## ◆ getCodingSchemeIdentificationSequence() [2/2]

const DRTCodingSchemeIdentificationSequence& DRTImageIOD::getCodingSchemeIdentificationSequence | ( |  | ) | const
| inline

get CodingSchemeIdentificationSequence (0008,0110)

Returns
  const reference to sequence element

## ◆ getColorSpace()

virtual OFCondition DRTImageIOD::getColorSpace | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ColorSpace (0028,2002)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getColumns()

virtual OFCondition DRTImageIOD::getColumns | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get Columns (0028,0011)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getCommentsOnThePerformedProcedureStep()

virtual OFCondition DRTImageIOD::getCommentsOnThePerformedProcedureStep | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get CommentsOnThePerformedProcedureStep (0040,0280)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getConsentForClinicalTrialUseSequence() [1/2]

DRTConsentForClinicalTrialUseSequence& DRTImageIOD::getConsentForClinicalTrialUseSequence | ( |  | ) |
| inline

get ConsentForClinicalTrialUseSequence (0012,0083)

Returns
  reference to sequence element

## ◆ getConsentForClinicalTrialUseSequence() [2/2]

const DRTConsentForClinicalTrialUseSequence& DRTImageIOD::getConsentForClinicalTrialUseSequence | ( |  | ) | const
| inline

get ConsentForClinicalTrialUseSequence (0012,0083)

Returns
  const reference to sequence element

## ◆ getConsultingPhysicianIdentificationSequence() [1/2]

DRTConsultingPhysicianIdentificationSequence& DRTImageIOD::getConsultingPhysicianIdentificationSequence | ( |  | ) |
| inline

get ConsultingPhysicianIdentificationSequence (0008,009d)

Returns
  reference to sequence element

## ◆ getConsultingPhysicianIdentificationSequence() [2/2]

const DRTConsultingPhysicianIdentificationSequence& DRTImageIOD::getConsultingPhysicianIdentificationSequence | ( |  | ) | const
| inline

get ConsultingPhysicianIdentificationSequence (0008,009d)

Returns
  const reference to sequence element

## ◆ getConsultingPhysicianName()

virtual OFCondition DRTImageIOD::getConsultingPhysicianName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ConsultingPhysicianName (0008,009c)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContentDate()

virtual OFCondition DRTImageIOD::getContentDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContentDate (0008,0023)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContentQualification()

virtual OFCondition DRTImageIOD::getContentQualification | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContentQualification (0018,9004)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContentTime()

virtual OFCondition DRTImageIOD::getContentTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContentTime (0008,0033)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContextGroupIdentificationSequence() [1/2]

DRTContextGroupIdentificationSequence& DRTImageIOD::getContextGroupIdentificationSequence | ( |  | ) |
| inline

get ContextGroupIdentificationSequence (0008,0123)

Returns
  reference to sequence element

## ◆ getContextGroupIdentificationSequence() [2/2]

const DRTContextGroupIdentificationSequence& DRTImageIOD::getContextGroupIdentificationSequence | ( |  | ) | const
| inline

get ContextGroupIdentificationSequence (0008,0123)

Returns
  const reference to sequence element

## ◆ getContrastBolusAdministrationRouteSequence() [1/2]

DRTContrastBolusAdministrationRouteSequence& DRTImageIOD::getContrastBolusAdministrationRouteSequence | ( |  | ) |
| inline

get ContrastBolusAdministrationRouteSequence (0018,0014)

Returns
  reference to sequence element

## ◆ getContrastBolusAdministrationRouteSequence() [2/2]

const DRTContrastBolusAdministrationRouteSequence& DRTImageIOD::getContrastBolusAdministrationRouteSequence | ( |  | ) | const
| inline

get ContrastBolusAdministrationRouteSequence (0018,0014)

Returns
  const reference to sequence element

## ◆ getContrastBolusAgent()

virtual OFCondition DRTImageIOD::getContrastBolusAgent | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusAgent (0018,0010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusAgentSequence() [1/2]

DRTContrastBolusAgentSequence& DRTImageIOD::getContrastBolusAgentSequence | ( |  | ) |
| inline

get ContrastBolusAgentSequence (0018,0012)

Returns
  reference to sequence element

## ◆ getContrastBolusAgentSequence() [2/2]

const DRTContrastBolusAgentSequence& DRTImageIOD::getContrastBolusAgentSequence | ( |  | ) | const
| inline

get ContrastBolusAgentSequence (0018,0012)

Returns
  const reference to sequence element

## ◆ getContrastBolusIngredient()

virtual OFCondition DRTImageIOD::getContrastBolusIngredient | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusIngredient (0018,1048)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusIngredientConcentration() [1/2]

virtual OFCondition DRTImageIOD::getContrastBolusIngredientConcentration | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusIngredientConcentration (0018,1049)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusIngredientConcentration() [2/2]

virtual OFCondition DRTImageIOD::getContrastBolusIngredientConcentration | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusIngredientConcentration (0018,1049)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusRoute()

virtual OFCondition DRTImageIOD::getContrastBolusRoute | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusRoute (0018,1040)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusStartTime()

virtual OFCondition DRTImageIOD::getContrastBolusStartTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusStartTime (0018,1042)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusStopTime()

virtual OFCondition DRTImageIOD::getContrastBolusStopTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusStopTime (0018,1043)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusTotalDose() [1/2]

virtual OFCondition DRTImageIOD::getContrastBolusTotalDose | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusTotalDose (0018,1044)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusTotalDose() [2/2]

virtual OFCondition DRTImageIOD::getContrastBolusTotalDose | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusTotalDose (0018,1044)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusVolume() [1/2]

virtual OFCondition DRTImageIOD::getContrastBolusVolume | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusVolume (0018,1041)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastBolusVolume() [2/2]

virtual OFCondition DRTImageIOD::getContrastBolusVolume | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastBolusVolume (0018,1041)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastFlowDuration() [1/3]

virtual OFCondition DRTImageIOD::getContrastFlowDuration | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ContrastFlowDuration (0018,1047)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastFlowDuration() [2/3]

virtual OFCondition DRTImageIOD::getContrastFlowDuration | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastFlowDuration (0018,1047)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastFlowDuration() [3/3]

virtual OFCondition DRTImageIOD::getContrastFlowDuration | ( | OFVector< Float64 > & | value | ) | const
| virtual

get ContrastFlowDuration (0018,1047)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastFlowRate() [1/3]

virtual OFCondition DRTImageIOD::getContrastFlowRate | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ContrastFlowRate (0018,1046)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastFlowRate() [2/3]

virtual OFCondition DRTImageIOD::getContrastFlowRate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ContrastFlowRate (0018,1046)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContrastFlowRate() [3/3]

virtual OFCondition DRTImageIOD::getContrastFlowRate | ( | OFVector< Float64 > & | value | ) | const
| virtual

get ContrastFlowRate (0018,1046)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getContributingEquipmentSequence() [1/2]

DRTContributingEquipmentSequence& DRTImageIOD::getContributingEquipmentSequence | ( |  | ) |
| inline

get ContributingEquipmentSequence (0018,a001)

Returns
  reference to sequence element

## ◆ getContributingEquipmentSequence() [2/2]

const DRTContributingEquipmentSequence& DRTImageIOD::getContributingEquipmentSequence | ( |  | ) | const
| inline

get ContributingEquipmentSequence (0018,a001)

Returns
  const reference to sequence element

## ◆ getConversionSourceAttributesSequence() [1/2]

DRTConversionSourceAttributesSequence& DRTImageIOD::getConversionSourceAttributesSequence | ( |  | ) |
| inline

get ConversionSourceAttributesSequence (0020,9172)

Returns
  reference to sequence element

## ◆ getConversionSourceAttributesSequence() [2/2]

const DRTConversionSourceAttributesSequence& DRTImageIOD::getConversionSourceAttributesSequence | ( |  | ) | const
| inline

get ConversionSourceAttributesSequence (0020,9172)

Returns
  const reference to sequence element

## ◆ getConversionType()

virtual OFCondition DRTImageIOD::getConversionType | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ConversionType (0008,0064)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getDateOfLastCalibration()

virtual OFCondition DRTImageIOD::getDateOfLastCalibration | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get DateOfLastCalibration (0018,1200)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getDeidentificationMethod()

virtual OFCondition DRTImageIOD::getDeidentificationMethod | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get DeidentificationMethod (0012,0063)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getDeidentificationMethodCodeSequence() [1/2]

DRTDeidentificationMethodCodeSequence& DRTImageIOD::getDeidentificationMethodCodeSequence | ( |  | ) |
| inline

get DeidentificationMethodCodeSequence (0012,0064)

Returns
  reference to sequence element

## ◆ getDeidentificationMethodCodeSequence() [2/2]

const DRTDeidentificationMethodCodeSequence& DRTImageIOD::getDeidentificationMethodCodeSequence | ( |  | ) | const
| inline

get DeidentificationMethodCodeSequence (0012,0064)

Returns
  const reference to sequence element

## ◆ getDerivationCodeSequence() [1/2]

DRTDerivationCodeSequence& DRTImageIOD::getDerivationCodeSequence | ( |  | ) |
| inline

get DerivationCodeSequence (0008,9215)

Returns
  reference to sequence element

## ◆ getDerivationCodeSequence() [2/2]

const DRTDerivationCodeSequence& DRTImageIOD::getDerivationCodeSequence | ( |  | ) | const
| inline

get DerivationCodeSequence (0008,9215)

Returns
  const reference to sequence element

## ◆ getDerivationDescription()

virtual OFCondition DRTImageIOD::getDerivationDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get DerivationDescription (0008,2111)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getDeviceSequence() [1/2]

DRTDeviceSequence& DRTImageIOD::getDeviceSequence | ( |  | ) |
| inline

get DeviceSequence (0050,0010)

Returns
  reference to sequence element

## ◆ getDeviceSequence() [2/2]

const DRTDeviceSequence& DRTImageIOD::getDeviceSequence | ( |  | ) | const
| inline

get DeviceSequence (0050,0010)

Returns
  const reference to sequence element

## ◆ getDeviceSerialNumber()

virtual OFCondition DRTImageIOD::getDeviceSerialNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get DeviceSerialNumber (0018,1000)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getDeviceUID()

virtual OFCondition DRTImageIOD::getDeviceUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get DeviceUID (0018,1002)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getDigitalSignaturesSequence() [1/2]

DRTDigitalSignaturesSequence& DRTImageIOD::getDigitalSignaturesSequence | ( |  | ) |
| inline

get DigitalSignaturesSequence (fffa,fffa)

Returns
  reference to sequence element

## ◆ getDigitalSignaturesSequence() [2/2]

const DRTDigitalSignaturesSequence& DRTImageIOD::getDigitalSignaturesSequence | ( |  | ) | const
| inline

get DigitalSignaturesSequence (fffa,fffa)

Returns
  const reference to sequence element

## ◆ getEffectiveDuration() [1/2]

virtual OFCondition DRTImageIOD::getEffectiveDuration | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get EffectiveDuration (0018,0072)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getEffectiveDuration() [2/2]

virtual OFCondition DRTImageIOD::getEffectiveDuration | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get EffectiveDuration (0018,0072)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getEncapsulatedPixelDataValueTotalLength()

virtual OFCondition DRTImageIOD::getEncapsulatedPixelDataValueTotalLength | ( | Uint64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get EncapsulatedPixelDataValueTotalLength (7fe0,0003)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getEncryptedAttributesSequence() [1/2]

DRTEncryptedAttributesSequence& DRTImageIOD::getEncryptedAttributesSequence | ( |  | ) |
| inline

get EncryptedAttributesSequence (0400,0500)

Returns
  reference to sequence element

## ◆ getEncryptedAttributesSequence() [2/2]

const DRTEncryptedAttributesSequence& DRTImageIOD::getEncryptedAttributesSequence | ( |  | ) | const
| inline

get EncryptedAttributesSequence (0400,0500)

Returns
  const reference to sequence element

## ◆ getEndCumulativeMetersetWeight() [1/2]

virtual OFCondition DRTImageIOD::getEndCumulativeMetersetWeight | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get EndCumulativeMetersetWeight (300c,0009)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getEndCumulativeMetersetWeight() [2/2]

virtual OFCondition DRTImageIOD::getEndCumulativeMetersetWeight | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get EndCumulativeMetersetWeight (300c,0009)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getEnhancedRTBeamLimitingDeviceDefinitionFlag()

virtual OFCondition DRTImageIOD::getEnhancedRTBeamLimitingDeviceDefinitionFlag | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get EnhancedRTBeamLimitingDeviceDefinitionFlag (3008,00a3)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getEnhancedRTBeamLimitingDeviceSequence() [1/2]

DRTEnhancedRTBeamLimitingDeviceSequence& DRTImageIOD::getEnhancedRTBeamLimitingDeviceSequence | ( |  | ) |
| inline

get EnhancedRTBeamLimitingDeviceSequence (3008,00a1)

Returns
  reference to sequence element

## ◆ getEnhancedRTBeamLimitingDeviceSequence() [2/2]

const DRTEnhancedRTBeamLimitingDeviceSequence& DRTImageIOD::getEnhancedRTBeamLimitingDeviceSequence | ( |  | ) | const
| inline

get EnhancedRTBeamLimitingDeviceSequence (3008,00a1)

Returns
  const reference to sequence element

## ◆ getEthnicGroup()

virtual OFCondition DRTImageIOD::getEthnicGroup | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get EthnicGroup (0010,2160)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getExposureSequence() [1/2]

DRTExposureSequence& DRTImageIOD::getExposureSequence | ( |  | ) |
| inline

get ExposureSequence (3002,0030)

Returns
  reference to sequence element

## ◆ getExposureSequence() [2/2]

const DRTExposureSequence& DRTImageIOD::getExposureSequence | ( |  | ) | const
| inline

get ExposureSequence (3002,0030)

Returns
  const reference to sequence element

## ◆ getExposureTime() [1/2]

virtual OFCondition DRTImageIOD::getExposureTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ExposureTime (0018,1150)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getExposureTime() [2/2]

virtual OFCondition DRTImageIOD::getExposureTime | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ExposureTime (0018,1150)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getExposureTimeInms()

virtual OFCondition DRTImageIOD::getExposureTimeInms | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ExposureTimeInms (0018,9328)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getExtendedOffsetTable()

virtual OFCondition DRTImageIOD::getExtendedOffsetTable | ( | Uint64 *& | value,
|  | unsigned long * | count = `NULL`
| ) |  | const
| virtual

get ExtendedOffsetTable (7fe0,0001)

Parameters

  value | reference to variable in which the value should be stored
  count | stores number of items in the result array (if not NULL)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getExtendedOffsetTableLengths()

virtual OFCondition DRTImageIOD::getExtendedOffsetTableLengths | ( | Uint64 *& | value,
|  | unsigned long * | count = `NULL`
| ) |  | const
| virtual

get ExtendedOffsetTableLengths (7fe0,0002)

Parameters

  value | reference to variable in which the value should be stored
  count | stores number of items in the result array (if not NULL)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFluenceMapSequence() [1/2]

DRTFluenceMapSequence& DRTImageIOD::getFluenceMapSequence | ( |  | ) |
| inline

get FluenceMapSequence (3002,0040)

Returns
  reference to sequence element

## ◆ getFluenceMapSequence() [2/2]

const DRTFluenceMapSequence& DRTImageIOD::getFluenceMapSequence | ( |  | ) | const
| inline

get FluenceMapSequence (3002,0040)

Returns
  const reference to sequence element

## ◆ getFractionNumber() [1/2]

virtual OFCondition DRTImageIOD::getFractionNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get FractionNumber (3002,0029)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFractionNumber() [2/2]

virtual OFCondition DRTImageIOD::getFractionNumber | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get FractionNumber (3002,0029)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameDelay() [1/2]

virtual OFCondition DRTImageIOD::getFrameDelay | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get FrameDelay (0018,1066)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameDelay() [2/2]

virtual OFCondition DRTImageIOD::getFrameDelay | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get FrameDelay (0018,1066)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameExtractionSequence() [1/2]

DRTFrameExtractionSequence& DRTImageIOD::getFrameExtractionSequence | ( |  | ) |
| inline

get FrameExtractionSequence (0008,1164)

Returns
  reference to sequence element

## ◆ getFrameExtractionSequence() [2/2]

const DRTFrameExtractionSequence& DRTImageIOD::getFrameExtractionSequence | ( |  | ) | const
| inline

get FrameExtractionSequence (0008,1164)

Returns
  const reference to sequence element

## ◆ getFrameIncrementPointer()

virtual OFCondition DRTImageIOD::getFrameIncrementPointer | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get FrameIncrementPointer (0028,0009)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameOfReferenceUID()

virtual OFCondition DRTImageIOD::getFrameOfReferenceUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get FrameOfReferenceUID (0020,0052)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameTime() [1/2]

virtual OFCondition DRTImageIOD::getFrameTime | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get FrameTime (0018,1063)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameTime() [2/2]

virtual OFCondition DRTImageIOD::getFrameTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get FrameTime (0018,1063)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameTimeVector() [1/3]

virtual OFCondition DRTImageIOD::getFrameTimeVector | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get FrameTimeVector (0018,1065)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameTimeVector() [2/3]

virtual OFCondition DRTImageIOD::getFrameTimeVector | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get FrameTimeVector (0018,1065)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getFrameTimeVector() [3/3]

virtual OFCondition DRTImageIOD::getFrameTimeVector | ( | OFVector< Float64 > & | value | ) | const
| virtual

get FrameTimeVector (0018,1065)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getGantryAngle() [1/2]

virtual OFCondition DRTImageIOD::getGantryAngle | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get GantryAngle (300a,011e)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getGantryAngle() [2/2]

virtual OFCondition DRTImageIOD::getGantryAngle | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get GantryAngle (300a,011e)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getGantryID()

virtual OFCondition DRTImageIOD::getGantryID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get GantryID (0018,1008)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getGantryPitchAngle()

virtual OFCondition DRTImageIOD::getGantryPitchAngle | ( | Float32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get GantryPitchAngle (300a,014a)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getGeneticModificationsSequence() [1/2]

DRTGeneticModificationsSequence& DRTImageIOD::getGeneticModificationsSequence | ( |  | ) |
| inline

get GeneticModificationsSequence (0010,0221)

Returns
  reference to sequence element

## ◆ getGeneticModificationsSequence() [2/2]

const DRTGeneticModificationsSequence& DRTImageIOD::getGeneticModificationsSequence | ( |  | ) | const
| inline

get GeneticModificationsSequence (0010,0221)

Returns
  const reference to sequence element

## ◆ getGreenPaletteColorLookupTableData()

virtual OFCondition DRTImageIOD::getGreenPaletteColorLookupTableData | ( | Uint16 *& | value,
|  | unsigned long * | count = `NULL`
| ) |  | const
| virtual

get GreenPaletteColorLookupTableData (0028,1202)

Parameters

  value | reference to variable in which the value should be stored
  count | stores number of items in the result array (if not NULL)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getGreenPaletteColorLookupTableDescriptor()

virtual OFCondition DRTImageIOD::getGreenPaletteColorLookupTableDescriptor | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get GreenPaletteColorLookupTableDescriptor (0028,1102)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getGroupOfPatientsIdentificationSequence() [1/2]

DRTGroupOfPatientsIdentificationSequence& DRTImageIOD::getGroupOfPatientsIdentificationSequence | ( |  | ) |
| inline

get GroupOfPatientsIdentificationSequence (0010,0027)

Returns
  reference to sequence element

## ◆ getGroupOfPatientsIdentificationSequence() [2/2]

const DRTGroupOfPatientsIdentificationSequence& DRTImageIOD::getGroupOfPatientsIdentificationSequence | ( |  | ) | const
| inline

get GroupOfPatientsIdentificationSequence (0010,0027)

Returns
  const reference to sequence element

## ◆ getHighBit()

virtual OFCondition DRTImageIOD::getHighBit | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get HighBit (0028,0102)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getHL7StructuredDocumentReferenceSequence() [1/2]

DRTHL7StructuredDocumentReferenceSequence& DRTImageIOD::getHL7StructuredDocumentReferenceSequence | ( |  | ) |
| inline

get HL7StructuredDocumentReferenceSequence (0040,a390)

Returns
  reference to sequence element

## ◆ getHL7StructuredDocumentReferenceSequence() [2/2]

const DRTHL7StructuredDocumentReferenceSequence& DRTImageIOD::getHL7StructuredDocumentReferenceSequence | ( |  | ) | const
| inline

get HL7StructuredDocumentReferenceSequence (0040,a390)

Returns
  const reference to sequence element

## ◆ getICCProfile()

virtual OFCondition DRTImageIOD::getICCProfile | ( | Uint8 *& | value,
|  | unsigned long * | count = `NULL`
| ) |  | const
| virtual

get ICCProfile (0028,2000)

Parameters

  value | reference to variable in which the value should be stored
  count | stores number of items in the result array (if not NULL)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getIconImageSequence() [1/2]

DRTIconImageSequence& DRTImageIOD::getIconImageSequence | ( |  | ) |
| inline

get IconImageSequence (0088,0200)

Returns
  reference to sequence element

## ◆ getIconImageSequence() [2/2]

const DRTIconImageSequence& DRTImageIOD::getIconImageSequence | ( |  | ) | const
| inline

get IconImageSequence (0088,0200)

Returns
  const reference to sequence element

## ◆ getImageComments()

virtual OFCondition DRTImageIOD::getImageComments | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ImageComments (0020,4000)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImageLaterality()

virtual OFCondition DRTImageIOD::getImageLaterality | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ImageLaterality (0020,0062)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImagePlanePixelSpacing() [1/3]

virtual OFCondition DRTImageIOD::getImagePlanePixelSpacing | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ImagePlanePixelSpacing (3002,0011)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImagePlanePixelSpacing() [2/3]

virtual OFCondition DRTImageIOD::getImagePlanePixelSpacing | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ImagePlanePixelSpacing (3002,0011)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImagePlanePixelSpacing() [3/3]

virtual OFCondition DRTImageIOD::getImagePlanePixelSpacing | ( | OFVector< Float64 > & | value | ) | const
| virtual

get ImagePlanePixelSpacing (3002,0011)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImagesInAcquisition() [1/2]

virtual OFCondition DRTImageIOD::getImagesInAcquisition | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ImagesInAcquisition (0020,1002)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImagesInAcquisition() [2/2]

virtual OFCondition DRTImageIOD::getImagesInAcquisition | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ImagesInAcquisition (0020,1002)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImageTriggerDelay() [1/2]

virtual OFCondition DRTImageIOD::getImageTriggerDelay | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ImageTriggerDelay (0018,1067)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImageTriggerDelay() [2/2]

virtual OFCondition DRTImageIOD::getImageTriggerDelay | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ImageTriggerDelay (0018,1067)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getImageType()

virtual OFCondition DRTImageIOD::getImageType | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ImageType (0008,0008)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstanceCoercionDateTime()

virtual OFCondition DRTImageIOD::getInstanceCoercionDateTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstanceCoercionDateTime (0008,0015)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstanceCreationDate()

virtual OFCondition DRTImageIOD::getInstanceCreationDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstanceCreationDate (0008,0012)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstanceCreationTime()

virtual OFCondition DRTImageIOD::getInstanceCreationTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstanceCreationTime (0008,0013)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstanceCreatorUID()

virtual OFCondition DRTImageIOD::getInstanceCreatorUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstanceCreatorUID (0008,0014)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstanceNumber() [1/2]

virtual OFCondition DRTImageIOD::getInstanceNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstanceNumber (0020,0013)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstanceNumber() [2/2]

virtual OFCondition DRTImageIOD::getInstanceNumber | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get InstanceNumber (0020,0013)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstanceOriginStatus()

virtual OFCondition DRTImageIOD::getInstanceOriginStatus | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstanceOriginStatus (0400,0600)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstitutionAddress()

virtual OFCondition DRTImageIOD::getInstitutionAddress | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstitutionAddress (0008,0081)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstitutionalDepartmentName()

virtual OFCondition DRTImageIOD::getInstitutionalDepartmentName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstitutionalDepartmentName (0008,1040)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getInstitutionalDepartmentTypeCodeSequence() [1/2]

DRTInstitutionalDepartmentTypeCodeSequence& DRTImageIOD::getInstitutionalDepartmentTypeCodeSequence | ( |  | ) |
| inline

get InstitutionalDepartmentTypeCodeSequence (0008,1041)

Returns
  reference to sequence element

## ◆ getInstitutionalDepartmentTypeCodeSequence() [2/2]

const DRTInstitutionalDepartmentTypeCodeSequence& DRTImageIOD::getInstitutionalDepartmentTypeCodeSequence | ( |  | ) | const
| inline

get InstitutionalDepartmentTypeCodeSequence (0008,1041)

Returns
  const reference to sequence element

## ◆ getInstitutionName()

virtual OFCondition DRTImageIOD::getInstitutionName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get InstitutionName (0008,0080)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getIrradiationEventUID()

virtual OFCondition DRTImageIOD::getIrradiationEventUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get IrradiationEventUID (0008,3010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getIsocenterPosition() [1/3]

virtual OFCondition DRTImageIOD::getIsocenterPosition | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get IsocenterPosition (300a,012c)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getIsocenterPosition() [2/3]

virtual OFCondition DRTImageIOD::getIsocenterPosition | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get IsocenterPosition (300a,012c)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getIsocenterPosition() [3/3]

virtual OFCondition DRTImageIOD::getIsocenterPosition | ( | OFVector< Float64 > & | value | ) | const
| virtual

get IsocenterPosition (300a,012c)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getIssuerOfAccessionNumberSequence() [1/2]

DRTIssuerOfAccessionNumberSequence& DRTImageIOD::getIssuerOfAccessionNumberSequence | ( |  | ) |
| inline

get IssuerOfAccessionNumberSequence (0008,0051)

Returns
  reference to sequence element

## ◆ getIssuerOfAccessionNumberSequence() [2/2]

const DRTIssuerOfAccessionNumberSequence& DRTImageIOD::getIssuerOfAccessionNumberSequence | ( |  | ) | const
| inline

get IssuerOfAccessionNumberSequence (0008,0051)

Returns
  const reference to sequence element

## ◆ getIssuerOfAdmissionIDSequence() [1/2]

DRTIssuerOfAdmissionIDSequence& DRTImageIOD::getIssuerOfAdmissionIDSequence | ( |  | ) |
| inline

get IssuerOfAdmissionIDSequence (0038,0014)

Returns
  reference to sequence element

## ◆ getIssuerOfAdmissionIDSequence() [2/2]

const DRTIssuerOfAdmissionIDSequence& DRTImageIOD::getIssuerOfAdmissionIDSequence | ( |  | ) | const
| inline

get IssuerOfAdmissionIDSequence (0038,0014)

Returns
  const reference to sequence element

## ◆ getIssuerOfPatientID()

virtual OFCondition DRTImageIOD::getIssuerOfPatientID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get IssuerOfPatientID (0010,0021)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getIssuerOfPatientIDQualifiersSequence() [1/2]

DRTIssuerOfPatientIDQualifiersSequence& DRTImageIOD::getIssuerOfPatientIDQualifiersSequence | ( |  | ) |
| inline

get IssuerOfPatientIDQualifiersSequence (0010,0024)

Returns
  reference to sequence element

## ◆ getIssuerOfPatientIDQualifiersSequence() [2/2]

const DRTIssuerOfPatientIDQualifiersSequence& DRTImageIOD::getIssuerOfPatientIDQualifiersSequence | ( |  | ) | const
| inline

get IssuerOfPatientIDQualifiersSequence (0010,0024)

Returns
  const reference to sequence element

## ◆ getIssuerOfServiceEpisodeIDSequence() [1/2]

DRTIssuerOfServiceEpisodeIDSequence& DRTImageIOD::getIssuerOfServiceEpisodeIDSequence | ( |  | ) |
| inline

get IssuerOfServiceEpisodeIDSequence (0038,0064)

Returns
  reference to sequence element

## ◆ getIssuerOfServiceEpisodeIDSequence() [2/2]

const DRTIssuerOfServiceEpisodeIDSequence& DRTImageIOD::getIssuerOfServiceEpisodeIDSequence | ( |  | ) | const
| inline

get IssuerOfServiceEpisodeIDSequence (0038,0064)

Returns
  const reference to sequence element

## ◆ getLargestImagePixelValue()

virtual OFCondition DRTImageIOD::getLargestImagePixelValue | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get LargestImagePixelValue (0028,0107)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLastMenstrualDate()

virtual OFCondition DRTImageIOD::getLastMenstrualDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get LastMenstrualDate (0010,21d0)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLongitudinalTemporalEventType()

virtual OFCondition DRTImageIOD::getLongitudinalTemporalEventType | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get LongitudinalTemporalEventType (0012,0053)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLongitudinalTemporalInformationModified()

virtual OFCondition DRTImageIOD::getLongitudinalTemporalInformationModified | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get LongitudinalTemporalInformationModified (0028,0303)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLongitudinalTemporalOffsetFromEvent()

virtual OFCondition DRTImageIOD::getLongitudinalTemporalOffsetFromEvent | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get LongitudinalTemporalOffsetFromEvent (0012,0052)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLossyImageCompression()

virtual OFCondition DRTImageIOD::getLossyImageCompression | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get LossyImageCompression (0028,2110)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLossyImageCompressionMethod()

virtual OFCondition DRTImageIOD::getLossyImageCompressionMethod | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get LossyImageCompressionMethod (0028,2114)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLossyImageCompressionRatio() [1/3]

virtual OFCondition DRTImageIOD::getLossyImageCompressionRatio | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get LossyImageCompressionRatio (0028,2112)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLossyImageCompressionRatio() [2/3]

virtual OFCondition DRTImageIOD::getLossyImageCompressionRatio | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get LossyImageCompressionRatio (0028,2112)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getLossyImageCompressionRatio() [3/3]

virtual OFCondition DRTImageIOD::getLossyImageCompressionRatio | ( | OFVector< Float64 > & | value | ) | const
| virtual

get LossyImageCompressionRatio (0028,2112)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getMACParametersSequence() [1/2]

DRTMACParametersSequence& DRTImageIOD::getMACParametersSequence | ( |  | ) |
| inline

get MACParametersSequence (4ffe,0001)

Returns
  reference to sequence element

## ◆ getMACParametersSequence() [2/2]

const DRTMACParametersSequence& DRTImageIOD::getMACParametersSequence | ( |  | ) | const
| inline

get MACParametersSequence (4ffe,0001)

Returns
  const reference to sequence element

## ◆ getManufacturer()

virtual OFCondition DRTImageIOD::getManufacturer | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get Manufacturer (0008,0070)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getManufacturerDeviceClassUID()

virtual OFCondition DRTImageIOD::getManufacturerDeviceClassUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ManufacturerDeviceClassUID (0018,100b)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getManufacturerModelName()

virtual OFCondition DRTImageIOD::getManufacturerModelName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ManufacturerModelName (0008,1090)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getMappingResourceIdentificationSequence() [1/2]

DRTMappingResourceIdentificationSequence& DRTImageIOD::getMappingResourceIdentificationSequence | ( |  | ) |
| inline

get MappingResourceIdentificationSequence (0008,0124)

Returns
  reference to sequence element

## ◆ getMappingResourceIdentificationSequence() [2/2]

const DRTMappingResourceIdentificationSequence& DRTImageIOD::getMappingResourceIdentificationSequence | ( |  | ) | const
| inline

get MappingResourceIdentificationSequence (0008,0124)

Returns
  const reference to sequence element

## ◆ getMeasuredAPDimension() [1/2]

virtual OFCondition DRTImageIOD::getMeasuredAPDimension | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get MeasuredAPDimension (0010,1023)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getMeasuredAPDimension() [2/2]

virtual OFCondition DRTImageIOD::getMeasuredAPDimension | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get MeasuredAPDimension (0010,1023)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getMeasuredLateralDimension() [1/2]

virtual OFCondition DRTImageIOD::getMeasuredLateralDimension | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get MeasuredLateralDimension (0010,1024)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getMeasuredLateralDimension() [2/2]

virtual OFCondition DRTImageIOD::getMeasuredLateralDimension | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get MeasuredLateralDimension (0010,1024)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getMedicalAlerts()

virtual OFCondition DRTImageIOD::getMedicalAlerts | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get MedicalAlerts (0010,2000)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getMetersetExposure() [1/2]

virtual OFCondition DRTImageIOD::getMetersetExposure | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get MetersetExposure (3002,0032)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getMetersetExposure() [2/2]

virtual OFCondition DRTImageIOD::getMetersetExposure | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get MetersetExposure (3002,0032)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getModality()

virtual OFCondition DRTImageIOD::getModality | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get Modality (0008,0060)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getModalityLUTSequence() [1/2]

DRTModalityLUTSequence& DRTImageIOD::getModalityLUTSequence | ( |  | ) |
| inline

get ModalityLUTSequence (0028,3000)

Returns
  reference to sequence element

## ◆ getModalityLUTSequence() [2/2]

const DRTModalityLUTSequence& DRTImageIOD::getModalityLUTSequence | ( |  | ) | const
| inline

get ModalityLUTSequence (0028,3000)

Returns
  const reference to sequence element

## ◆ getMultiplexedAudioChannelsDescriptionCodeSequence() [1/2]

DRTMultiplexedAudioChannelsDescriptionCodeSequence& DRTImageIOD::getMultiplexedAudioChannelsDescriptionCodeSequence | ( |  | ) |
| inline

get MultiplexedAudioChannelsDescriptionCodeSequence (003a,0300)

Returns
  reference to sequence element

## ◆ getMultiplexedAudioChannelsDescriptionCodeSequence() [2/2]

const DRTMultiplexedAudioChannelsDescriptionCodeSequence& DRTImageIOD::getMultiplexedAudioChannelsDescriptionCodeSequence | ( |  | ) | const
| inline

get MultiplexedAudioChannelsDescriptionCodeSequence (003a,0300)

Returns
  const reference to sequence element

## ◆ getNameOfPhysiciansReadingStudy()

virtual OFCondition DRTImageIOD::getNameOfPhysiciansReadingStudy | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get NameOfPhysiciansReadingStudy (0008,1060)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getNumberOfFrames() [1/2]

virtual OFCondition DRTImageIOD::getNumberOfFrames | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get NumberOfFrames (0028,0008)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getNumberOfFrames() [2/2]

virtual OFCondition DRTImageIOD::getNumberOfFrames | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get NumberOfFrames (0028,0008)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getOccupation()

virtual OFCondition DRTImageIOD::getOccupation | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get Occupation (0010,2180)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getOperatorIdentificationSequence() [1/2]

DRTOperatorIdentificationSequence& DRTImageIOD::getOperatorIdentificationSequence | ( |  | ) |
| inline

get OperatorIdentificationSequence (0008,1072)

Returns
  reference to sequence element

## ◆ getOperatorIdentificationSequence() [2/2]

const DRTOperatorIdentificationSequence& DRTImageIOD::getOperatorIdentificationSequence | ( |  | ) | const
| inline

get OperatorIdentificationSequence (0008,1072)

Returns
  const reference to sequence element

## ◆ getOperatorsName()

virtual OFCondition DRTImageIOD::getOperatorsName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get OperatorsName (0008,1070)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getOriginalAttributesSequence() [1/2]

DRTOriginalAttributesSequence& DRTImageIOD::getOriginalAttributesSequence | ( |  | ) |
| inline

get OriginalAttributesSequence (0400,0561)

Returns
  reference to sequence element

## ◆ getOriginalAttributesSequence() [2/2]

const DRTOriginalAttributesSequence& DRTImageIOD::getOriginalAttributesSequence | ( |  | ) | const
| inline

get OriginalAttributesSequence (0400,0561)

Returns
  const reference to sequence element

## ◆ getOriginalSpecializedSOPClassUID()

virtual OFCondition DRTImageIOD::getOriginalSpecializedSOPClassUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get OriginalSpecializedSOPClassUID (0008,001b)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getOtherPatientIDsSequence() [1/2]

DRTOtherPatientIDsSequence& DRTImageIOD::getOtherPatientIDsSequence | ( |  | ) |
| inline

get OtherPatientIDsSequence (0010,1002)

Returns
  reference to sequence element

## ◆ getOtherPatientIDsSequence() [2/2]

const DRTOtherPatientIDsSequence& DRTImageIOD::getOtherPatientIDsSequence | ( |  | ) | const
| inline

get OtherPatientIDsSequence (0010,1002)

Returns
  const reference to sequence element

## ◆ getOtherPatientNames()

virtual OFCondition DRTImageIOD::getOtherPatientNames | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get OtherPatientNames (0010,1001)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientAge()

virtual OFCondition DRTImageIOD::getPatientAge | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientAge (0010,1010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientAlternativeCalendar()

virtual OFCondition DRTImageIOD::getPatientAlternativeCalendar | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientAlternativeCalendar (0010,0035)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientBirthDate()

virtual OFCondition DRTImageIOD::getPatientBirthDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientBirthDate (0010,0030)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientBirthDateInAlternativeCalendar()

virtual OFCondition DRTImageIOD::getPatientBirthDateInAlternativeCalendar | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientBirthDateInAlternativeCalendar (0010,0033)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientBirthTime()

virtual OFCondition DRTImageIOD::getPatientBirthTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientBirthTime (0010,0032)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientBodyMassIndex() [1/2]

virtual OFCondition DRTImageIOD::getPatientBodyMassIndex | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PatientBodyMassIndex (0010,1022)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientBodyMassIndex() [2/2]

virtual OFCondition DRTImageIOD::getPatientBodyMassIndex | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientBodyMassIndex (0010,1022)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientBreedCodeSequence() [1/2]

DRTPatientBreedCodeSequence& DRTImageIOD::getPatientBreedCodeSequence | ( |  | ) |
| inline

get PatientBreedCodeSequence (0010,2293)

Returns
  reference to sequence element

## ◆ getPatientBreedCodeSequence() [2/2]

const DRTPatientBreedCodeSequence& DRTImageIOD::getPatientBreedCodeSequence | ( |  | ) | const
| inline

get PatientBreedCodeSequence (0010,2293)

Returns
  const reference to sequence element

## ◆ getPatientBreedDescription()

virtual OFCondition DRTImageIOD::getPatientBreedDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientBreedDescription (0010,2292)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientComments()

virtual OFCondition DRTImageIOD::getPatientComments | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientComments (0010,4000)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientDeathDateInAlternativeCalendar()

virtual OFCondition DRTImageIOD::getPatientDeathDateInAlternativeCalendar | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientDeathDateInAlternativeCalendar (0010,0034)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientID()

virtual OFCondition DRTImageIOD::getPatientID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientID (0010,0020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientIdentityRemoved()

virtual OFCondition DRTImageIOD::getPatientIdentityRemoved | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientIdentityRemoved (0012,0062)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientName()

virtual OFCondition DRTImageIOD::getPatientName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientName (0010,0010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientOrientation()

virtual OFCondition DRTImageIOD::getPatientOrientation | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientOrientation (0020,0020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientPosition()

virtual OFCondition DRTImageIOD::getPatientPosition | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientPosition (0018,5100)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientSex()

virtual OFCondition DRTImageIOD::getPatientSex | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientSex (0010,0040)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientSexNeutered()

virtual OFCondition DRTImageIOD::getPatientSexNeutered | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientSexNeutered (0010,2203)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientSize() [1/2]

virtual OFCondition DRTImageIOD::getPatientSize | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PatientSize (0010,1020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientSize() [2/2]

virtual OFCondition DRTImageIOD::getPatientSize | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientSize (0010,1020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientSizeCodeSequence() [1/2]

DRTPatientSizeCodeSequence& DRTImageIOD::getPatientSizeCodeSequence | ( |  | ) |
| inline

get PatientSizeCodeSequence (0010,1021)

Returns
  reference to sequence element

## ◆ getPatientSizeCodeSequence() [2/2]

const DRTPatientSizeCodeSequence& DRTImageIOD::getPatientSizeCodeSequence | ( |  | ) | const
| inline

get PatientSizeCodeSequence (0010,1021)

Returns
  const reference to sequence element

## ◆ getPatientSpeciesCodeSequence() [1/2]

DRTPatientSpeciesCodeSequence& DRTImageIOD::getPatientSpeciesCodeSequence | ( |  | ) |
| inline

get PatientSpeciesCodeSequence (0010,2202)

Returns
  reference to sequence element

## ◆ getPatientSpeciesCodeSequence() [2/2]

const DRTPatientSpeciesCodeSequence& DRTImageIOD::getPatientSpeciesCodeSequence | ( |  | ) | const
| inline

get PatientSpeciesCodeSequence (0010,2202)

Returns
  const reference to sequence element

## ◆ getPatientSpeciesDescription()

virtual OFCondition DRTImageIOD::getPatientSpeciesDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientSpeciesDescription (0010,2201)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientState()

virtual OFCondition DRTImageIOD::getPatientState | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientState (0038,0500)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientSupportAngle() [1/2]

virtual OFCondition DRTImageIOD::getPatientSupportAngle | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PatientSupportAngle (300a,0122)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientSupportAngle() [2/2]

virtual OFCondition DRTImageIOD::getPatientSupportAngle | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientSupportAngle (300a,0122)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientWeight() [1/2]

virtual OFCondition DRTImageIOD::getPatientWeight | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PatientWeight (0010,1030)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPatientWeight() [2/2]

virtual OFCondition DRTImageIOD::getPatientWeight | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PatientWeight (0010,1030)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPerformedProcedureStepDescription()

virtual OFCondition DRTImageIOD::getPerformedProcedureStepDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PerformedProcedureStepDescription (0040,0254)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPerformedProcedureStepEndDate()

virtual OFCondition DRTImageIOD::getPerformedProcedureStepEndDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PerformedProcedureStepEndDate (0040,0250)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPerformedProcedureStepEndTime()

virtual OFCondition DRTImageIOD::getPerformedProcedureStepEndTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PerformedProcedureStepEndTime (0040,0251)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPerformedProcedureStepID()

virtual OFCondition DRTImageIOD::getPerformedProcedureStepID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PerformedProcedureStepID (0040,0253)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPerformedProcedureStepStartDate()

virtual OFCondition DRTImageIOD::getPerformedProcedureStepStartDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PerformedProcedureStepStartDate (0040,0244)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPerformedProcedureStepStartTime()

virtual OFCondition DRTImageIOD::getPerformedProcedureStepStartTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PerformedProcedureStepStartTime (0040,0245)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPerformedProtocolCodeSequence() [1/2]

DRTPerformedProtocolCodeSequence& DRTImageIOD::getPerformedProtocolCodeSequence | ( |  | ) |
| inline

get PerformedProtocolCodeSequence (0040,0260)

Returns
  reference to sequence element

## ◆ getPerformedProtocolCodeSequence() [2/2]

const DRTPerformedProtocolCodeSequence& DRTImageIOD::getPerformedProtocolCodeSequence | ( |  | ) | const
| inline

get PerformedProtocolCodeSequence (0040,0260)

Returns
  const reference to sequence element

## ◆ getPhotometricInterpretation()

virtual OFCondition DRTImageIOD::getPhotometricInterpretation | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PhotometricInterpretation (0028,0004)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPhysiciansOfRecord()

virtual OFCondition DRTImageIOD::getPhysiciansOfRecord | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PhysiciansOfRecord (0008,1048)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPhysiciansOfRecordIdentificationSequence() [1/2]

DRTPhysiciansOfRecordIdentificationSequence& DRTImageIOD::getPhysiciansOfRecordIdentificationSequence | ( |  | ) |
| inline

get PhysiciansOfRecordIdentificationSequence (0008,1049)

Returns
  reference to sequence element

## ◆ getPhysiciansOfRecordIdentificationSequence() [2/2]

const DRTPhysiciansOfRecordIdentificationSequence& DRTImageIOD::getPhysiciansOfRecordIdentificationSequence | ( |  | ) | const
| inline

get PhysiciansOfRecordIdentificationSequence (0008,1049)

Returns
  const reference to sequence element

## ◆ getPhysiciansReadingStudyIdentificationSequence() [1/2]

DRTPhysiciansReadingStudyIdentificationSequence& DRTImageIOD::getPhysiciansReadingStudyIdentificationSequence | ( |  | ) |
| inline

get PhysiciansReadingStudyIdentificationSequence (0008,1062)

Returns
  reference to sequence element

## ◆ getPhysiciansReadingStudyIdentificationSequence() [2/2]

const DRTPhysiciansReadingStudyIdentificationSequence& DRTImageIOD::getPhysiciansReadingStudyIdentificationSequence | ( |  | ) | const
| inline

get PhysiciansReadingStudyIdentificationSequence (0008,1062)

Returns
  const reference to sequence element

## ◆ getPixelAspectRatio() [1/2]

virtual OFCondition DRTImageIOD::getPixelAspectRatio | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PixelAspectRatio (0028,0034)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPixelAspectRatio() [2/2]

virtual OFCondition DRTImageIOD::getPixelAspectRatio | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PixelAspectRatio (0028,0034)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPixelData() [1/2]

DcmPixelData& DRTImageIOD::getPixelData | ( |  | ) |
| inline

get PixelData (7fe0,0010)

Returns
  reference to pixel data element

## ◆ getPixelData() [2/2]

const DcmPixelData& DRTImageIOD::getPixelData | ( |  | ) | const
| inline

get PixelData (7fe0,0010)

Returns
  const reference to pixel data element

## ◆ getPixelDataProviderURL()

virtual OFCondition DRTImageIOD::getPixelDataProviderURL | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PixelDataProviderURL (0028,7fe0)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPixelIntensityRelationship()

virtual OFCondition DRTImageIOD::getPixelIntensityRelationship | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PixelIntensityRelationship (0028,1040)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPixelIntensityRelationshipSign()

virtual OFCondition DRTImageIOD::getPixelIntensityRelationshipSign | ( | Sint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PixelIntensityRelationshipSign (0028,1041)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPixelPaddingRangeLimit()

virtual OFCondition DRTImageIOD::getPixelPaddingRangeLimit | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PixelPaddingRangeLimit (0028,0121)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPixelPaddingValue()

virtual OFCondition DRTImageIOD::getPixelPaddingValue | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PixelPaddingValue (0028,0120)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPixelRepresentation()

virtual OFCondition DRTImageIOD::getPixelRepresentation | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PixelRepresentation (0028,0103)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPlanarConfiguration()

virtual OFCondition DRTImageIOD::getPlanarConfiguration | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PlanarConfiguration (0028,0006)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPositionReferenceIndicator()

virtual OFCondition DRTImageIOD::getPositionReferenceIndicator | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PositionReferenceIndicator (0020,1040)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPreferredPlaybackSequencing()

virtual OFCondition DRTImageIOD::getPreferredPlaybackSequencing | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PreferredPlaybackSequencing (0018,1244)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPregnancyStatus()

virtual OFCondition DRTImageIOD::getPregnancyStatus | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get PregnancyStatus (0010,21c0)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPresentationLUTShape()

virtual OFCondition DRTImageIOD::getPresentationLUTShape | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PresentationLUTShape (2050,0020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPrimaryAnatomicStructureSequence() [1/2]

DRTPrimaryAnatomicStructureSequence& DRTImageIOD::getPrimaryAnatomicStructureSequence | ( |  | ) |
| inline

get PrimaryAnatomicStructureSequence (0008,2228)

Returns
  reference to sequence element

## ◆ getPrimaryAnatomicStructureSequence() [2/2]

const DRTPrimaryAnatomicStructureSequence& DRTImageIOD::getPrimaryAnatomicStructureSequence | ( |  | ) | const
| inline

get PrimaryAnatomicStructureSequence (0008,2228)

Returns
  const reference to sequence element

## ◆ getPrimaryDosimeterUnit()

virtual OFCondition DRTImageIOD::getPrimaryDosimeterUnit | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get PrimaryDosimeterUnit (300a,00b3)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getPrivateDataElementCharacteristicsSequence() [1/2]

DRTPrivateDataElementCharacteristicsSequence& DRTImageIOD::getPrivateDataElementCharacteristicsSequence | ( |  | ) |
| inline

get PrivateDataElementCharacteristicsSequence (0008,0300)

Returns
  reference to sequence element

## ◆ getPrivateDataElementCharacteristicsSequence() [2/2]

const DRTPrivateDataElementCharacteristicsSequence& DRTImageIOD::getPrivateDataElementCharacteristicsSequence | ( |  | ) | const
| inline

get PrivateDataElementCharacteristicsSequence (0008,0300)

Returns
  const reference to sequence element

## ◆ getProcedureCodeSequence() [1/2]

DRTProcedureCodeSequence& DRTImageIOD::getProcedureCodeSequence | ( |  | ) |
| inline

get ProcedureCodeSequence (0008,1032)

Returns
  reference to sequence element

## ◆ getProcedureCodeSequence() [2/2]

const DRTProcedureCodeSequence& DRTImageIOD::getProcedureCodeSequence | ( |  | ) | const
| inline

get ProcedureCodeSequence (0008,1032)

Returns
  const reference to sequence element

## ◆ getQualityControlImage()

virtual OFCondition DRTImageIOD::getQualityControlImage | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get QualityControlImage (0028,0300)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getQualityControlSubject()

virtual OFCondition DRTImageIOD::getQualityControlSubject | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get QualityControlSubject (0010,0200)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getQueryRetrieveView()

virtual OFCondition DRTImageIOD::getQueryRetrieveView | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get QueryRetrieveView (0008,0053)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRadiationMachineName()

virtual OFCondition DRTImageIOD::getRadiationMachineName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RadiationMachineName (3002,0020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRadiationMachineSAD() [1/2]

virtual OFCondition DRTImageIOD::getRadiationMachineSAD | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RadiationMachineSAD (3002,0022)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRadiationMachineSAD() [2/2]

virtual OFCondition DRTImageIOD::getRadiationMachineSAD | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RadiationMachineSAD (3002,0022)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRadiationMachineSSD() [1/2]

virtual OFCondition DRTImageIOD::getRadiationMachineSSD | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RadiationMachineSSD (3002,0024)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRadiationMachineSSD() [2/2]

virtual OFCondition DRTImageIOD::getRadiationMachineSSD | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RadiationMachineSSD (3002,0024)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRealWorldValueMappingSequence() [1/2]

DRTRealWorldValueMappingSequence& DRTImageIOD::getRealWorldValueMappingSequence | ( |  | ) |
| inline

get RealWorldValueMappingSequence (0040,9096)

Returns
  reference to sequence element

## ◆ getRealWorldValueMappingSequence() [2/2]

const DRTRealWorldValueMappingSequence& DRTImageIOD::getRealWorldValueMappingSequence | ( |  | ) | const
| inline

get RealWorldValueMappingSequence (0040,9096)

Returns
  const reference to sequence element

## ◆ getReasonForPerformedProcedureCodeSequence() [1/2]

DRTReasonForPerformedProcedureCodeSequence& DRTImageIOD::getReasonForPerformedProcedureCodeSequence | ( |  | ) |
| inline

get ReasonForPerformedProcedureCodeSequence (0040,1012)

Returns
  reference to sequence element

## ◆ getReasonForPerformedProcedureCodeSequence() [2/2]

const DRTReasonForPerformedProcedureCodeSequence& DRTImageIOD::getReasonForPerformedProcedureCodeSequence | ( |  | ) | const
| inline

get ReasonForPerformedProcedureCodeSequence (0040,1012)

Returns
  const reference to sequence element

## ◆ getReasonForVisit()

virtual OFCondition DRTImageIOD::getReasonForVisit | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ReasonForVisit (0032,1066)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReasonForVisitCodeSequence() [1/2]

DRTReasonForVisitCodeSequence& DRTImageIOD::getReasonForVisitCodeSequence | ( |  | ) |
| inline

get ReasonForVisitCodeSequence (0032,1067)

Returns
  reference to sequence element

## ◆ getReasonForVisitCodeSequence() [2/2]

const DRTReasonForVisitCodeSequence& DRTImageIOD::getReasonForVisitCodeSequence | ( |  | ) | const
| inline

get ReasonForVisitCodeSequence (0032,1067)

Returns
  const reference to sequence element

## ◆ getRecognizableVisualFeatures()

virtual OFCondition DRTImageIOD::getRecognizableVisualFeatures | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RecognizableVisualFeatures (0028,0302)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRecommendedDisplayFrameRate() [1/2]

virtual OFCondition DRTImageIOD::getRecommendedDisplayFrameRate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RecommendedDisplayFrameRate (0008,2144)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRecommendedDisplayFrameRate() [2/2]

virtual OFCondition DRTImageIOD::getRecommendedDisplayFrameRate | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RecommendedDisplayFrameRate (0008,2144)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRedPaletteColorLookupTableData()

virtual OFCondition DRTImageIOD::getRedPaletteColorLookupTableData | ( | Uint16 *& | value,
|  | unsigned long * | count = `NULL`
| ) |  | const
| virtual

get RedPaletteColorLookupTableData (0028,1201)

Parameters

  value | reference to variable in which the value should be stored
  count | stores number of items in the result array (if not NULL)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRedPaletteColorLookupTableDescriptor()

virtual OFCondition DRTImageIOD::getRedPaletteColorLookupTableDescriptor | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RedPaletteColorLookupTableDescriptor (0028,1101)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReferencedBeamNumber() [1/2]

virtual OFCondition DRTImageIOD::getReferencedBeamNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ReferencedBeamNumber (300c,0006)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReferencedBeamNumber() [2/2]

virtual OFCondition DRTImageIOD::getReferencedBeamNumber | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ReferencedBeamNumber (300c,0006)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReferencedDefinedProtocolSequence() [1/2]

DRTReferencedDefinedProtocolSequence& DRTImageIOD::getReferencedDefinedProtocolSequence | ( |  | ) |
| inline

get ReferencedDefinedProtocolSequence (0018,990c)

Returns
  reference to sequence element

## ◆ getReferencedDefinedProtocolSequence() [2/2]

const DRTReferencedDefinedProtocolSequence& DRTImageIOD::getReferencedDefinedProtocolSequence | ( |  | ) | const
| inline

get ReferencedDefinedProtocolSequence (0018,990c)

Returns
  const reference to sequence element

## ◆ getReferencedFractionGroupNumber() [1/2]

virtual OFCondition DRTImageIOD::getReferencedFractionGroupNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ReferencedFractionGroupNumber (300c,0022)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReferencedFractionGroupNumber() [2/2]

virtual OFCondition DRTImageIOD::getReferencedFractionGroupNumber | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get ReferencedFractionGroupNumber (300c,0022)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReferencedImageSequence() [1/2]

DRTReferencedImageSequence& DRTImageIOD::getReferencedImageSequence | ( |  | ) |
| inline

get ReferencedImageSequence (0008,1140)

Returns
  reference to sequence element

## ◆ getReferencedImageSequence() [2/2]

const DRTReferencedImageSequence& DRTImageIOD::getReferencedImageSequence | ( |  | ) | const
| inline

get ReferencedImageSequence (0008,1140)

Returns
  const reference to sequence element

## ◆ getReferencedInstanceSequence() [1/2]

DRTReferencedInstanceSequence& DRTImageIOD::getReferencedInstanceSequence | ( |  | ) |
| inline

get ReferencedInstanceSequence (0008,114a)

Returns
  reference to sequence element

## ◆ getReferencedInstanceSequence() [2/2]

const DRTReferencedInstanceSequence& DRTImageIOD::getReferencedInstanceSequence | ( |  | ) | const
| inline

get ReferencedInstanceSequence (0008,114a)

Returns
  const reference to sequence element

## ◆ getReferencedPatientPhotoSequence() [1/2]

DRTReferencedPatientPhotoSequence& DRTImageIOD::getReferencedPatientPhotoSequence | ( |  | ) |
| inline

get ReferencedPatientPhotoSequence (0010,1100)

Returns
  reference to sequence element

## ◆ getReferencedPatientPhotoSequence() [2/2]

const DRTReferencedPatientPhotoSequence& DRTImageIOD::getReferencedPatientPhotoSequence | ( |  | ) | const
| inline

get ReferencedPatientPhotoSequence (0010,1100)

Returns
  const reference to sequence element

## ◆ getReferencedPatientSequence() [1/2]

DRTReferencedPatientSequence& DRTImageIOD::getReferencedPatientSequence | ( |  | ) |
| inline

get ReferencedPatientSequence (0008,1120)

Returns
  reference to sequence element

## ◆ getReferencedPatientSequence() [2/2]

const DRTReferencedPatientSequence& DRTImageIOD::getReferencedPatientSequence | ( |  | ) | const
| inline

get ReferencedPatientSequence (0008,1120)

Returns
  const reference to sequence element

## ◆ getReferencedPerformedProcedureStepSequence() [1/2]

DRTReferencedPerformedProcedureStepSequence& DRTImageIOD::getReferencedPerformedProcedureStepSequence | ( |  | ) |
| inline

get ReferencedPerformedProcedureStepSequence (0008,1111)

Returns
  reference to sequence element

## ◆ getReferencedPerformedProcedureStepSequence() [2/2]

const DRTReferencedPerformedProcedureStepSequence& DRTImageIOD::getReferencedPerformedProcedureStepSequence | ( |  | ) | const
| inline

get ReferencedPerformedProcedureStepSequence (0008,1111)

Returns
  const reference to sequence element

## ◆ getReferencedPerformedProtocolSequence() [1/2]

DRTReferencedPerformedProtocolSequence& DRTImageIOD::getReferencedPerformedProtocolSequence | ( |  | ) |
| inline

get ReferencedPerformedProtocolSequence (0018,990d)

Returns
  reference to sequence element

## ◆ getReferencedPerformedProtocolSequence() [2/2]

const DRTReferencedPerformedProtocolSequence& DRTImageIOD::getReferencedPerformedProtocolSequence | ( |  | ) | const
| inline

get ReferencedPerformedProtocolSequence (0018,990d)

Returns
  const reference to sequence element

## ◆ getReferencedRTPlanSequence() [1/2]

DRTReferencedRTPlanSequenceInRTImageModule& DRTImageIOD::getReferencedRTPlanSequence | ( |  | ) |
| inline

get ReferencedRTPlanSequence (300c,0002)

Returns
  reference to sequence element

## ◆ getReferencedRTPlanSequence() [2/2]

const DRTReferencedRTPlanSequenceInRTImageModule& DRTImageIOD::getReferencedRTPlanSequence | ( |  | ) | const
| inline

get ReferencedRTPlanSequence (300c,0002)

Returns
  const reference to sequence element

## ◆ getReferencedSeriesSequence() [1/2]

DRTReferencedSeriesSequence& DRTImageIOD::getReferencedSeriesSequence | ( |  | ) |
| inline

get ReferencedSeriesSequence (0008,1115)

Returns
  reference to sequence element

## ◆ getReferencedSeriesSequence() [2/2]

const DRTReferencedSeriesSequence& DRTImageIOD::getReferencedSeriesSequence | ( |  | ) | const
| inline

get ReferencedSeriesSequence (0008,1115)

Returns
  const reference to sequence element

## ◆ getReferencedStudySequence() [1/2]

DRTReferencedStudySequence& DRTImageIOD::getReferencedStudySequence | ( |  | ) |
| inline

get ReferencedStudySequence (0008,1110)

Returns
  reference to sequence element

## ◆ getReferencedStudySequence() [2/2]

const DRTReferencedStudySequence& DRTImageIOD::getReferencedStudySequence | ( |  | ) | const
| inline

get ReferencedStudySequence (0008,1110)

Returns
  const reference to sequence element

## ◆ getReferringPhysicianIdentificationSequence() [1/2]

DRTReferringPhysicianIdentificationSequence& DRTImageIOD::getReferringPhysicianIdentificationSequence | ( |  | ) |
| inline

get ReferringPhysicianIdentificationSequence (0008,0096)

Returns
  reference to sequence element

## ◆ getReferringPhysicianIdentificationSequence() [2/2]

const DRTReferringPhysicianIdentificationSequence& DRTImageIOD::getReferringPhysicianIdentificationSequence | ( |  | ) | const
| inline

get ReferringPhysicianIdentificationSequence (0008,0096)

Returns
  const reference to sequence element

## ◆ getReferringPhysicianName()

virtual OFCondition DRTImageIOD::getReferringPhysicianName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ReferringPhysicianName (0008,0090)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRelatedGeneralSOPClassUID()

virtual OFCondition DRTImageIOD::getRelatedGeneralSOPClassUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RelatedGeneralSOPClassUID (0008,001a)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReportedValuesOrigin()

virtual OFCondition DRTImageIOD::getReportedValuesOrigin | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ReportedValuesOrigin (3002,000a)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRequestAttributesSequence() [1/2]

DRTRequestAttributesSequence& DRTImageIOD::getRequestAttributesSequence | ( |  | ) |
| inline

get RequestAttributesSequence (0040,0275)

Returns
  reference to sequence element

## ◆ getRequestAttributesSequence() [2/2]

const DRTRequestAttributesSequence& DRTImageIOD::getRequestAttributesSequence | ( |  | ) | const
| inline

get RequestAttributesSequence (0040,0275)

Returns
  const reference to sequence element

## ◆ getRequestingService()

virtual OFCondition DRTImageIOD::getRequestingService | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RequestingService (0032,1033)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRequestingServiceCodeSequence() [1/2]

DRTRequestingServiceCodeSequence& DRTImageIOD::getRequestingServiceCodeSequence | ( |  | ) |
| inline

get RequestingServiceCodeSequence (0032,1034)

Returns
  reference to sequence element

## ◆ getRequestingServiceCodeSequence() [2/2]

const DRTRequestingServiceCodeSequence& DRTImageIOD::getRequestingServiceCodeSequence | ( |  | ) | const
| inline

get RequestingServiceCodeSequence (0032,1034)

Returns
  const reference to sequence element

## ◆ getRescaleIntercept() [1/2]

virtual OFCondition DRTImageIOD::getRescaleIntercept | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RescaleIntercept (0028,1052)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRescaleIntercept() [2/2]

virtual OFCondition DRTImageIOD::getRescaleIntercept | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RescaleIntercept (0028,1052)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRescaleSlope() [1/2]

virtual OFCondition DRTImageIOD::getRescaleSlope | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RescaleSlope (0028,1053)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRescaleSlope() [2/2]

virtual OFCondition DRTImageIOD::getRescaleSlope | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RescaleSlope (0028,1053)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRescaleType()

virtual OFCondition DRTImageIOD::getRescaleType | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RescaleType (0028,1054)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getResponsibleOrganization()

virtual OFCondition DRTImageIOD::getResponsibleOrganization | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ResponsibleOrganization (0010,2299)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getResponsiblePerson()

virtual OFCondition DRTImageIOD::getResponsiblePerson | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ResponsiblePerson (0010,2297)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getResponsiblePersonRole()

virtual OFCondition DRTImageIOD::getResponsiblePersonRole | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ResponsiblePersonRole (0010,2298)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReviewDate()

virtual OFCondition DRTImageIOD::getReviewDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ReviewDate (300e,0004)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReviewerName()

virtual OFCondition DRTImageIOD::getReviewerName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ReviewerName (300e,0008)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getReviewTime()

virtual OFCondition DRTImageIOD::getReviewTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ReviewTime (300e,0005)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRows()

virtual OFCondition DRTImageIOD::getRows | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get Rows (0028,0010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImageDescription()

virtual OFCondition DRTImageIOD::getRTImageDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RTImageDescription (3002,0004)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImageLabel()

virtual OFCondition DRTImageIOD::getRTImageLabel | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RTImageLabel (3002,0002)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImageName()

virtual OFCondition DRTImageIOD::getRTImageName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RTImageName (3002,0003)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImageOrientation() [1/3]

virtual OFCondition DRTImageIOD::getRTImageOrientation | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RTImageOrientation (3002,0010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImageOrientation() [2/3]

virtual OFCondition DRTImageIOD::getRTImageOrientation | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RTImageOrientation (3002,0010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImageOrientation() [3/3]

virtual OFCondition DRTImageIOD::getRTImageOrientation | ( | OFVector< Float64 > & | value | ) | const
| virtual

get RTImageOrientation (3002,0010)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImagePlane()

virtual OFCondition DRTImageIOD::getRTImagePlane | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RTImagePlane (3002,000c)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImagePosition() [1/3]

virtual OFCondition DRTImageIOD::getRTImagePosition | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RTImagePosition (3002,0012)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImagePosition() [2/3]

virtual OFCondition DRTImageIOD::getRTImagePosition | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RTImagePosition (3002,0012)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImagePosition() [3/3]

virtual OFCondition DRTImageIOD::getRTImagePosition | ( | OFVector< Float64 > & | value | ) | const
| virtual

get RTImagePosition (3002,0012)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImageSID() [1/2]

virtual OFCondition DRTImageIOD::getRTImageSID | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get RTImageSID (3002,0026)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getRTImageSID() [2/2]

virtual OFCondition DRTImageIOD::getRTImageSID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get RTImageSID (3002,0026)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSamplesPerPixel()

virtual OFCondition DRTImageIOD::getSamplesPerPixel | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get SamplesPerPixel (0028,0002)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSeriesDate()

virtual OFCondition DRTImageIOD::getSeriesDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SeriesDate (0008,0021)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSeriesDescription()

virtual OFCondition DRTImageIOD::getSeriesDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SeriesDescription (0008,103e)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSeriesDescriptionCodeSequence() [1/2]

DRTSeriesDescriptionCodeSequence& DRTImageIOD::getSeriesDescriptionCodeSequence | ( |  | ) |
| inline

get SeriesDescriptionCodeSequence (0008,103f)

Returns
  reference to sequence element

## ◆ getSeriesDescriptionCodeSequence() [2/2]

const DRTSeriesDescriptionCodeSequence& DRTImageIOD::getSeriesDescriptionCodeSequence | ( |  | ) | const
| inline

get SeriesDescriptionCodeSequence (0008,103f)

Returns
  const reference to sequence element

## ◆ getSeriesInstanceUID()

virtual OFCondition DRTImageIOD::getSeriesInstanceUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SeriesInstanceUID (0020,000e)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSeriesNumber() [1/2]

virtual OFCondition DRTImageIOD::getSeriesNumber | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SeriesNumber (0020,0011)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSeriesNumber() [2/2]

virtual OFCondition DRTImageIOD::getSeriesNumber | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get SeriesNumber (0020,0011)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSeriesTime()

virtual OFCondition DRTImageIOD::getSeriesTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SeriesTime (0008,0031)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getServiceEpisodeDescription()

virtual OFCondition DRTImageIOD::getServiceEpisodeDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ServiceEpisodeDescription (0038,0062)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getServiceEpisodeID()

virtual OFCondition DRTImageIOD::getServiceEpisodeID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get ServiceEpisodeID (0038,0060)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSmallestImagePixelValue()

virtual OFCondition DRTImageIOD::getSmallestImagePixelValue | ( | Uint16 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get SmallestImagePixelValue (0028,0106)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSmokingStatus()

virtual OFCondition DRTImageIOD::getSmokingStatus | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SmokingStatus (0010,21a0)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSoftwareVersions()

virtual OFCondition DRTImageIOD::getSoftwareVersions | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SoftwareVersions (0018,1020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSOPAuthorizationComment()

virtual OFCondition DRTImageIOD::getSOPAuthorizationComment | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SOPAuthorizationComment (0100,0424)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSOPAuthorizationDateTime()

virtual OFCondition DRTImageIOD::getSOPAuthorizationDateTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SOPAuthorizationDateTime (0100,0420)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSOPClassUID()

virtual OFCondition DRTImageIOD::getSOPClassUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SOPClassUID (0008,0016)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSOPInstanceStatus()

virtual OFCondition DRTImageIOD::getSOPInstanceStatus | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SOPInstanceStatus (0100,0410)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSOPInstanceUID()

virtual OFCondition DRTImageIOD::getSOPInstanceUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SOPInstanceUID (0008,0018)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSourceImageSequence() [1/2]

DRTSourceImageSequence& DRTImageIOD::getSourceImageSequence | ( |  | ) |
| inline

get SourceImageSequence (0008,2112)

Returns
  reference to sequence element

## ◆ getSourceImageSequence() [2/2]

const DRTSourceImageSequence& DRTImageIOD::getSourceImageSequence | ( |  | ) | const
| inline

get SourceImageSequence (0008,2112)

Returns
  const reference to sequence element

## ◆ getSourceInstanceSequence() [1/2]

DRTSourceInstanceSequence& DRTImageIOD::getSourceInstanceSequence | ( |  | ) |
| inline

get SourceInstanceSequence (0042,0013)

Returns
  reference to sequence element

## ◆ getSourceInstanceSequence() [2/2]

const DRTSourceInstanceSequence& DRTImageIOD::getSourceInstanceSequence | ( |  | ) | const
| inline

get SourceInstanceSequence (0042,0013)

Returns
  const reference to sequence element

## ◆ getSourcePatientGroupIdentificationSequence() [1/2]

DRTSourcePatientGroupIdentificationSequence& DRTImageIOD::getSourcePatientGroupIdentificationSequence | ( |  | ) |
| inline

get SourcePatientGroupIdentificationSequence (0010,0026)

Returns
  reference to sequence element

## ◆ getSourcePatientGroupIdentificationSequence() [2/2]

const DRTSourcePatientGroupIdentificationSequence& DRTImageIOD::getSourcePatientGroupIdentificationSequence | ( |  | ) | const
| inline

get SourcePatientGroupIdentificationSequence (0010,0026)

Returns
  const reference to sequence element

## ◆ getSourceToReferenceObjectDistance() [1/2]

virtual OFCondition DRTImageIOD::getSourceToReferenceObjectDistance | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get SourceToReferenceObjectDistance (3002,0028)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSourceToReferenceObjectDistance() [2/2]

virtual OFCondition DRTImageIOD::getSourceToReferenceObjectDistance | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SourceToReferenceObjectDistance (3002,0028)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSpatialResolution() [1/2]

virtual OFCondition DRTImageIOD::getSpatialResolution | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get SpatialResolution (0018,1050)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSpatialResolution() [2/2]

virtual OFCondition DRTImageIOD::getSpatialResolution | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SpatialResolution (0018,1050)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getSpecificCharacterSet()

virtual OFCondition DRTImageIOD::getSpecificCharacterSet | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get SpecificCharacterSet (0008,0005)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStartCumulativeMetersetWeight() [1/2]

virtual OFCondition DRTImageIOD::getStartCumulativeMetersetWeight | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get StartCumulativeMetersetWeight (300c,0008)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStartCumulativeMetersetWeight() [2/2]

virtual OFCondition DRTImageIOD::getStartCumulativeMetersetWeight | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StartCumulativeMetersetWeight (300c,0008)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStartTrim() [1/2]

virtual OFCondition DRTImageIOD::getStartTrim | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StartTrim (0008,2142)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStartTrim() [2/2]

virtual OFCondition DRTImageIOD::getStartTrim | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get StartTrim (0008,2142)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStationName()

virtual OFCondition DRTImageIOD::getStationName | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StationName (0008,1010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStereoPairsPresent()

virtual OFCondition DRTImageIOD::getStereoPairsPresent | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StereoPairsPresent (0022,0028)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStopTrim() [1/2]

virtual OFCondition DRTImageIOD::getStopTrim | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StopTrim (0008,2143)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStopTrim() [2/2]

virtual OFCondition DRTImageIOD::getStopTrim | ( | Sint32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get StopTrim (0008,2143)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStrainAdditionalInformation()

virtual OFCondition DRTImageIOD::getStrainAdditionalInformation | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StrainAdditionalInformation (0010,0218)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStrainCodeSequence() [1/2]

DRTStrainCodeSequence& DRTImageIOD::getStrainCodeSequence | ( |  | ) |
| inline

get StrainCodeSequence (0010,0219)

Returns
  reference to sequence element

## ◆ getStrainCodeSequence() [2/2]

const DRTStrainCodeSequence& DRTImageIOD::getStrainCodeSequence | ( |  | ) | const
| inline

get StrainCodeSequence (0010,0219)

Returns
  const reference to sequence element

## ◆ getStrainDescription()

virtual OFCondition DRTImageIOD::getStrainDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StrainDescription (0010,0212)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStrainNomenclature()

virtual OFCondition DRTImageIOD::getStrainNomenclature | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StrainNomenclature (0010,0213)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStrainStockSequence() [1/2]

DRTStrainStockSequence& DRTImageIOD::getStrainStockSequence | ( |  | ) |
| inline

get StrainStockSequence (0010,0216)

Returns
  reference to sequence element

## ◆ getStrainStockSequence() [2/2]

const DRTStrainStockSequence& DRTImageIOD::getStrainStockSequence | ( |  | ) | const
| inline

get StrainStockSequence (0010,0216)

Returns
  const reference to sequence element

## ◆ getStudiesContainingOtherReferencedInstancesSequence() [1/2]

DRTStudiesContainingOtherReferencedInstancesSequence& DRTImageIOD::getStudiesContainingOtherReferencedInstancesSequence | ( |  | ) |
| inline

get StudiesContainingOtherReferencedInstancesSequence (0008,1200)

Returns
  reference to sequence element

## ◆ getStudiesContainingOtherReferencedInstancesSequence() [2/2]

const DRTStudiesContainingOtherReferencedInstancesSequence& DRTImageIOD::getStudiesContainingOtherReferencedInstancesSequence | ( |  | ) | const
| inline

get StudiesContainingOtherReferencedInstancesSequence (0008,1200)

Returns
  const reference to sequence element

## ◆ getStudyDate()

virtual OFCondition DRTImageIOD::getStudyDate | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StudyDate (0008,0020)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStudyDescription()

virtual OFCondition DRTImageIOD::getStudyDescription | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StudyDescription (0008,1030)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStudyID()

virtual OFCondition DRTImageIOD::getStudyID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StudyID (0020,0010)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStudyInstanceUID()

virtual OFCondition DRTImageIOD::getStudyInstanceUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StudyInstanceUID (0020,000d)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getStudyTime()

virtual OFCondition DRTImageIOD::getStudyTime | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get StudyTime (0008,0030)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopEccentricAngle() [1/2]

virtual OFCondition DRTImageIOD::getTableTopEccentricAngle | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get TableTopEccentricAngle (300a,0125)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopEccentricAngle() [2/2]

virtual OFCondition DRTImageIOD::getTableTopEccentricAngle | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TableTopEccentricAngle (300a,0125)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopEccentricAxisDistance() [1/2]

virtual OFCondition DRTImageIOD::getTableTopEccentricAxisDistance | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get TableTopEccentricAxisDistance (300a,0124)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopEccentricAxisDistance() [2/2]

virtual OFCondition DRTImageIOD::getTableTopEccentricAxisDistance | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TableTopEccentricAxisDistance (300a,0124)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopLateralPosition() [1/2]

virtual OFCondition DRTImageIOD::getTableTopLateralPosition | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get TableTopLateralPosition (300a,012a)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopLateralPosition() [2/2]

virtual OFCondition DRTImageIOD::getTableTopLateralPosition | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TableTopLateralPosition (300a,012a)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopLongitudinalPosition() [1/2]

virtual OFCondition DRTImageIOD::getTableTopLongitudinalPosition | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get TableTopLongitudinalPosition (300a,0129)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopLongitudinalPosition() [2/2]

virtual OFCondition DRTImageIOD::getTableTopLongitudinalPosition | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TableTopLongitudinalPosition (300a,0129)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopPitchAngle()

virtual OFCondition DRTImageIOD::getTableTopPitchAngle | ( | Float32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get TableTopPitchAngle (300a,0140)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopRollAngle()

virtual OFCondition DRTImageIOD::getTableTopRollAngle | ( | Float32 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get TableTopRollAngle (300a,0144)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopVerticalPosition() [1/2]

virtual OFCondition DRTImageIOD::getTableTopVerticalPosition | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get TableTopVerticalPosition (300a,0128)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTableTopVerticalPosition() [2/2]

virtual OFCondition DRTImageIOD::getTableTopVerticalPosition | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TableTopVerticalPosition (300a,0128)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTimeOfLastCalibration()

virtual OFCondition DRTImageIOD::getTimeOfLastCalibration | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TimeOfLastCalibration (0018,1201)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTimezoneOffsetFromUTC()

virtual OFCondition DRTImageIOD::getTimezoneOffsetFromUTC | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TimezoneOffsetFromUTC (0008,0201)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTreatmentSessionUID()

virtual OFCondition DRTImageIOD::getTreatmentSessionUID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TreatmentSessionUID (300a,0700)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getTypeOfPatientID()

virtual OFCondition DRTImageIOD::getTypeOfPatientID | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get TypeOfPatientID (0010,0022)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getUDISequence() [1/2]

DRTUDISequence& DRTImageIOD::getUDISequence | ( |  | ) |
| inline

get UDISequence (0018,100a)

Returns
  reference to sequence element

## ◆ getUDISequence() [2/2]

const DRTUDISequence& DRTImageIOD::getUDISequence | ( |  | ) | const
| inline

get UDISequence (0018,100a)

Returns
  const reference to sequence element

## ◆ getVOILUTFunction()

virtual OFCondition DRTImageIOD::getVOILUTFunction | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get VOILUTFunction (0028,1056)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getVOILUTSequence() [1/2]

DRTVOILUTSequence& DRTImageIOD::getVOILUTSequence | ( |  | ) |
| inline

get VOILUTSequence (0028,3010)

Returns
  reference to sequence element

## ◆ getVOILUTSequence() [2/2]

const DRTVOILUTSequence& DRTImageIOD::getVOILUTSequence | ( |  | ) | const
| inline

get VOILUTSequence (0028,3010)

Returns
  const reference to sequence element

## ◆ getWindowCenter() [1/3]

virtual OFCondition DRTImageIOD::getWindowCenter | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get WindowCenter (0028,1050)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getWindowCenter() [2/3]

virtual OFCondition DRTImageIOD::getWindowCenter | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get WindowCenter (0028,1050)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getWindowCenter() [3/3]

virtual OFCondition DRTImageIOD::getWindowCenter | ( | OFVector< Float64 > & | value | ) | const
| virtual

get WindowCenter (0028,1050)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getWindowCenterWidthExplanation()

virtual OFCondition DRTImageIOD::getWindowCenterWidthExplanation | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get WindowCenterWidthExplanation (0028,1055)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getWindowWidth() [1/3]

virtual OFCondition DRTImageIOD::getWindowWidth | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get WindowWidth (0028,1051)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getWindowWidth() [2/3]

virtual OFCondition DRTImageIOD::getWindowWidth | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get WindowWidth (0028,1051)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getWindowWidth() [3/3]

virtual OFCondition DRTImageIOD::getWindowWidth | ( | OFVector< Float64 > & | value | ) | const
| virtual

get WindowWidth (0028,1051)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getXRayImageReceptorAngle() [1/2]

virtual OFCondition DRTImageIOD::getXRayImageReceptorAngle | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get XRayImageReceptorAngle (3002,000e)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getXRayImageReceptorAngle() [2/2]

virtual OFCondition DRTImageIOD::getXRayImageReceptorAngle | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get XRayImageReceptorAngle (3002,000e)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getXRayImageReceptorTranslation() [1/3]

virtual OFCondition DRTImageIOD::getXRayImageReceptorTranslation | ( | Float64 & | value,
|  | const unsigned long | pos = `0`
| ) |  | const
| virtual

get XRayImageReceptorTranslation (3002,000d)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1)

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getXRayImageReceptorTranslation() [2/3]

virtual OFCondition DRTImageIOD::getXRayImageReceptorTranslation | ( | OFString & | value,
|  | const signed long | pos = `0`
| ) |  | const
| virtual

get XRayImageReceptorTranslation (3002,000d)

Parameters

  value | reference to variable in which the value should be stored
  pos | index of the value to get (0..vm-1), -1 for all components

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ getXRayImageReceptorTranslation() [3/3]

virtual OFCondition DRTImageIOD::getXRayImageReceptorTranslation | ( | OFVector< Float64 > & | value | ) | const
| virtual

get XRayImageReceptorTranslation (3002,000d)

Parameters

  value | reference to variable in which the value(s) should be stored

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ isApprovalModulePresent()

virtual OFBool DRTImageIOD::isApprovalModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether ApprovalModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isCineModulePresent()

virtual OFBool DRTImageIOD::isCineModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether CineModule (C) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isClinicalTrialSeriesModulePresent()

virtual OFBool DRTImageIOD::isClinicalTrialSeriesModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether ClinicalTrialSeriesModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isClinicalTrialStudyModulePresent()

virtual OFBool DRTImageIOD::isClinicalTrialStudyModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether ClinicalTrialStudyModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isClinicalTrialSubjectModulePresent()

virtual OFBool DRTImageIOD::isClinicalTrialSubjectModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether ClinicalTrialSubjectModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isCommonInstanceReferenceModulePresent()

virtual OFBool DRTImageIOD::isCommonInstanceReferenceModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether CommonInstanceReferenceModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isContrastBolusModulePresent()

virtual OFBool DRTImageIOD::isContrastBolusModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether ContrastBolusModule (C) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isDeviceModulePresent()

virtual OFBool DRTImageIOD::isDeviceModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether DeviceModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isFrameExtractionModulePresent()

virtual OFBool DRTImageIOD::isFrameExtractionModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether FrameExtractionModule (C) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isFrameOfReferenceModulePresent()

virtual OFBool DRTImageIOD::isFrameOfReferenceModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether FrameOfReferenceModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isGeneralReferenceModulePresent()

virtual OFBool DRTImageIOD::isGeneralReferenceModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether GeneralReferenceModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isModalityLUTModulePresent()

virtual OFBool DRTImageIOD::isModalityLUTModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether ModalityLUTModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isMultiFrameModulePresent()

virtual OFBool DRTImageIOD::isMultiFrameModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether MultiFrameModule (C) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isPatientStudyModulePresent()

virtual OFBool DRTImageIOD::isPatientStudyModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether PatientStudyModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ isValid()

virtual OFBool DRTImageIOD::isValid | ( |  | ) |
| virtual

check whether the current internal state is valid

Returns
  OFTrue if valid, OFFalse otherwise

## ◆ isVOILUTModulePresent()

virtual OFBool DRTImageIOD::isVOILUTModulePresent | ( | const OFBool | complete = `OFFalse` | ) |
| virtual

check whether VOILUTModule (U) is present.

By default, a module is reported as being present if at least one attribute from this module has a non-empty value.

Parameters

  complete | check for all mandatory attributes of this module if enabled

Returns
  OFTrue if module is present, OFFalse otherwise

## ◆ operator=()

DRTImageIOD& DRTImageIOD::operator= | ( | const DRTImageIOD & | copy | ) |

assignment operator

Parameters

  copy | IOD object to be copied

Returns
  reference to this object

## ◆ read()

virtual OFCondition DRTImageIOD::read | ( | DcmItem & | dataset | ) |
| virtual

read object from dataset

Parameters

  dataset | reference to DICOM dataset from which the object should be read

Returns
  status, EC_Normal if successful, an error code otherwise

Reimplemented in DRTImage.

## ◆ readPatientData()

virtual OFCondition DRTImageIOD::readPatientData | ( | DcmItem & | dataset | ) |
| virtual

read PatientData from dataset

Parameters

  dataset | reference to DICOM dataset from which the data should be read

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ readSeriesData()

virtual OFCondition DRTImageIOD::readSeriesData | ( | DcmItem & | dataset | ) |
| virtual

read SeriesData from dataset.

Also reads PatientData, StudyData.

Parameters

  dataset | reference to DICOM dataset from which the data should be read

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ readStudyData()

virtual OFCondition DRTImageIOD::readStudyData | ( | DcmItem & | dataset | ) |
| virtual

read StudyData from dataset.

Also reads PatientData.

Parameters

  dataset | reference to DICOM dataset from which the data should be read

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAccessionNumber()

virtual OFCondition DRTImageIOD::setAccessionNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AccessionNumber (0008,0050)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAcquisitionDate()

virtual OFCondition DRTImageIOD::setAcquisitionDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AcquisitionDate (0008,0022)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAcquisitionDateTime()

virtual OFCondition DRTImageIOD::setAcquisitionDateTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AcquisitionDateTime (0008,002a)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAcquisitionDuration()

virtual OFCondition DRTImageIOD::setAcquisitionDuration | ( | const Float64 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set AcquisitionDuration (0018,9073)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAcquisitionNumber()

virtual OFCondition DRTImageIOD::setAcquisitionNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AcquisitionNumber (0020,0012)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAcquisitionTime()

virtual OFCondition DRTImageIOD::setAcquisitionTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AcquisitionTime (0008,0032)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAcquisitionUID()

virtual OFCondition DRTImageIOD::setAcquisitionUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AcquisitionUID (0008,0017)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setActualFrameDuration()

virtual OFCondition DRTImageIOD::setActualFrameDuration | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ActualFrameDuration (0018,1242)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAdditionalPatientHistory()

virtual OFCondition DRTImageIOD::setAdditionalPatientHistory | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AdditionalPatientHistory (0010,21b0)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAdmissionID()

virtual OFCondition DRTImageIOD::setAdmissionID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AdmissionID (0038,0010)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAdmittingDiagnosesDescription()

virtual OFCondition DRTImageIOD::setAdmittingDiagnosesDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AdmittingDiagnosesDescription (0008,1080)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAllergies()

virtual OFCondition DRTImageIOD::setAllergies | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set Allergies (0010,2110)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setApprovalStatus()

virtual OFCondition DRTImageIOD::setApprovalStatus | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ApprovalStatus (300e,0002)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setAuthorizationEquipmentCertificationNumber()

virtual OFCondition DRTImageIOD::setAuthorizationEquipmentCertificationNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set AuthorizationEquipmentCertificationNumber (0100,0426)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setBarcodeValue()

virtual OFCondition DRTImageIOD::setBarcodeValue | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set BarcodeValue (2200,0005)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setBeamLimitingDeviceAngle()

virtual OFCondition DRTImageIOD::setBeamLimitingDeviceAngle | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set BeamLimitingDeviceAngle (300a,0120)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setBitsAllocated()

virtual OFCondition DRTImageIOD::setBitsAllocated | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set BitsAllocated (0028,0100)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setBitsStored()

virtual OFCondition DRTImageIOD::setBitsStored | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set BitsStored (0028,0101)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setBluePaletteColorLookupTableData()

virtual OFCondition DRTImageIOD::setBluePaletteColorLookupTableData | ( | const Uint16 * | value,
|  | const unsigned long | count
| ) |  |
| virtual

set BluePaletteColorLookupTableData (0028,1203)

Parameters

  value | array value to be set (data is copied)
  count | number of items in the array

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setBluePaletteColorLookupTableDescriptor()

virtual OFCondition DRTImageIOD::setBluePaletteColorLookupTableDescriptor | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set BluePaletteColorLookupTableDescriptor (0028,1103)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=3

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setBurnedInAnnotation()

virtual OFCondition DRTImageIOD::setBurnedInAnnotation | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set BurnedInAnnotation (0028,0301)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setCineRate()

virtual OFCondition DRTImageIOD::setCineRate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set CineRate (0018,0040)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialCoordinatingCenterName()

virtual OFCondition DRTImageIOD::setClinicalTrialCoordinatingCenterName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialCoordinatingCenterName (0012,0060)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialProtocolEthicsCommitteeApprovalNumber()

virtual OFCondition DRTImageIOD::setClinicalTrialProtocolEthicsCommitteeApprovalNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialProtocolEthicsCommitteeApprovalNumber (0012,0082)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialProtocolEthicsCommitteeName()

virtual OFCondition DRTImageIOD::setClinicalTrialProtocolEthicsCommitteeName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialProtocolEthicsCommitteeName (0012,0081)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialProtocolID()

virtual OFCondition DRTImageIOD::setClinicalTrialProtocolID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialProtocolID (0012,0020)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialProtocolName()

virtual OFCondition DRTImageIOD::setClinicalTrialProtocolName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialProtocolName (0012,0021)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialSeriesDescription()

virtual OFCondition DRTImageIOD::setClinicalTrialSeriesDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialSeriesDescription (0012,0072)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialSeriesID()

virtual OFCondition DRTImageIOD::setClinicalTrialSeriesID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialSeriesID (0012,0071)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialSiteID()

virtual OFCondition DRTImageIOD::setClinicalTrialSiteID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialSiteID (0012,0030)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialSiteName()

virtual OFCondition DRTImageIOD::setClinicalTrialSiteName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialSiteName (0012,0031)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialSponsorName()

virtual OFCondition DRTImageIOD::setClinicalTrialSponsorName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialSponsorName (0012,0010)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialSubjectID()

virtual OFCondition DRTImageIOD::setClinicalTrialSubjectID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialSubjectID (0012,0040)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialSubjectReadingID()

virtual OFCondition DRTImageIOD::setClinicalTrialSubjectReadingID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialSubjectReadingID (0012,0042)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialTimePointDescription()

virtual OFCondition DRTImageIOD::setClinicalTrialTimePointDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialTimePointDescription (0012,0051)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (ST) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setClinicalTrialTimePointID()

virtual OFCondition DRTImageIOD::setClinicalTrialTimePointID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ClinicalTrialTimePointID (0012,0050)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setColorSpace()

virtual OFCondition DRTImageIOD::setColorSpace | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ColorSpace (0028,2002)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setColumns()

virtual OFCondition DRTImageIOD::setColumns | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set Columns (0028,0011)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setCommentsOnThePerformedProcedureStep()

virtual OFCondition DRTImageIOD::setCommentsOnThePerformedProcedureStep | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set CommentsOnThePerformedProcedureStep (0040,0280)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (ST) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setConsultingPhysicianName()

virtual OFCondition DRTImageIOD::setConsultingPhysicianName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ConsultingPhysicianName (0008,009c)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContentDate()

virtual OFCondition DRTImageIOD::setContentDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContentDate (0008,0023)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContentQualification()

virtual OFCondition DRTImageIOD::setContentQualification | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContentQualification (0018,9004)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContentTime()

virtual OFCondition DRTImageIOD::setContentTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContentTime (0008,0033)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastBolusAgent()

virtual OFCondition DRTImageIOD::setContrastBolusAgent | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastBolusAgent (0018,0010)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastBolusIngredient()

virtual OFCondition DRTImageIOD::setContrastBolusIngredient | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastBolusIngredient (0018,1048)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastBolusIngredientConcentration()

virtual OFCondition DRTImageIOD::setContrastBolusIngredientConcentration | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastBolusIngredientConcentration (0018,1049)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastBolusRoute()

virtual OFCondition DRTImageIOD::setContrastBolusRoute | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastBolusRoute (0018,1040)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastBolusStartTime()

virtual OFCondition DRTImageIOD::setContrastBolusStartTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastBolusStartTime (0018,1042)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastBolusStopTime()

virtual OFCondition DRTImageIOD::setContrastBolusStopTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastBolusStopTime (0018,1043)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastBolusTotalDose()

virtual OFCondition DRTImageIOD::setContrastBolusTotalDose | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastBolusTotalDose (0018,1044)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastBolusVolume()

virtual OFCondition DRTImageIOD::setContrastBolusVolume | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastBolusVolume (0018,1041)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastFlowDuration()

virtual OFCondition DRTImageIOD::setContrastFlowDuration | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastFlowDuration (0018,1047)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setContrastFlowRate()

virtual OFCondition DRTImageIOD::setContrastFlowRate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ContrastFlowRate (0018,1046)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setConversionType()

virtual OFCondition DRTImageIOD::setConversionType | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ConversionType (0008,0064)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setDateOfLastCalibration()

virtual OFCondition DRTImageIOD::setDateOfLastCalibration | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set DateOfLastCalibration (0018,1200)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setDeidentificationMethod()

virtual OFCondition DRTImageIOD::setDeidentificationMethod | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set DeidentificationMethod (0012,0063)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setDerivationDescription()

virtual OFCondition DRTImageIOD::setDerivationDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set DerivationDescription (0008,2111)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (ST) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setDeviceSerialNumber()

virtual OFCondition DRTImageIOD::setDeviceSerialNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set DeviceSerialNumber (0018,1000)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setDeviceUID()

virtual OFCondition DRTImageIOD::setDeviceUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set DeviceUID (0018,1002)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setEffectiveDuration()

virtual OFCondition DRTImageIOD::setEffectiveDuration | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set EffectiveDuration (0018,0072)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setEncapsulatedPixelDataValueTotalLength()

virtual OFCondition DRTImageIOD::setEncapsulatedPixelDataValueTotalLength | ( | const Uint64 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set EncapsulatedPixelDataValueTotalLength (7fe0,0003)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setEndCumulativeMetersetWeight()

virtual OFCondition DRTImageIOD::setEndCumulativeMetersetWeight | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set EndCumulativeMetersetWeight (300c,0009)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setEnhancedRTBeamLimitingDeviceDefinitionFlag()

virtual OFCondition DRTImageIOD::setEnhancedRTBeamLimitingDeviceDefinitionFlag | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set EnhancedRTBeamLimitingDeviceDefinitionFlag (3008,00a3)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setEthnicGroup()

virtual OFCondition DRTImageIOD::setEthnicGroup | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set EthnicGroup (0010,2160)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setExposureTime()

virtual OFCondition DRTImageIOD::setExposureTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ExposureTime (0018,1150)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setExposureTimeInms()

virtual OFCondition DRTImageIOD::setExposureTimeInms | ( | const Float64 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set ExposureTimeInms (0018,9328)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setExtendedOffsetTable()

virtual OFCondition DRTImageIOD::setExtendedOffsetTable | ( | const Uint64 * | value,
|  | const unsigned long | count
| ) |  |
| virtual

set ExtendedOffsetTable (7fe0,0001)

Parameters

  value | array value to be set (data is copied)
  count | number of items in the array

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setExtendedOffsetTableLengths()

virtual OFCondition DRTImageIOD::setExtendedOffsetTableLengths | ( | const Uint64 * | value,
|  | const unsigned long | count
| ) |  |
| virtual

set ExtendedOffsetTableLengths (7fe0,0002)

Parameters

  value | array value to be set (data is copied)
  count | number of items in the array

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setFractionNumber()

virtual OFCondition DRTImageIOD::setFractionNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set FractionNumber (3002,0029)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setFrameDelay()

virtual OFCondition DRTImageIOD::setFrameDelay | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set FrameDelay (0018,1066)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setFrameIncrementPointer()

virtual OFCondition DRTImageIOD::setFrameIncrementPointer | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set FrameIncrementPointer (0028,0009)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (AT) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setFrameOfReferenceUID()

virtual OFCondition DRTImageIOD::setFrameOfReferenceUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set FrameOfReferenceUID (0020,0052)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setFrameTime()

virtual OFCondition DRTImageIOD::setFrameTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set FrameTime (0018,1063)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setFrameTimeVector()

virtual OFCondition DRTImageIOD::setFrameTimeVector | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set FrameTimeVector (0018,1065)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setGantryAngle()

virtual OFCondition DRTImageIOD::setGantryAngle | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set GantryAngle (300a,011e)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setGantryID()

virtual OFCondition DRTImageIOD::setGantryID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set GantryID (0018,1008)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setGantryPitchAngle()

virtual OFCondition DRTImageIOD::setGantryPitchAngle | ( | const Float32 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set GantryPitchAngle (300a,014a)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setGreenPaletteColorLookupTableData()

virtual OFCondition DRTImageIOD::setGreenPaletteColorLookupTableData | ( | const Uint16 * | value,
|  | const unsigned long | count
| ) |  |
| virtual

set GreenPaletteColorLookupTableData (0028,1202)

Parameters

  value | array value to be set (data is copied)
  count | number of items in the array

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setGreenPaletteColorLookupTableDescriptor()

virtual OFCondition DRTImageIOD::setGreenPaletteColorLookupTableDescriptor | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set GreenPaletteColorLookupTableDescriptor (0028,1102)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=3

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setHighBit()

virtual OFCondition DRTImageIOD::setHighBit | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set HighBit (0028,0102)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setICCProfile()

virtual OFCondition DRTImageIOD::setICCProfile | ( | const Uint8 * | value,
|  | const unsigned long | count
| ) |  |
| virtual

set ICCProfile (0028,2000)

Parameters

  value | array value to be set (data is copied)
  count | number of items in the array

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setImageComments()

virtual OFCondition DRTImageIOD::setImageComments | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ImageComments (0020,4000)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setImageLaterality()

virtual OFCondition DRTImageIOD::setImageLaterality | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ImageLaterality (0020,0062)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setImagePlanePixelSpacing()

virtual OFCondition DRTImageIOD::setImagePlanePixelSpacing | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ImagePlanePixelSpacing (3002,0011)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (2) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setImagesInAcquisition()

virtual OFCondition DRTImageIOD::setImagesInAcquisition | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ImagesInAcquisition (0020,1002)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setImageTriggerDelay()

virtual OFCondition DRTImageIOD::setImageTriggerDelay | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ImageTriggerDelay (0018,1067)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setImageType()

virtual OFCondition DRTImageIOD::setImageType | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ImageType (0008,0008)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (2-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstanceCoercionDateTime()

virtual OFCondition DRTImageIOD::setInstanceCoercionDateTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstanceCoercionDateTime (0008,0015)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstanceCreationDate()

virtual OFCondition DRTImageIOD::setInstanceCreationDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstanceCreationDate (0008,0012)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstanceCreationTime()

virtual OFCondition DRTImageIOD::setInstanceCreationTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstanceCreationTime (0008,0013)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstanceCreatorUID()

virtual OFCondition DRTImageIOD::setInstanceCreatorUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstanceCreatorUID (0008,0014)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstanceNumber()

virtual OFCondition DRTImageIOD::setInstanceNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstanceNumber (0020,0013)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstanceOriginStatus()

virtual OFCondition DRTImageIOD::setInstanceOriginStatus | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstanceOriginStatus (0400,0600)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstitutionAddress()

virtual OFCondition DRTImageIOD::setInstitutionAddress | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstitutionAddress (0008,0081)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (ST) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstitutionalDepartmentName()

virtual OFCondition DRTImageIOD::setInstitutionalDepartmentName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstitutionalDepartmentName (0008,1040)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setInstitutionName()

virtual OFCondition DRTImageIOD::setInstitutionName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set InstitutionName (0008,0080)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setIrradiationEventUID()

virtual OFCondition DRTImageIOD::setIrradiationEventUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set IrradiationEventUID (0008,3010)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setIsocenterPosition()

virtual OFCondition DRTImageIOD::setIsocenterPosition | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set IsocenterPosition (300a,012c)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (3) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setIssuerOfPatientID()

virtual OFCondition DRTImageIOD::setIssuerOfPatientID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set IssuerOfPatientID (0010,0021)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setLargestImagePixelValue()

virtual OFCondition DRTImageIOD::setLargestImagePixelValue | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set LargestImagePixelValue (0028,0107)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setLastMenstrualDate()

virtual OFCondition DRTImageIOD::setLastMenstrualDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set LastMenstrualDate (0010,21d0)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setLongitudinalTemporalEventType()

virtual OFCondition DRTImageIOD::setLongitudinalTemporalEventType | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set LongitudinalTemporalEventType (0012,0053)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setLongitudinalTemporalInformationModified()

virtual OFCondition DRTImageIOD::setLongitudinalTemporalInformationModified | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set LongitudinalTemporalInformationModified (0028,0303)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setLongitudinalTemporalOffsetFromEvent()

virtual OFCondition DRTImageIOD::setLongitudinalTemporalOffsetFromEvent | ( | const Float64 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set LongitudinalTemporalOffsetFromEvent (0012,0052)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setLossyImageCompression()

virtual OFCondition DRTImageIOD::setLossyImageCompression | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set LossyImageCompression (0028,2110)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setLossyImageCompressionMethod()

virtual OFCondition DRTImageIOD::setLossyImageCompressionMethod | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set LossyImageCompressionMethod (0028,2114)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setLossyImageCompressionRatio()

virtual OFCondition DRTImageIOD::setLossyImageCompressionRatio | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set LossyImageCompressionRatio (0028,2112)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setManufacturer()

virtual OFCondition DRTImageIOD::setManufacturer | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set Manufacturer (0008,0070)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setManufacturerDeviceClassUID()

virtual OFCondition DRTImageIOD::setManufacturerDeviceClassUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ManufacturerDeviceClassUID (0018,100b)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setManufacturerModelName()

virtual OFCondition DRTImageIOD::setManufacturerModelName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ManufacturerModelName (0008,1090)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setMeasuredAPDimension()

virtual OFCondition DRTImageIOD::setMeasuredAPDimension | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set MeasuredAPDimension (0010,1023)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setMeasuredLateralDimension()

virtual OFCondition DRTImageIOD::setMeasuredLateralDimension | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set MeasuredLateralDimension (0010,1024)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setMedicalAlerts()

virtual OFCondition DRTImageIOD::setMedicalAlerts | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set MedicalAlerts (0010,2000)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setMetersetExposure()

virtual OFCondition DRTImageIOD::setMetersetExposure | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set MetersetExposure (3002,0032)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setModality()

virtual OFCondition DRTImageIOD::setModality | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set Modality (0008,0060)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setNameOfPhysiciansReadingStudy()

virtual OFCondition DRTImageIOD::setNameOfPhysiciansReadingStudy | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set NameOfPhysiciansReadingStudy (0008,1060)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setNumberOfFrames()

virtual OFCondition DRTImageIOD::setNumberOfFrames | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set NumberOfFrames (0028,0008)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setOccupation()

virtual OFCondition DRTImageIOD::setOccupation | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set Occupation (0010,2180)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setOperatorsName()

virtual OFCondition DRTImageIOD::setOperatorsName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set OperatorsName (0008,1070)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setOriginalSpecializedSOPClassUID()

virtual OFCondition DRTImageIOD::setOriginalSpecializedSOPClassUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set OriginalSpecializedSOPClassUID (0008,001b)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setOtherPatientNames()

virtual OFCondition DRTImageIOD::setOtherPatientNames | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set OtherPatientNames (0010,1001)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientAge()

virtual OFCondition DRTImageIOD::setPatientAge | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientAge (0010,1010)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (AS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientAlternativeCalendar()

virtual OFCondition DRTImageIOD::setPatientAlternativeCalendar | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientAlternativeCalendar (0010,0035)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientBirthDate()

virtual OFCondition DRTImageIOD::setPatientBirthDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientBirthDate (0010,0030)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientBirthDateInAlternativeCalendar()

virtual OFCondition DRTImageIOD::setPatientBirthDateInAlternativeCalendar | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientBirthDateInAlternativeCalendar (0010,0033)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientBirthTime()

virtual OFCondition DRTImageIOD::setPatientBirthTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientBirthTime (0010,0032)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientBodyMassIndex()

virtual OFCondition DRTImageIOD::setPatientBodyMassIndex | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientBodyMassIndex (0010,1022)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientBreedDescription()

virtual OFCondition DRTImageIOD::setPatientBreedDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientBreedDescription (0010,2292)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientComments()

virtual OFCondition DRTImageIOD::setPatientComments | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientComments (0010,4000)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientDeathDateInAlternativeCalendar()

virtual OFCondition DRTImageIOD::setPatientDeathDateInAlternativeCalendar | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientDeathDateInAlternativeCalendar (0010,0034)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientID()

virtual OFCondition DRTImageIOD::setPatientID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientID (0010,0020)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientIdentityRemoved()

virtual OFCondition DRTImageIOD::setPatientIdentityRemoved | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientIdentityRemoved (0012,0062)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientName()

virtual OFCondition DRTImageIOD::setPatientName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientName (0010,0010)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientOrientation()

virtual OFCondition DRTImageIOD::setPatientOrientation | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientOrientation (0020,0020)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (2) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientPosition()

virtual OFCondition DRTImageIOD::setPatientPosition | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientPosition (0018,5100)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientSex()

virtual OFCondition DRTImageIOD::setPatientSex | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientSex (0010,0040)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientSexNeutered()

virtual OFCondition DRTImageIOD::setPatientSexNeutered | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientSexNeutered (0010,2203)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientSize()

virtual OFCondition DRTImageIOD::setPatientSize | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientSize (0010,1020)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientSpeciesDescription()

virtual OFCondition DRTImageIOD::setPatientSpeciesDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientSpeciesDescription (0010,2201)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientState()

virtual OFCondition DRTImageIOD::setPatientState | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientState (0038,0500)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientSupportAngle()

virtual OFCondition DRTImageIOD::setPatientSupportAngle | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientSupportAngle (300a,0122)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPatientWeight()

virtual OFCondition DRTImageIOD::setPatientWeight | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PatientWeight (0010,1030)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPerformedProcedureStepDescription()

virtual OFCondition DRTImageIOD::setPerformedProcedureStepDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PerformedProcedureStepDescription (0040,0254)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPerformedProcedureStepEndDate()

virtual OFCondition DRTImageIOD::setPerformedProcedureStepEndDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PerformedProcedureStepEndDate (0040,0250)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPerformedProcedureStepEndTime()

virtual OFCondition DRTImageIOD::setPerformedProcedureStepEndTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PerformedProcedureStepEndTime (0040,0251)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPerformedProcedureStepID()

virtual OFCondition DRTImageIOD::setPerformedProcedureStepID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PerformedProcedureStepID (0040,0253)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPerformedProcedureStepStartDate()

virtual OFCondition DRTImageIOD::setPerformedProcedureStepStartDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PerformedProcedureStepStartDate (0040,0244)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPerformedProcedureStepStartTime()

virtual OFCondition DRTImageIOD::setPerformedProcedureStepStartTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PerformedProcedureStepStartTime (0040,0245)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPhotometricInterpretation()

virtual OFCondition DRTImageIOD::setPhotometricInterpretation | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PhotometricInterpretation (0028,0004)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPhysiciansOfRecord()

virtual OFCondition DRTImageIOD::setPhysiciansOfRecord | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PhysiciansOfRecord (0008,1048)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPixelAspectRatio()

virtual OFCondition DRTImageIOD::setPixelAspectRatio | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PixelAspectRatio (0028,0034)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (2) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPixelDataProviderURL()

virtual OFCondition DRTImageIOD::setPixelDataProviderURL | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PixelDataProviderURL (0028,7fe0)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UR) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPixelIntensityRelationship()

virtual OFCondition DRTImageIOD::setPixelIntensityRelationship | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PixelIntensityRelationship (0028,1040)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPixelIntensityRelationshipSign()

virtual OFCondition DRTImageIOD::setPixelIntensityRelationshipSign | ( | const Sint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set PixelIntensityRelationshipSign (0028,1041)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPixelPaddingRangeLimit()

virtual OFCondition DRTImageIOD::setPixelPaddingRangeLimit | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set PixelPaddingRangeLimit (0028,0121)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPixelPaddingValue()

virtual OFCondition DRTImageIOD::setPixelPaddingValue | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set PixelPaddingValue (0028,0120)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPixelRepresentation()

virtual OFCondition DRTImageIOD::setPixelRepresentation | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set PixelRepresentation (0028,0103)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPlanarConfiguration()

virtual OFCondition DRTImageIOD::setPlanarConfiguration | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set PlanarConfiguration (0028,0006)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPositionReferenceIndicator()

virtual OFCondition DRTImageIOD::setPositionReferenceIndicator | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PositionReferenceIndicator (0020,1040)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPreferredPlaybackSequencing()

virtual OFCondition DRTImageIOD::setPreferredPlaybackSequencing | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set PreferredPlaybackSequencing (0018,1244)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPregnancyStatus()

virtual OFCondition DRTImageIOD::setPregnancyStatus | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set PregnancyStatus (0010,21c0)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPresentationLUTShape()

virtual OFCondition DRTImageIOD::setPresentationLUTShape | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PresentationLUTShape (2050,0020)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setPrimaryDosimeterUnit()

virtual OFCondition DRTImageIOD::setPrimaryDosimeterUnit | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set PrimaryDosimeterUnit (300a,00b3)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setQualityControlImage()

virtual OFCondition DRTImageIOD::setQualityControlImage | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set QualityControlImage (0028,0300)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setQualityControlSubject()

virtual OFCondition DRTImageIOD::setQualityControlSubject | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set QualityControlSubject (0010,0200)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setQueryRetrieveView()

virtual OFCondition DRTImageIOD::setQueryRetrieveView | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set QueryRetrieveView (0008,0053)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRadiationMachineName()

virtual OFCondition DRTImageIOD::setRadiationMachineName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RadiationMachineName (3002,0020)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRadiationMachineSAD()

virtual OFCondition DRTImageIOD::setRadiationMachineSAD | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RadiationMachineSAD (3002,0022)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRadiationMachineSSD()

virtual OFCondition DRTImageIOD::setRadiationMachineSSD | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RadiationMachineSSD (3002,0024)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setReasonForVisit()

virtual OFCondition DRTImageIOD::setReasonForVisit | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ReasonForVisit (0032,1066)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRecognizableVisualFeatures()

virtual OFCondition DRTImageIOD::setRecognizableVisualFeatures | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RecognizableVisualFeatures (0028,0302)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRecommendedDisplayFrameRate()

virtual OFCondition DRTImageIOD::setRecommendedDisplayFrameRate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RecommendedDisplayFrameRate (0008,2144)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRedPaletteColorLookupTableData()

virtual OFCondition DRTImageIOD::setRedPaletteColorLookupTableData | ( | const Uint16 * | value,
|  | const unsigned long | count
| ) |  |
| virtual

set RedPaletteColorLookupTableData (0028,1201)

Parameters

  value | array value to be set (data is copied)
  count | number of items in the array

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRedPaletteColorLookupTableDescriptor()

virtual OFCondition DRTImageIOD::setRedPaletteColorLookupTableDescriptor | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set RedPaletteColorLookupTableDescriptor (0028,1101)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=3

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setReferencedBeamNumber()

virtual OFCondition DRTImageIOD::setReferencedBeamNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ReferencedBeamNumber (300c,0006)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setReferencedFractionGroupNumber()

virtual OFCondition DRTImageIOD::setReferencedFractionGroupNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ReferencedFractionGroupNumber (300c,0022)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setReferringPhysicianName()

virtual OFCondition DRTImageIOD::setReferringPhysicianName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ReferringPhysicianName (0008,0090)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRelatedGeneralSOPClassUID()

virtual OFCondition DRTImageIOD::setRelatedGeneralSOPClassUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RelatedGeneralSOPClassUID (0008,001a)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setReportedValuesOrigin()

virtual OFCondition DRTImageIOD::setReportedValuesOrigin | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ReportedValuesOrigin (3002,000a)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRequestingService()

virtual OFCondition DRTImageIOD::setRequestingService | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RequestingService (0032,1033)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRescaleIntercept()

virtual OFCondition DRTImageIOD::setRescaleIntercept | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RescaleIntercept (0028,1052)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRescaleSlope()

virtual OFCondition DRTImageIOD::setRescaleSlope | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RescaleSlope (0028,1053)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRescaleType()

virtual OFCondition DRTImageIOD::setRescaleType | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RescaleType (0028,1054)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setResponsibleOrganization()

virtual OFCondition DRTImageIOD::setResponsibleOrganization | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ResponsibleOrganization (0010,2299)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setResponsiblePerson()

virtual OFCondition DRTImageIOD::setResponsiblePerson | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ResponsiblePerson (0010,2297)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setResponsiblePersonRole()

virtual OFCondition DRTImageIOD::setResponsiblePersonRole | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ResponsiblePersonRole (0010,2298)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setReviewDate()

virtual OFCondition DRTImageIOD::setReviewDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ReviewDate (300e,0004)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setReviewerName()

virtual OFCondition DRTImageIOD::setReviewerName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ReviewerName (300e,0008)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (PN) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setReviewTime()

virtual OFCondition DRTImageIOD::setReviewTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ReviewTime (300e,0005)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRows()

virtual OFCondition DRTImageIOD::setRows | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set Rows (0028,0010)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRTImageDescription()

virtual OFCondition DRTImageIOD::setRTImageDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RTImageDescription (3002,0004)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (ST) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRTImageLabel()

virtual OFCondition DRTImageIOD::setRTImageLabel | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RTImageLabel (3002,0002)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRTImageName()

virtual OFCondition DRTImageIOD::setRTImageName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RTImageName (3002,0003)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRTImageOrientation()

virtual OFCondition DRTImageIOD::setRTImageOrientation | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RTImageOrientation (3002,0010)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (6) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRTImagePlane()

virtual OFCondition DRTImageIOD::setRTImagePlane | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RTImagePlane (3002,000c)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRTImagePosition()

virtual OFCondition DRTImageIOD::setRTImagePosition | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RTImagePosition (3002,0012)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (2) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setRTImageSID()

virtual OFCondition DRTImageIOD::setRTImageSID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set RTImageSID (3002,0026)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSamplesPerPixel()

virtual OFCondition DRTImageIOD::setSamplesPerPixel | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set SamplesPerPixel (0028,0002)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSeriesDate()

virtual OFCondition DRTImageIOD::setSeriesDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SeriesDate (0008,0021)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSeriesDescription()

virtual OFCondition DRTImageIOD::setSeriesDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SeriesDescription (0008,103e)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSeriesInstanceUID()

virtual OFCondition DRTImageIOD::setSeriesInstanceUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SeriesInstanceUID (0020,000e)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSeriesNumber()

virtual OFCondition DRTImageIOD::setSeriesNumber | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SeriesNumber (0020,0011)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSeriesTime()

virtual OFCondition DRTImageIOD::setSeriesTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SeriesTime (0008,0031)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setServiceEpisodeDescription()

virtual OFCondition DRTImageIOD::setServiceEpisodeDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ServiceEpisodeDescription (0038,0062)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setServiceEpisodeID()

virtual OFCondition DRTImageIOD::setServiceEpisodeID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set ServiceEpisodeID (0038,0060)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSmallestImagePixelValue()

virtual OFCondition DRTImageIOD::setSmallestImagePixelValue | ( | const Uint16 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set SmallestImagePixelValue (0028,0106)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSmokingStatus()

virtual OFCondition DRTImageIOD::setSmokingStatus | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SmokingStatus (0010,21a0)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSoftwareVersions()

virtual OFCondition DRTImageIOD::setSoftwareVersions | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SoftwareVersions (0018,1020)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSOPAuthorizationComment()

virtual OFCondition DRTImageIOD::setSOPAuthorizationComment | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SOPAuthorizationComment (0100,0424)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSOPAuthorizationDateTime()

virtual OFCondition DRTImageIOD::setSOPAuthorizationDateTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SOPAuthorizationDateTime (0100,0420)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSOPClassUID()

virtual OFCondition DRTImageIOD::setSOPClassUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SOPClassUID (0008,0016)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSOPInstanceStatus()

virtual OFCondition DRTImageIOD::setSOPInstanceStatus | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SOPInstanceStatus (0100,0410)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSOPInstanceUID()

virtual OFCondition DRTImageIOD::setSOPInstanceUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SOPInstanceUID (0008,0018)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSourceToReferenceObjectDistance()

virtual OFCondition DRTImageIOD::setSourceToReferenceObjectDistance | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SourceToReferenceObjectDistance (3002,0028)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSpatialResolution()

virtual OFCondition DRTImageIOD::setSpatialResolution | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SpatialResolution (0018,1050)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setSpecificCharacterSet()

virtual OFCondition DRTImageIOD::setSpecificCharacterSet | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set SpecificCharacterSet (0008,0005)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStartCumulativeMetersetWeight()

virtual OFCondition DRTImageIOD::setStartCumulativeMetersetWeight | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StartCumulativeMetersetWeight (300c,0008)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStartTrim()

virtual OFCondition DRTImageIOD::setStartTrim | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StartTrim (0008,2142)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStationName()

virtual OFCondition DRTImageIOD::setStationName | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StationName (0008,1010)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStereoPairsPresent()

virtual OFCondition DRTImageIOD::setStereoPairsPresent | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StereoPairsPresent (0022,0028)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStopTrim()

virtual OFCondition DRTImageIOD::setStopTrim | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StopTrim (0008,2143)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (IS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStrainAdditionalInformation()

virtual OFCondition DRTImageIOD::setStrainAdditionalInformation | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StrainAdditionalInformation (0010,0218)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UT) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStrainDescription()

virtual OFCondition DRTImageIOD::setStrainDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StrainDescription (0010,0212)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UC) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStrainNomenclature()

virtual OFCondition DRTImageIOD::setStrainNomenclature | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StrainNomenclature (0010,0213)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStudyDate()

virtual OFCondition DRTImageIOD::setStudyDate | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StudyDate (0008,0020)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DA) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStudyDescription()

virtual OFCondition DRTImageIOD::setStudyDescription | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StudyDescription (0008,1030)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStudyID()

virtual OFCondition DRTImageIOD::setStudyID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StudyID (0020,0010)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStudyInstanceUID()

virtual OFCondition DRTImageIOD::setStudyInstanceUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StudyInstanceUID (0020,000d)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setStudyTime()

virtual OFCondition DRTImageIOD::setStudyTime | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set StudyTime (0008,0030)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTableTopEccentricAngle()

virtual OFCondition DRTImageIOD::setTableTopEccentricAngle | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TableTopEccentricAngle (300a,0125)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTableTopEccentricAxisDistance()

virtual OFCondition DRTImageIOD::setTableTopEccentricAxisDistance | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TableTopEccentricAxisDistance (300a,0124)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTableTopLateralPosition()

virtual OFCondition DRTImageIOD::setTableTopLateralPosition | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TableTopLateralPosition (300a,012a)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTableTopLongitudinalPosition()

virtual OFCondition DRTImageIOD::setTableTopLongitudinalPosition | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TableTopLongitudinalPosition (300a,0129)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTableTopPitchAngle()

virtual OFCondition DRTImageIOD::setTableTopPitchAngle | ( | const Float32 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set TableTopPitchAngle (300a,0140)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTableTopRollAngle()

virtual OFCondition DRTImageIOD::setTableTopRollAngle | ( | const Float32 | value,
|  | const unsigned long | pos = `0`
| ) |  |
| virtual

set TableTopRollAngle (300a,0144)

Parameters

  value | value to be set (should be valid for this VR)
  pos | index of the value to be set (0..vm-1), vm=1

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTableTopVerticalPosition()

virtual OFCondition DRTImageIOD::setTableTopVerticalPosition | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TableTopVerticalPosition (300a,0128)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTimeOfLastCalibration()

virtual OFCondition DRTImageIOD::setTimeOfLastCalibration | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TimeOfLastCalibration (0018,1201)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (TM) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTimezoneOffsetFromUTC()

virtual OFCondition DRTImageIOD::setTimezoneOffsetFromUTC | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TimezoneOffsetFromUTC (0008,0201)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (SH) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTreatmentSessionUID()

virtual OFCondition DRTImageIOD::setTreatmentSessionUID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TreatmentSessionUID (300a,0700)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (UI) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setTypeOfPatientID()

virtual OFCondition DRTImageIOD::setTypeOfPatientID | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set TypeOfPatientID (0010,0022)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setVOILUTFunction()

virtual OFCondition DRTImageIOD::setVOILUTFunction | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set VOILUTFunction (0028,1056)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (CS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setWindowCenter()

virtual OFCondition DRTImageIOD::setWindowCenter | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set WindowCenter (0028,1050)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setWindowCenterWidthExplanation()

virtual OFCondition DRTImageIOD::setWindowCenterWidthExplanation | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set WindowCenterWidthExplanation (0028,1055)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (LO) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setWindowWidth()

virtual OFCondition DRTImageIOD::setWindowWidth | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set WindowWidth (0028,1051)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1-n) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setXRayImageReceptorAngle()

virtual OFCondition DRTImageIOD::setXRayImageReceptorAngle | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set XRayImageReceptorAngle (3002,000e)

Parameters

  value | value to be set (single value only) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (1) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ setXRayImageReceptorTranslation()

virtual OFCondition DRTImageIOD::setXRayImageReceptorTranslation | ( | const OFString & | value,
|  | const OFBool | check = `OFTrue`
| ) |  |
| virtual

set XRayImageReceptorTranslation (3002,000d)

Parameters

  value | value to be set (possibly multi-valued) or "" for no value
  check | check 'value' for conformance with VR (DS) and VM (3) if enabled

Returns
  status, EC_Normal if successful, an error code otherwise

## ◆ write()

virtual OFCondition DRTImageIOD::write | ( | DcmItem & | dataset | ) |
| virtual

write object to dataset

Parameters

  dataset | reference to DICOM dataset to which the object should be written

Returns
  status, EC_Normal if successful, an error code otherwise

## Member Data Documentation

## ◆ BitsAllocated

DcmUnsignedShort DRTImageIOD::BitsAllocated
| private

BitsAllocated (0028,0100) vr=US, vm=1, type=1.

- also defined in: ImagePixelModule

## ◆ BitsStored

DcmUnsignedShort DRTImageIOD::BitsStored
| private

BitsStored (0028,0101) vr=US, vm=1, type=1.

- also defined in: ImagePixelModule

## ◆ HighBit

DcmUnsignedShort DRTImageIOD::HighBit
| private

HighBit (0028,0102) vr=US, vm=1, type=1.

- also defined in: ImagePixelModule

## ◆ ImageType

DcmCodeString DRTImageIOD::ImageType
| private

ImageType (0008,0008) vr=CS, vm=2-n, type=1.

- also defined in: GeneralImageModule

## ◆ InstanceNumber

DcmIntegerString DRTImageIOD::InstanceNumber
| private

InstanceNumber (0020,0013) vr=IS, vm=1, type=2.

- also defined in: SOPCommonModule

## ◆ PhotometricInterpretation

DcmCodeString DRTImageIOD::PhotometricInterpretation
| private

PhotometricInterpretation (0028,0004) vr=CS, vm=1, type=1.

- also defined in: ImagePixelModule

## ◆ PixelRepresentation

DcmUnsignedShort DRTImageIOD::PixelRepresentation
| private

PixelRepresentation (0028,0103) vr=US, vm=1, type=1.

- also defined in: ImagePixelModule

## ◆ SamplesPerPixel

DcmUnsignedShort DRTImageIOD::SamplesPerPixel
| private

SamplesPerPixel (0028,0002) vr=US, vm=1, type=1.

- also defined in: ImagePixelModule

The documentation for this class was generated from the following file:

- dcmrt/include/dcmtk/dcmrt/drtimage.h

Generated on Mon Dec 15 2025 for DCMTK Version 3.7.0 by Doxygen 1.9.1