DCMTK Version 3.7.0 OFFIS DICOM Toolkit

dcmqrscp: DICOM image archive (central test node)

# SYNOPSIS

    dcmqrscp [options] [port]

# DESCRIPTION

The Image Central Test Node (dcmqrscp) Application implements a simple image archive. It manages a number of storage areas and allows images to be stored in these storage areas using the DICOM Storage Service Class. It also allows image attributes to be queried and images to be retrieved using the DICOM Query/Retrieve Service Class. The dcmqrscp application also implements access restriction rules to limit operations to specific peer application entities.

The dcmqrscp application is intended to be used in DICOM demonstrations and as a compatibility test tool. In particular, dcmqrscp will delete images if its quota restrictions have been exceeded.

Caution: Note that the format of dcmqrdb's binary index.dat file changed on 20130705 due to a bug fix in the corresponding code. An index.dat file created before that date will not work with dcmqrdb code compiled after that date but must be re-created. Use dcmqridx for that task or re-send all images to the server after deleting all old files (and creating a new empty index.dat file).

# PARAMETERS

    port  tcp/ip port number to listen on (default: in config file)

# OPTIONS

## general options

      -h    --help
              print this help text and exit

            --version
              print version information and exit

            --arguments
              print expanded command line arguments

      -q    --quiet
              quiet mode, print no warnings and errors

      -v    --verbose
              verbose mode, print processing details

      -d    --debug
              debug mode, print debug information

      -ll   --log-level  [l]evel: string constant
              (fatal, error, warn, info, debug, trace)
              use level l for the logger

      -lc   --log-config  [f]ilename: string
              use config file f for the logger

      -c    --config  [f]ilename: string
              use specific configuration file
              (default: /usr/local/etc/dcmtk-<VERSION>/dcmqrscp.cfg)

      # This option allows a specific configuration file to be
      # specified.  By default, the configuration file in the
      # system configuration directory ("etc" on Unix systems and
      # current working directory on Windows systems) with the name
      # "dcmqrscp.cfg" will be used.  It is an error if a valid
      # configuration file is not available.  See the documentation
      # on configuration for more information (dcmqrcnf.txt and the
      # example configuration file dcmqrscp.cfg).

## multi-process options

      -s    --single-process
              single process mode

      # This option instructs dcmqrscp to run in single process mode.
      # Normally, dcmqrscp will spawn a new copy of itself to handle
      # each association.  This option will prevent such copies being
      # spawned and is particularly useful when running within a
      # debugger.

            --fork
              fork child process for each association (default)

      # Please note that the multi-process options are only available
      # on systems that support the fork() call, i.e. not on Windows.

## database options

    association negotiation:

            --require-find
              reject all MOVE/GET presentation contexts for
              which no corresponding FIND context is proposed

      # This option causes dcmqrscp to enforce a restriction about
      # FIND and MOVE presentation contexts.  The RSNA'93 demonstration
      # required that a CTN refuse to accept a presentation context for
      # a MOVE if a FIND presentation context is not also requested.
      # This option enforces this restriction.

            --no-parallel-store
              reject multiple simultaneous STORE presentation
              contexts for one application entity title

      # This option causes dcmqrscp to refuse storage presentations
      # contexts for AE Titles if another association has already
      # successfully negotiated storage presentation contexts for the
      # AE Title.  This option should only be needed for debugging
      # since the dcmqrscp database back-end sequentialises access via
      # file-locking.

            --disable-get
              disable C-GET support

            --allow-shutdown
              allow external shutdown via a private SOP class

    checking identifier validity:

      -XF   --check-find
              check C-FIND identifier validity

      # This option causes dcmqrscp database back-end to perform checks
      # on the Query Identifiers for a C-FIND command.  With this option,
      # dcmqrscp will reject any queries which do not conform to the very
      # strict DICOM rules for Query Identifiers.

            --no-check-find
              do not check C-FIND identifier validity (default)

      -XM   --check-move
              check C-MOVE identifier validity

      # This option causes dcmqrscp database back-end to perform checks
      # on the Query Identifiers for a C-MOVE command.  With this option,
      # dcmqrscp will reject any queries which do not conform to the very
      # strict DICOM rules for Query Identifiers.

            --no-check-move
              do not check C-MOVE identifier validity (default)

    restriction of move targets:

            --move-unrestricted
              do not restrict move destination (default)

      -ZA   --move-aetitle
              restrict move destination to requesting AE title

      -ZH   --move-host
              restrict move destination to requesting host

      -ZV   --move-vendor
              restrict move destination to requesting vendor

    restriction of query/retrieve models:

      -QP   --no-patient-root
              do not support Patient Root Q/R models

      -QS   --no-study-root
              do not support Study Root Q/R models

      -QO   --no-patient-study
              do not support Patient/Study Only Q/R models

## network options

    IP protocol version:

      -i4   --ipv4
              use IPv4 only (default)

      -i6   --ipv6
              use IPv6 only

      -i0   --ip-auto
              use IPv6/IPv4 dual stack

    association negotiation profiles from configuration file:

      -xf   --assoc-config-file
              [f]ilename, [i]n-profile, [o]ut-profile: string
              use profile i from f for incoming associations,
              and profile o from f for outgoing associations

    preferred network transfer syntaxes (incoming associations):

      +x=   --prefer-uncompr
              prefer explicit VR local byte order (default)

      +xe   --prefer-little
              prefer explicit VR little endian TS

      +xb   --prefer-big
              prefer explicit VR big endian TS

      +xs   --prefer-lossless
              prefer default JPEG lossless TS

      +xy   --prefer-jpeg8
              prefer default JPEG lossy TS for 8 bit data

      +xx   --prefer-jpeg12
              prefer default JPEG lossy TS for 12 bit data

      +xv   --prefer-j2k-lossless
              prefer JPEG 2000 lossless TS

      +xw   --prefer-j2k-lossy
              prefer JPEG 2000 lossy TS

      +xt   --prefer-jls-lossless
              prefer JPEG-LS lossless TS

      +xu   --prefer-jls-lossy
              prefer JPEG-LS lossy TS

      +xm   --prefer-mpeg2
              prefer MPEG2 Main Profile @ Main Level TS

      +xh   --prefer-mpeg2-high
              prefer MPEG2 Main Profile @ High Level TS

      +xn   --prefer-mpeg4
              prefer MPEG4 AVC/H.264 High Profile / Level 4.1 TS

      +xl   --prefer-mpeg4-bd
              prefer MPEG4 AVC/H.264 BD-compatible HP / Level 4.1 TS

      +x2   --prefer-mpeg4-2-2d
              prefer MPEG4 AVC/H.264 HP / Level 4.2 TS for 2D Videos

      +x3   --prefer-mpeg4-2-3d
              prefer MPEG4 AVC/H.264 HP / Level 4.2 TS for 3D Videos

      +xo   --prefer-mpeg4-2-st
              prefer MPEG4 AVC/H.264 Stereo HP / Level 4.2 TS

      +x4   --prefer-hevc
              prefer HEVC/H.265 Main Profile / Level 5.1 TS

      +x5   --prefer-hevc10
              prefer HEVC/H.265 Main 10 Profile / Level 5.1 TS

      +xr   --prefer-rle
              prefer RLE lossless TS

      +xd   --prefer-deflated
              prefer deflated explicit VR little endian TS

      +xi   --implicit
              accept implicit VR little endian TS only

    proposed transmission transfer syntaxes (outgoing associations):

      -x=   --propose-uncompr
              propose all uncompressed TS, explicit VR
              with local byte ordering first (default)

      -xe   --propose-little
              propose all uncompressed TS, explicit VR little endian first

      -xb   --propose-big
              propose all uncompressed TS, explicit VR big endian first

      -xi   --propose-implicit
              propose implicit VR little endian TS only

      -xs   --propose-lossless
              propose default JPEG lossless TS
              and all uncompressed transfer syntaxes

      -xy   --propose-jpeg8
              propose default JPEG lossy TS for 8 bit data
              and all uncompressed transfer syntaxes

      -xx   --propose-jpeg12
              propose default JPEG lossy TS for 12 bit data
              and all uncompressed transfer syntaxes

      -xv   --propose-j2k-lossless
              propose JPEG 2000 lossless TS
              and all uncompressed transfer syntaxes

      -xw   --propose-j2k-lossy
              propose JPEG 2000 lossy TS
              and all uncompressed transfer syntaxes

      -xt   --propose-jls-lossless
              propose JPEG-LS lossless TS
              and all uncompressed transfer syntaxes

      -xu   --propose-jls-lossy
              propose JPEG-LS lossy TS
              and all uncompressed transfer syntaxes

      -xm   --propose-mpeg2
              propose MPEG2 Main Profile @ Main Level TS only

      -xh   --propose-mpeg2-high
              propose MPEG2 Main Profile @ High Level TS only

      -xn   --propose-mpeg4
              propose MPEG4 AVC/H.264 High Profile / Level 4.1 TS only

      -xl   --propose-mpeg4-bd
              propose MPEG4 AVC/H.264 BD-compatible HP / Level 4.1 TS only

      -x2   --propose-mpeg4-2-2d
              propose MPEG4 AVC/H.264 HP / Level 4.2 TS for 2D Videos only

      -x3   --propose-mpeg4-2-3d
              propose MPEG4 AVC/H.264 HP / Level 4.2 TS for 3D Videos only

      -xo   --propose-mpeg4-2-st
              propose MPEG4 AVC/H.264 Stereo HP / Level 4.2 TS only

      -x4   --propose-hevc
              propose HEVC/H.265 Main Profile / Level 5.1 TS only

      -x5   --propose-hevc10
              propose HEVC/H.265 Main 10 Profile / Level 5.1 TS only

      -xr   --propose-rle
              propose RLE lossless TS
              and all uncompressed transfer syntaxes

      -xd   --propose-deflated
              propose deflated explicit VR little endian TS
              and all uncompressed transfer syntaxes

    network host access control (tcp wrapper):

      -ac   --access-full
              accept connections from any host (default)

      +ac   --access-control
              enforce host access control rules

    other network options:

      -to   --timeout  [s]econds: integer (default: unlimited)
              timeout for connection requests

      -ta   --acse-timeout  [s]econds: integer (default: 30)
              timeout for ACSE messages

      -td   --dimse-timeout  [s]econds: integer (default: unlimited)
              timeout for DIMSE messages

      -pdu  --max-pdu  [n]umber of bytes: integer (4096..131072)
              set max receive pdu to n bytes
              (default: use value from configuration file)

      -dhl  --disable-host-lookup
              disable hostname lookup

            --refuse
              refuse association

            --reject
              reject association if no implementation class UID

            --ignore
              ignore store data, receive but do not store

      # This option causes dcmqrscp database back-end to ignore
      # all images received by the Storage Service Class.  All images
      # will be received from the network but not stored to disk nor
      # recorded in database.

      -up   --uid-padding
              silently correct space-padded UIDs

## processing options

    specific character set:

      # the following options require support from an underlying character
      # encoding library (see output of --version on which one is available)

      +Cr   --use-request-charset
              try to convert all element values that are affected by
              Specific Character Set (0008,0005) to the one specified
              in the request data set, fall back to the one specified
              via --convert-to-xxx if that is not possible
              (default, unless overridden by config file)

      -Cr   --override-charset
              convert affected element values to the character set
              specified via --convert-to-xxx, ignoring the one
              specified in the request

      +A7   --convert-to-ascii
              convert affected element values to 7-bit ASCII
              (default, unless overridden by config file)

      +U8   --convert-to-utf8
              convert affected element values to UTF-8

      +L1   --convert-to-latin1
              convert affected element values to ISO 8859-1

      +C    --convert-to-charset  [c]harset: string
              convert affected element values to the character set
              specified by the DICOM defined term c

      -Ct   --transliterate
              try to approximate characters that cannot be
              represented through similar looking characters

      -Cd   --discard-illegal
              discard characters that cannot be represented
              in destination character set

## transport layer security (TLS) options

    transport protocol stack:

      -tls  --disable-tls
              use normal TCP/IP connection (default)

      +tls  --enable-tls  [p]rivate key file, [c]ertificate file: string
              use authenticated secure TLS connection

    private key password (only with --enable-tls):

      +ps   --std-passwd
              prompt user to type password on stdin (default)

      +pw   --use-passwd  [p]assword: string
              use specified password

      -pw   --null-passwd
              use empty string as password

    key and certificate file format:

      -pem  --pem-keys
              read keys and certificates as PEM file (default)

      -der  --der-keys
              read keys and certificates as DER file

    certification authority:

      +cf   --add-cert-file  [f]ilename: string
              add certificate file to list of certificates

      +cd   --add-cert-dir  [d]irectory: string
              add certificates in d to list of certificates

      +crl  --add-crl-file  [f]ilename: string
              add certificate revocation list file
              (implies --enable-crl-vfy)

      +crv  --enable-crl-vfy
              enable leaf CRL verification

      +cra  --enable-crl-all
              enable full chain CRL verification

    security profile:

      +ph   --list-profiles
              list supported TLS profiles and exit

      +pg   --profile-8996
              BCP 195 RFC 8996 TLS Profile (default)

      +pm   --profile-8996-mod
              Modified BCP 195 RFC 8996 TLS Profile

              # only available if underlying TLS library supports
              # all TLS features required for this profile

      +py   --profile-bcp195-nd
              Non-downgrading BCP 195 TLS Profile (retired)

      +px   --profile-bcp195
              BCP 195 TLS Profile (retired)

      +pz   --profile-bcp195-ex
              Extended BCP 195 TLS Profile (retired)

      +pb   --profile-basic
              Basic TLS Secure Transport Connection Profile (retired)

              # only available if underlying TLS library supports 3DES

      +pa   --profile-aes
              AES TLS Secure Transport Connection Profile (retired)

      +pn   --profile-null
              Authenticated unencrypted communication
              (retired, was used in IHE ATNA)

    ciphersuite:

      +cc   --list-ciphers
              list supported TLS ciphersuites and exit

      +cs   --cipher  [c]iphersuite name: string
              add ciphersuite to list of negotiated suites

      +dp   --dhparam  [f]ilename: string
              read DH parameters for DH/DSS ciphersuites

    server name indication:

            --no-sni
              do not use SNI (default)

            --expect-sni  [s]erver name: string
              expect requests for server name s

    pseudo random generator:

      +rs   --seed  [f]ilename: string
              seed random generator with contents of f

      +ws   --write-seed
              write back modified seed (only with --seed)

      +wf   --write-seed-file  [f]ilename: string (only with --seed)
              write modified seed to file f

    peer authentication:

      -rc   --require-peer-cert
              verify peer certificate, fail if absent (default)

      -vc   --verify-peer-cert
              verify peer certificate if present

      -ic   --ignore-peer-cert
              don't verify peer certificate

## output options

    bit preserving mode:

      -B    --normal
              allow implicit format conversions (default)

      +B    --bit-preserving
              write data exactly as read

    output file format:

      +F    --write-file
              write file format (default)

      -F    --write-dataset
              write data set without file meta information

    output transfer syntax:
    (not with --bit-preserving or compressed transmission)

      +t=   --write-xfer-same
              write with same TS as input (default)

      +te   --write-xfer-little
              write with explicit VR little endian TS

      +tb   --write-xfer-big
              write with explicit VR big endian TS

      +ti   --write-xfer-implicit
              write with implicit VR little endian TS

      +td   --write-xfer-deflated
              write with deflated explicit VR little endian TS

    post-1993 value representations:

      +u    --enable-new-vr
              enable support for new VRs (UN/UT) (default)

      -u    --disable-new-vr
              disable support for new VRs, convert to OB

    group length encoding (not with --bit-preserving):

      +g=   --group-length-recalc
              recalculate group lengths if present (default)

      +g    --group-length-create
              always write with group length elements

      -g    --group-length-remove
              always write without group length elements

    length encoding in sequences and items (not with --bit-preserving):

      +e    --length-explicit
              write with explicit lengths (default)

      -e    --length-undefined
              write with undefined lengths

    data set trailing padding (not with --write-dataset or --bit-preserving):

      -p    --padding-off
              no padding (default)

      +p    --padding-create  [f]ile-pad [i]tem-pad: integer
              align file on multiple of f bytes
              and items on multiple of i bytes

    deflate compression level (only with --propose-deflated or
    --write-xfer-deflated/same):

      +cl   --compression-level  [l]evel: integer (default: 6)
              0=uncompressed, 1=fastest, 9=best compression

# NOTES

## Operation

dcmqrscp waits for another application to connect at the presentation address (port number) specified in its configuration file (or overridden by a command line option). When another application connects, dcmqrscp expects it to be a DICOM application and to use calling and called AE Titles specified in dcmqrscp's configuration file. dcmqrscp will accept associations with Presentation Contexts for SOP Classes of the Verification Service Class, Storage Service Class and Query/Retrieve Service Class. Associations will be rejected or Presentation Contexts will be refused if the peer application does not have appropriate access rights as specified by dcmqrscp configuration file.

dcmqrscp will receive images on Presentation Contexts of the Storage Service Class, write them to a configurable storage area associated with the class AE title, extract attributes from these images and store them in a database. dcmqrscp will receive query requests and generate query responses on Presentation Contexts of the Query/Retrieve Service class. dcmqrscp will receive retrieve requests and generate retrieve responses on Presentation Contexts of the Query/Retrieve Service class. dcmqrscp will also process C-CANCEL messages to interrupt query/retrieve operations.

Under normal operations dcmqrscp will never exit, it keeps on waiting for new associations until killed.

## DICOM Conformance

### SCU Conformance

The dcmqrscp application supports the following SOP Classes as an SCU:

    VerificationSOPClass                                 1.2.840.10008.1.1

    RETIRED_StoredPrintStorage                           1.2.840.10008.5.1.1.27
    RETIRED_HardcopyGrayscaleImageStorage                1.2.840.10008.5.1.1.29
    RETIRED_HardcopyColorImageStorage                    1.2.840.10008.5.1.1.30
    ComputedRadiographyImageStorage                      1.2.840.10008.5.1.4.1.1.1
    DigitalXRayImageStorageForPresentation               1.2.840.10008.5.1.4.1.1.1.1
    DigitalXRayImageStorageForProcessing                 1.2.840.10008.5.1.4.1.1.1.1.1
    DigitalMammographyXRayImageStorageForPresentation    1.2.840.10008.5.1.4.1.1.1.2
    DigitalMammographyXRayImageStorageForProcessing      1.2.840.10008.5.1.4.1.1.1.2.1
    DigitalIntraOralXRayImageStorageForPresentation      1.2.840.10008.5.1.4.1.1.1.3
    DigitalIntraOralXRayImageStorageForProcessing        1.2.840.10008.5.1.4.1.1.1.3.1
    CTImageStorage                                       1.2.840.10008.5.1.4.1.1.2
    EnhancedCTImageStorage                               1.2.840.10008.5.1.4.1.1.2.1
    LegacyConvertedEnhancedCTImageStorage                1.2.840.10008.5.1.4.1.1.2.2
    RETIRED_UltrasoundMultiframeImageStorage             1.2.840.10008.5.1.4.1.1.3
    UltrasoundMultiframeImageStorage                     1.2.840.10008.5.1.4.1.1.3.1
    MRImageStorage                                       1.2.840.10008.5.1.4.1.1.4
    EnhancedMRImageStorage                               1.2.840.10008.5.1.4.1.1.4.1
    MRSpectroscopyStorage                                1.2.840.10008.5.1.4.1.1.4.2
    EnhancedMRColorImageStorage                          1.2.840.10008.5.1.4.1.1.4.3
    LegacyConvertedEnhancedMRImageStorage                1.2.840.10008.5.1.4.1.1.4.4
    RETIRED_NuclearMedicineImageStorage                  1.2.840.10008.5.1.4.1.1.5
    RETIRED_UltrasoundImageStorage                       1.2.840.10008.5.1.4.1.1.6
    UltrasoundImageStorage                               1.2.840.10008.5.1.4.1.1.6.1
    EnhancedUSVolumeStorage                              1.2.840.10008.5.1.4.1.1.6.2
    SecondaryCaptureImageStorage                         1.2.840.10008.5.1.4.1.1.7
    MultiframeSingleBitSecondaryCaptureImageStorage      1.2.840.10008.5.1.4.1.1.7.1
    MultiframeGrayscaleByteSecondaryCaptureImageStorage  1.2.840.10008.5.1.4.1.1.7.2
    MultiframeGrayscaleWordSecondaryCaptureImageStorage  1.2.840.10008.5.1.4.1.1.7.3
    MultiframeTrueColorSecondaryCaptureImageStorage      1.2.840.10008.5.1.4.1.1.7.4
    RETIRED_StandaloneOverlayStorage                     1.2.840.10008.5.1.4.1.1.8
    RETIRED_StandaloneCurveStorage                       1.2.840.10008.5.1.4.1.1.9
    TwelveLeadECGWaveformStorage                         1.2.840.10008.5.1.4.1.1.9.1.1
    GeneralECGWaveformStorage                            1.2.840.10008.5.1.4.1.1.9.1.2
    AmbulatoryECGWaveformStorage                         1.2.840.10008.5.1.4.1.1.9.1.3
    HemodynamicWaveformStorage                           1.2.840.10008.5.1.4.1.1.9.2.1
    CardiacElectrophysiologyWaveformStorage              1.2.840.10008.5.1.4.1.1.9.3.1
    BasicVoiceAudioWaveformStorage                       1.2.840.10008.5.1.4.1.1.9.4.1
    GeneralAudioWaveformStorage                          1.2.840.10008.5.1.4.1.1.9.4.2
    ArterialPulseWaveformStorage                         1.2.840.10008.5.1.4.1.1.9.5.1
    RespiratoryWaveformStorage                           1.2.840.10008.5.1.4.1.1.9.6.1
    RETIRED_StandaloneModalityLUTStorage                 1.2.840.10008.5.1.4.1.1.10
    RETIRED_StandaloneVOILUTStorage                      1.2.840.10008.5.1.4.1.1.11
    GrayscaleSoftcopyPresentationStateStorage            1.2.840.10008.5.1.4.1.1.11.1
    ColorSoftcopyPresentationStateStorage                1.2.840.10008.5.1.4.1.1.11.2
    PseudoColorSoftcopyPresentationStateStorage          1.2.840.10008.5.1.4.1.1.11.3
    BlendingSoftcopyPresentationStateStorage             1.2.840.10008.5.1.4.1.1.11.4
    XAXRFGrayscaleSoftcopyPresentationStateStorage       1.2.840.10008.5.1.4.1.1.11.5
    XRayAngiographicImageStorage                         1.2.840.10008.5.1.4.1.1.12.1
    EnhancedXAImageStorage                               1.2.840.10008.5.1.4.1.1.12.1.1
    XRayRadiofluoroscopicImageStorage                    1.2.840.10008.5.1.4.1.1.12.2
    EnhancedXRFImageStorage                              1.2.840.10008.5.1.4.1.1.12.2.1
    RETIRED_XRayAngiographicBiPlaneImageStorage          1.2.840.10008.5.1.4.1.1.12.3
    XRay3DAngiographicImageStorage                       1.2.840.10008.5.1.4.1.1.13.1.1
    XRay3DCraniofacialImageStorage                       1.2.840.10008.5.1.4.1.1.13.1.2
    BreastTomosynthesisImageStorage                      1.2.840.10008.5.1.4.1.1.13.1.3
    IntravascularOpt.Coh.Tom.ImageStorageForPresentation 1.2.840.10008.5.1.4.1.1.14.1
    IntravascularOpt.Coh.Tom.ImageStorageForProcessing   1.2.840.10008.5.1.4.1.1.14.2
    NuclearMedicineImageStorage                          1.2.840.10008.5.1.4.1.1.20
    RawDataStorage                                       1.2.840.10008.5.1.4.1.1.66
    SpatialRegistrationStorage                           1.2.840.10008.5.1.4.1.1.66.1
    SpatialFiducialsStorage                              1.2.840.10008.5.1.4.1.1.66.2
    DeformableSpatialRegistrationStorage                 1.2.840.10008.5.1.4.1.1.66.3
    SegmentationStorage                                  1.2.840.10008.5.1.4.1.1.66.4
    SurfaceSegmentationStorage                           1.2.840.10008.5.1.4.1.1.66.5
    RealWorldValueMappingStorage                         1.2.840.10008.5.1.4.1.1.67
    SurfaceScanMeshStorage                               1.2.840.10008.5.1.4.1.1.68.1
    SurfaceScanPointCloudStorage                         1.2.840.10008.5.1.4.1.1.68.2
    RETIRED_VLImageStorage                               1.2.840.10008.5.1.4.1.1.77.1
    VLEndoscopicImageStorage                             1.2.840.10008.5.1.4.1.1.77.1.1
    VideoEndoscopicImageStorage                          1.2.840.10008.5.1.4.1.1.77.1.1.1
    VLMicroscopicImageStorage                            1.2.840.10008.5.1.4.1.1.77.1.2
    VideoMicroscopicImageStorage                         1.2.840.10008.5.1.4.1.1.77.1.2.1
    VLSlideCoordinatesMicroscopicImageStorage            1.2.840.10008.5.1.4.1.1.77.1.3
    VLPhotographicImageStorage                           1.2.840.10008.5.1.4.1.1.77.1.4
    VideoPhotographicImageStorage                        1.2.840.10008.5.1.4.1.1.77.1.4.1
    OphthalmicPhotography8BitImageStorage                1.2.840.10008.5.1.4.1.1.77.1.5.1
    OphthalmicPhotography16BitImageStorage               1.2.840.10008.5.1.4.1.1.77.1.5.2
    StereometricRelationshipStorage                      1.2.840.10008.5.1.4.1.1.77.1.5.3
    OphthalmicTomographyImageStorage                     1.2.840.10008.5.1.4.1.1.77.1.5.4
    VLWholeSlideMicroscopyImageStorage                   1.2.840.10008.5.1.4.1.1.77.1.6
    RETIRED_VLMultiframeImageStorage                     1.2.840.10008.5.1.4.1.1.77.2
    LensometryMeasurementsStorage                        1.2.840.10008.5.1.4.1.1.78.1
    AutorefractionMeasurementsStorage                    1.2.840.10008.5.1.4.1.1.78.2
    KeratometryMeasurementsStorage                       1.2.840.10008.5.1.4.1.1.78.3
    SubjectiveRefractionMeasurementsStorage              1.2.840.10008.5.1.4.1.1.78.4
    VisualAcuityMeasurementsStorage                      1.2.840.10008.5.1.4.1.1.78.5
    SpectaclePrescriptionReportStorage                   1.2.840.10008.5.1.4.1.1.78.6
    OphthalmicAxialMeasurementsStorage                   1.2.840.10008.5.1.4.1.1.78.7
    IntraocularLensCalculationsStorage                   1.2.840.10008.5.1.4.1.1.78.8
    MacularGridThicknessAndVolumeReportStorage           1.2.840.10008.5.1.4.1.1.79.1
    OphthalmicVisualFieldStaticPerimetryMeasurementsSt.  1.2.840.10008.5.1.4.1.1.80.1
    OphthalmicThicknessMapStorage                        1.2.840.10008.5.1.4.1.1.81.1
    BasicTextSRStorage                                   1.2.840.10008.5.1.4.1.1.88.11
    EnhancedSRStorage                                    1.2.840.10008.5.1.4.1.1.88.22
    ComprehensiveSRStorage                               1.2.840.10008.5.1.4.1.1.88.33
    Comprehensive3DSRStorage                             1.2.840.10008.5.1.4.1.1.88.34
    ProcedureLogStorage                                  1.2.840.10008.5.1.4.1.1.88.40
    MammographyCADSRStorage                              1.2.840.10008.5.1.4.1.1.88.50
    KeyObjectSelectionDocumentStorage                    1.2.840.10008.5.1.4.1.1.88.59
    ChestCADSRStorage                                    1.2.840.10008.5.1.4.1.1.88.65
    XRayRadiationDoseSRStorage                           1.2.840.10008.5.1.4.1.1.88.67
    ColonCADSRStorage                                    1.2.840.10008.5.1.4.1.1.88.69
    ImplantationPlanSRStorage                            1.2.840.10008.5.1.4.1.1.88.70
    EncapsulatedPDFStorage                               1.2.840.10008.5.1.4.1.1.104.1
    EncapsulatedCDAStorage                               1.2.840.10008.5.1.4.1.1.104.2
    PositronEmissionTomographyImageStorage               1.2.840.10008.5.1.4.1.1.128
    LegacyConvertedEnhancedPETImageStorage               1.2.840.10008.5.1.4.1.1.128.1
    RETIRED_StandalonePETCurveStorage                    1.2.840.10008.5.1.4.1.1.129
    EnhancedPETImageStorage                              1.2.840.10008.5.1.4.1.1.130
    BasicStructuredDisplayStorage                        1.2.840.10008.5.1.4.1.1.131
    RTImageStorage                                       1.2.840.10008.5.1.4.1.1.481.1
    RTDoseStorage                                        1.2.840.10008.5.1.4.1.1.481.2
    RTStructureSetStorage                                1.2.840.10008.5.1.4.1.1.481.3
    RTBeamsTreatmentRecordStorage                        1.2.840.10008.5.1.4.1.1.481.4
    RTPlanStorage                                        1.2.840.10008.5.1.4.1.1.481.5
    RTBrachyTreatmentRecordStorage                       1.2.840.10008.5.1.4.1.1.481.6
    RTTreatmentSummaryRecordStorage                      1.2.840.10008.5.1.4.1.1.481.7
    RTIonPlanStorage                                     1.2.840.10008.5.1.4.1.1.481.8
    RTIonBeamsTreatmentRecordStorage                     1.2.840.10008.5.1.4.1.1.481.9
    RTBeamsDeliveryInstructionStorage                    1.2.840.10008.5.1.4.34.7

The dcmqrscp application will propose presentation contexts for all of the abovementioned supported SOP Classes using the transfer syntaxes:

    LittleEndianImplicitTransferSyntax                   1.2.840.10008.1.2
    LittleEndianExplicitTransferSyntax                   1.2.840.10008.1.2.1
    BigEndianExplicitTransferSyntax                      1.2.840.10008.1.2.2

This default behavior can be changed with the –propose options (see above). Depending on these options, the following transfer syntaxes are supported:

    LittleEndianImplicitTransferSyntax                   1.2.840.10008.1.2
    LittleEndianExplicitTransferSyntax                   1.2.840.10008.1.2.1
    DeflatedExplicitVRLittleEndianTransferSyntax         1.2.840.10008.1.2.1.99 (*)
    BigEndianExplicitTransferSyntax                      1.2.840.10008.1.2.2
    JPEGProcess1TransferSyntax                           1.2.840.10008.1.2.4.50
    JPEGProcess2_4TransferSyntax                         1.2.840.10008.1.2.4.51
    JPEGProcess14SV1TransferSyntax                       1.2.840.10008.1.2.4.70
    JPEGLSLosslessTransferSyntax                         1.2.840.10008.1.2.4.80
    JPEGLSLossyTransferSyntax                            1.2.840.10008.1.2.4.81
    JPEG2000LosslessOnlyTransferSyntax                   1.2.840.10008.1.2.4.90
    JPEG2000TransferSyntax                               1.2.840.10008.1.2.4.91
    MPEG2MainProfileAtMainLevelTransferSyntax            1.2.840.10008.1.2.4.100
    MPEG2MainProfileAtHighLevelTransferSyntax            1.2.840.10008.1.2.4.101
    MPEG4HighProfileLevel4_1TransferSyntax               1.2.840.10008.1.2.4.102
    MPEG4BDcompatibleHighProfileLevel4_1TransferSyntax   1.2.840.10008.1.2.4.103
    MPEG4HighProfileLevel4_2_For2DVideoTransferSyntax    1.2.840.10008.1.2.4.104
    MPEG4HighProfileLevel4_2_For3DVideoTransferSyntax    1.2.840.10008.1.2.4.105
    MPEG4StereoHighProfileLevel4_2TransferSyntax         1.2.840.10008.1.2.4.106
    HEVCMainProfileLevel5_1TransferSyntax                1.2.840.10008.1.2.4.107
    HEVCMain10ProfileLevel5_1TransferSyntax              1.2.840.10008.1.2.4.108
    RLELosslessTransferSyntax                            1.2.840.10008.1.2.5

(*) if compiled with zlib support enabled (see –version output)

The dcmqrscp application does not support extended negotiation.

Presentation contexts for other SOP Classes and/or transfer syntaxes may be configured via the –assoc-config-file option by selecting an appropriate profile for outgoing associations. The selected profile will completely override the above mentioned default configuration.

### SCP Conformance

The dcmqrscp application supports the following SOP Classes as an SCP:

    VerificationSOPClass                                 1.2.840.10008.1.1

    FINDPatientRootQueryRetrieveInformationModel         1.2.840.10008.5.1.4.1.2.1.1
    FINDPatientStudyOnlyQueryRetrieveInformationModel    1.2.840.10008.5.1.4.1.2.3.1
    FINDStudyRootQueryRetrieveInformationModel           1.2.840.10008.5.1.4.1.2.2.1
    GETPatientRootQueryRetrieveInformationModel          1.2.840.10008.5.1.4.1.2.1.3
    GETPatientStudyOnlyQueryRetrieveInformationModel     1.2.840.10008.5.1.4.1.2.3.3
    GETStudyRootQueryRetrieveInformationModel            1.2.840.10008.5.1.4.1.2.2.3
    MOVEPatientRootQueryRetrieveInformationModel         1.2.840.10008.5.1.4.1.2.1.2
    MOVEPatientStudyOnlyQueryRetrieveInformationModel    1.2.840.10008.5.1.4.1.2.3.2
    MOVEStudyRootQueryRetrieveInformationModel           1.2.840.10008.5.1.4.1.2.2.2

    RETIRED_StoredPrintStorage                           1.2.840.10008.5.1.1.27
    RETIRED_HardcopyGrayscaleImageStorage                1.2.840.10008.5.1.1.29
    RETIRED_HardcopyColorImageStorage                    1.2.840.10008.5.1.1.30
    ComputedRadiographyImageStorage                      1.2.840.10008.5.1.4.1.1.1
    DigitalXRayImageStorageForPresentation               1.2.840.10008.5.1.4.1.1.1.1
    DigitalXRayImageStorageForProcessing                 1.2.840.10008.5.1.4.1.1.1.1.1
    DigitalMammographyXRayImageStorageForPresentation    1.2.840.10008.5.1.4.1.1.1.2
    DigitalMammographyXRayImageStorageForProcessing      1.2.840.10008.5.1.4.1.1.1.2.1
    DigitalIntraOralXRayImageStorageForPresentation      1.2.840.10008.5.1.4.1.1.1.3
    DigitalIntraOralXRayImageStorageForProcessing        1.2.840.10008.5.1.4.1.1.1.3.1
    CTImageStorage                                       1.2.840.10008.5.1.4.1.1.2
    EnhancedCTImageStorage                               1.2.840.10008.5.1.4.1.1.2.1
    LegacyConvertedEnhancedCTImageStorage                1.2.840.10008.5.1.4.1.1.2.2
    RETIRED_UltrasoundMultiframeImageStorage             1.2.840.10008.5.1.4.1.1.3
    UltrasoundMultiframeImageStorage                     1.2.840.10008.5.1.4.1.1.3.1
    MRImageStorage                                       1.2.840.10008.5.1.4.1.1.4
    EnhancedMRImageStorage                               1.2.840.10008.5.1.4.1.1.4.1
    MRSpectroscopyStorage                                1.2.840.10008.5.1.4.1.1.4.2
    EnhancedMRColorImageStorage                          1.2.840.10008.5.1.4.1.1.4.3
    LegacyConvertedEnhancedMRImageStorage                1.2.840.10008.5.1.4.1.1.4.4
    RETIRED_NuclearMedicineImageStorage                  1.2.840.10008.5.1.4.1.1.5
    RETIRED_UltrasoundImageStorage                       1.2.840.10008.5.1.4.1.1.6
    UltrasoundImageStorage                               1.2.840.10008.5.1.4.1.1.6.1
    EnhancedUSVolumeStorage                              1.2.840.10008.5.1.4.1.1.6.2
    PhotoacousticImageStorage                            1.2.840.10008.5.1.4.1.1.6.3
    SecondaryCaptureImageStorage                         1.2.840.10008.5.1.4.1.1.7
    MultiframeSingleBitSecondaryCaptureImageStorage      1.2.840.10008.5.1.4.1.1.7.1
    MultiframeGrayscaleByteSecondaryCaptureImageStorage  1.2.840.10008.5.1.4.1.1.7.2
    MultiframeGrayscaleWordSecondaryCaptureImageStorage  1.2.840.10008.5.1.4.1.1.7.3
    MultiframeTrueColorSecondaryCaptureImageStorage      1.2.840.10008.5.1.4.1.1.7.4
    RETIRED_StandaloneOverlayStorage                     1.2.840.10008.5.1.4.1.1.8
    RETIRED_StandaloneCurveStorage                       1.2.840.10008.5.1.4.1.1.9
    DRAFT_WaveformStorage                                1.2.840.10008.5.1.4.1.1.9.1
    TwelveLeadECGWaveformStorage                         1.2.840.10008.5.1.4.1.1.9.1.1
    GeneralECGWaveformStorage                            1.2.840.10008.5.1.4.1.1.9.1.2
    AmbulatoryECGWaveformStorage                         1.2.840.10008.5.1.4.1.1.9.1.3
    General32BitECGWaveformStorage                       1.2.840.10008.5.1.4.1.1.9.1.4
    HemodynamicWaveformStorage                           1.2.840.10008.5.1.4.1.1.9.2.1
    CardiacElectrophysiologyWaveformStorage              1.2.840.10008.5.1.4.1.1.9.3.1
    BasicVoiceAudioWaveformStorage                       1.2.840.10008.5.1.4.1.1.9.4.1
    GeneralAudioWaveformStorage                          1.2.840.10008.5.1.4.1.1.9.4.2
    ArterialPulseWaveformStorage                         1.2.840.10008.5.1.4.1.1.9.5.1
    RespiratoryWaveformStorage                           1.2.840.10008.5.1.4.1.1.9.6.1
    MultichannelRespiratoryWaveformStorage               1.2.840.10008.5.1.4.1.1.9.6.2
    RoutineScalpElectroencephalogramWaveformStorage      1.2.840.10008.5.1.4.1.1.9.7.1
    ElectromyogramWaveformStorage                        1.2.840.10008.5.1.4.1.1.9.7.2
    ElectrooculogramWaveformStorage                      1.2.840.10008.5.1.4.1.1.9.7.3
    SleepElectroencephalogramWaveformStorage             1.2.840.10008.5.1.4.1.1.9.7.4
    BodyPositionWaveformStorage                          1.2.840.10008.5.1.4.1.1.9.8.1
    WaveformPresentationStateStorage                     1.2.840.10008.5.1.4.1.1.9.100.1
    WaveformAcquisitionPresentationStateStorage          1.2.840.10008.5.1.4.1.1.9.100.2
    RETIRED_StandaloneModalityLUTStorage                 1.2.840.10008.5.1.4.1.1.10
    RETIRED_StandaloneVOILUTStorage                      1.2.840.10008.5.1.4.1.1.11
    GrayscaleSoftcopyPresentationStateStorage            1.2.840.10008.5.1.4.1.1.11.1
    ColorSoftcopyPresentationStateStorage                1.2.840.10008.5.1.4.1.1.11.2
    PseudoColorSoftcopyPresentationStateStorage          1.2.840.10008.5.1.4.1.1.11.3
    BlendingSoftcopyPresentationStateStorage             1.2.840.10008.5.1.4.1.1.11.4
    XAXRFGrayscaleSoftcopyPresentationStateStorage       1.2.840.10008.5.1.4.1.1.11.5
    GrayscalePlanarMPRVolumetricPresentationStateStorage 1.2.840.10008.5.1.4.1.1.11.6
    CompositingPlanarMPRVolumetricPresent.StateStorage   1.2.840.10008.5.1.4.1.1.11.7
    AdvancedBlendingPresentationStateStorage             1.2.840.10008.5.1.4.1.1.11.8
    VolumeRenderingVolumetricPresentationStateStorage    1.2.840.10008.5.1.4.1.1.11.9
    SegmentedVolumeRenderingVolumetricPres.StateStorage  1.2.840.10008.5.1.4.1.1.11.10
    MultipleVolumeRenderingVolumetricPres.StateStorage   1.2.840.10008.5.1.4.1.1.11.11
    VariableModalityLUTSoftcopyPresentationStateStorage  1.2.840.10008.5.1.4.1.1.11.12
    XRayAngiographicImageStorage                         1.2.840.10008.5.1.4.1.1.12.1
    EnhancedXAImageStorage                               1.2.840.10008.5.1.4.1.1.12.1.1
    XRayRadiofluoroscopicImageStorage                    1.2.840.10008.5.1.4.1.1.12.2
    EnhancedXRFImageStorage                              1.2.840.10008.5.1.4.1.1.12.2.1
    RETIRED_XRayAngiographicBiPlaneImageStorage          1.2.840.10008.5.1.4.1.1.12.3
    XRay3DAngiographicImageStorage                       1.2.840.10008.5.1.4.1.1.13.1.1
    XRay3DCraniofacialImageStorage                       1.2.840.10008.5.1.4.1.1.13.1.2
    BreastTomosynthesisImageStorage                      1.2.840.10008.5.1.4.1.1.13.1.3
    BreastProjectionXRayImageStorageForPresentation      1.2.840.10008.5.1.4.1.1.13.1.4
    BreastProjectionXRayImageStorageForProcessing        1.2.840.10008.5.1.4.1.1.13.1.5
    IntravascularOpt.Coh.Tom.ImageStorageForPresentation 1.2.840.10008.5.1.4.1.1.14.1
    IntravascularOpt.Coh.Tom.ImageStorageForProcessing   1.2.840.10008.5.1.4.1.1.14.2
    NuclearMedicineImageStorage                          1.2.840.10008.5.1.4.1.1.20
    ParametricMapStorage                                 1.2.840.10008.5.1.4.1.1.30
    RawDataStorage                                       1.2.840.10008.5.1.4.1.1.66
    SpatialRegistrationStorage                           1.2.840.10008.5.1.4.1.1.66.1
    SpatialFiducialsStorage                              1.2.840.10008.5.1.4.1.1.66.2
    DeformableSpatialRegistrationStorage                 1.2.840.10008.5.1.4.1.1.66.3
    SegmentationStorage                                  1.2.840.10008.5.1.4.1.1.66.4
    SurfaceSegmentationStorage                           1.2.840.10008.5.1.4.1.1.66.5
    TractographyResultsStorage                           1.2.840.10008.5.1.4.1.1.66.6
    LabelMapSegmentationStorage                          1.2.840.10008.5.1.4.1.1.66.7
    HeightMapSegmentationStorage                         1.2.840.10008.5.1.4.1.1.66.8
    RealWorldValueMappingStorage                         1.2.840.10008.5.1.4.1.1.67
    SurfaceScanMeshStorage                               1.2.840.10008.5.1.4.1.1.68.1
    SurfaceScanPointCloudStorage                         1.2.840.10008.5.1.4.1.1.68.2
    RETIRED_VLImageStorage                               1.2.840.10008.5.1.4.1.1.77.1
    VLEndoscopicImageStorage                             1.2.840.10008.5.1.4.1.1.77.1.1
    VideoEndoscopicImageStorage                          1.2.840.10008.5.1.4.1.1.77.1.1.1
    VLMicroscopicImageStorage                            1.2.840.10008.5.1.4.1.1.77.1.2
    VideoMicroscopicImageStorage                         1.2.840.10008.5.1.4.1.1.77.1.2.1
    VLSlideCoordinatesMicroscopicImageStorage            1.2.840.10008.5.1.4.1.1.77.1.3
    VLPhotographicImageStorage                           1.2.840.10008.5.1.4.1.1.77.1.4
    VideoPhotographicImageStorage                        1.2.840.10008.5.1.4.1.1.77.1.4.1
    OphthalmicPhotography8BitImageStorage                1.2.840.10008.5.1.4.1.1.77.1.5.1
    OphthalmicPhotography16BitImageStorage               1.2.840.10008.5.1.4.1.1.77.1.5.2
    StereometricRelationshipStorage                      1.2.840.10008.5.1.4.1.1.77.1.5.3
    OphthalmicTomographyImageStorage                     1.2.840.10008.5.1.4.1.1.77.1.5.4
    WideFieldOphthalmicPhoto.Stereogr.Proj.ImageStorage  1.2.840.10008.5.1.4.1.1.77.1.5.5
    WideFieldOphthalmicPhotogr.3DCoordinatesImageStorage 1.2.840.10008.5.1.4.1.1.77.1.5.6
    OphthalmicOpticalCoherenceTomogr.EnFaceImageStorage  1.2.840.10008.5.1.4.1.1.77.1.5.7
    OphthalmicOpticalCoh.Tomogr.BscanVolumeAnalysisStor. 1.2.840.10008.5.1.4.1.1.77.1.5.8
    VLWholeSlideMicroscopyImageStorage                   1.2.840.10008.5.1.4.1.1.77.1.6
    DermoscopicPhotographyImageStorage                   1.2.840.10008.5.1.4.1.1.77.1.7
    ConfocalMicroscopyImageStorage                       1.2.840.10008.5.1.4.1.1.77.1.8
    ConfocalMicroscopyTiledPyramidalImageStorage         1.2.840.10008.5.1.4.1.1.77.1.9
    RETIRED_VLMultiframeImageStorage                     1.2.840.10008.5.1.4.1.1.77.2
    LensometryMeasurementsStorage                        1.2.840.10008.5.1.4.1.1.78.1
    AutorefractionMeasurementsStorage                    1.2.840.10008.5.1.4.1.1.78.2
    KeratometryMeasurementsStorage                       1.2.840.10008.5.1.4.1.1.78.3
    SubjectiveRefractionMeasurementsStorage              1.2.840.10008.5.1.4.1.1.78.4
    VisualAcuityMeasurementsStorage                      1.2.840.10008.5.1.4.1.1.78.5
    SpectaclePrescriptionReportStorage                   1.2.840.10008.5.1.4.1.1.78.6
    OphthalmicAxialMeasurementsStorage                   1.2.840.10008.5.1.4.1.1.78.7
    IntraocularLensCalculationsStorage                   1.2.840.10008.5.1.4.1.1.78.8
    MacularGridThicknessAndVolumeReportStorage           1.2.840.10008.5.1.4.1.1.79.1
    OphthalmicVisualFieldStaticPerimetryMeasurementsSt.  1.2.840.10008.5.1.4.1.1.80.1
    OphthalmicThicknessMapStorage                        1.2.840.10008.5.1.4.1.1.81.1
    CornealTopographyMapStorage                          1.2.840.10008.5.1.4.1.1.82.1
    DRAFT_SRTextStorage                                  1.2.840.10008.5.1.4.1.1.88.1
    DRAFT_SRAudioStorage                                 1.2.840.10008.5.1.4.1.1.88.2
    DRAFT_SRDetailStorage                                1.2.840.10008.5.1.4.1.1.88.3
    DRAFT_SRComprehensiveStorage                         1.2.840.10008.5.1.4.1.1.88.4
    BasicTextSRStorage                                   1.2.840.10008.5.1.4.1.1.88.11
    EnhancedSRStorage                                    1.2.840.10008.5.1.4.1.1.88.22
    ComprehensiveSRStorage                               1.2.840.10008.5.1.4.1.1.88.33
    Comprehensive3DSRStorage                             1.2.840.10008.5.1.4.1.1.88.34
    ExtensibleSRStorage                                  1.2.840.10008.5.1.4.1.1.88.35
    ProcedureLogStorage                                  1.2.840.10008.5.1.4.1.1.88.40
    MammographyCADSRStorage                              1.2.840.10008.5.1.4.1.1.88.50
    KeyObjectSelectionDocumentStorage                    1.2.840.10008.5.1.4.1.1.88.59
    ChestCADSRStorage                                    1.2.840.10008.5.1.4.1.1.88.65
    XRayRadiationDoseSRStorage                           1.2.840.10008.5.1.4.1.1.88.67
    RadiopharmaceuticalRadiationDoseSRStorage            1.2.840.10008.5.1.4.1.1.88.68
    ColonCADSRStorage                                    1.2.840.10008.5.1.4.1.1.88.69
    ImplantationPlanSRStorage                            1.2.840.10008.5.1.4.1.1.88.70
    AcquisitionContextSRStorage                          1.2.840.10008.5.1.4.1.1.88.71
    SimplifiedAdultEchoSRStorage                         1.2.840.10008.5.1.4.1.1.88.72
    PatientRadiationDoseSRStorage                        1.2.840.10008.5.1.4.1.1.88.73
    PlannedImagingAgentAdministrationSRStorage           1.2.840.10008.5.1.4.1.1.88.74
    PerformedImagingAgentAdministrationSRStorage         1.2.840.10008.5.1.4.1.1.88.75
    EnhancedXRayRadiationDoseSRStorage                   1.2.840.10008.5.1.4.1.1.88.76
    WaveformAnnotationSRStorage                          1.2.840.10008.5.1.4.1.1.88.77
    ContentAssessmentResultsStorage                      1.2.840.10008.5.1.4.1.1.90.1
    MicroscopyBulkSimpleAnnotationsStorage               1.2.840.10008.5.1.4.1.1.91.1
    EncapsulatedPDFStorage                               1.2.840.10008.5.1.4.1.1.104.1
    EncapsulatedCDAStorage                               1.2.840.10008.5.1.4.1.1.104.2
    EncapsulatedSTLStorage                               1.2.840.10008.5.1.4.1.1.104.3
    EncapsulatedOBJStorage                               1.2.840.10008.5.1.4.1.1.104.4
    EncapsulatedMTLStorage                               1.2.840.10008.5.1.4.1.1.104.5
    PositronEmissionTomographyImageStorage               1.2.840.10008.5.1.4.1.1.128
    LegacyConvertedEnhancedPETImageStorage               1.2.840.10008.5.1.4.1.1.128.1
    RETIRED_StandalonePETCurveStorage                    1.2.840.10008.5.1.4.1.1.129
    EnhancedPETImageStorage                              1.2.840.10008.5.1.4.1.1.130
    BasicStructuredDisplayStorage                        1.2.840.10008.5.1.4.1.1.131
    CTPerformedProcedureProtocolStorage                  1.2.840.10008.5.1.4.1.1.200.2
    XAPerformedProcedureProtocolStorage                  1.2.840.10008.5.1.4.1.1.200.8
    RTImageStorage                                       1.2.840.10008.5.1.4.1.1.481.1
    RTDoseStorage                                        1.2.840.10008.5.1.4.1.1.481.2
    RTStructureSetStorage                                1.2.840.10008.5.1.4.1.1.481.3
    RTBeamsTreatmentRecordStorage                        1.2.840.10008.5.1.4.1.1.481.4
    RTPlanStorage                                        1.2.840.10008.5.1.4.1.1.481.5
    RTBrachyTreatmentRecordStorage                       1.2.840.10008.5.1.4.1.1.481.6
    RTTreatmentSummaryRecordStorage                      1.2.840.10008.5.1.4.1.1.481.7
    RTIonPlanStorage                                     1.2.840.10008.5.1.4.1.1.481.8
    RTIonBeamsTreatmentRecordStorage                     1.2.840.10008.5.1.4.1.1.481.9
    RTPhysicianIntentStorage                             1.2.840.10008.5.1.4.1.1.481.10
    RTSegmentAnnotationStorage                           1.2.840.10008.5.1.4.1.1.481.11
    RTRadiationSetStorage                                1.2.840.10008.5.1.4.1.1.481.12
    CArmPhotonElectronRadiationStorage                   1.2.840.10008.5.1.4.1.1.481.13
    TomotherapeuticRadiationStorage                      1.2.840.10008.5.1.4.1.1.481.14
    RoboticArmRadiationStorage                           1.2.840.10008.5.1.4.1.1.481.15
    RTRadiationRecordSetStorage                          1.2.840.10008.5.1.4.1.1.481.16
    RTRadiationSalvageRecordStorage                      1.2.840.10008.5.1.4.1.1.481.17
    TomotherapeuticRadiationRecordStorage                1.2.840.10008.5.1.4.1.1.481.18
    CArmPhotonElectronRadiationRecordStorage             1.2.840.10008.5.1.4.1.1.481.19
    RoboticRadiationRecordStorage                        1.2.840.10008.5.1.4.1.1.481.20
    RTRadiationSetDeliveryInstructionStorage             1.2.840.10008.5.1.4.1.1.481.21
    RTTreatmentPreparationStorage                        1.2.840.10008.5.1.4.1.1.481.22
    EnhancedRTImageStorage                               1.2.840.10008.5.1.4.1.1.481.23
    EnhancedContinuousRTImageStorage                     1.2.840.10008.5.1.4.1.1.481.24
    RTPatientPositionAcquisitionInstructionStorage       1.2.840.10008.5.1.4.1.1.481.25
    DICOS_CTImageStorage                                 1.2.840.10008.5.1.4.1.1.501.1
    DICOS_DigitalXRayImageStorageForPresentation         1.2.840.10008.5.1.4.1.1.501.2.1
    DICOS_DigitalXRayImageStorageForProcessing           1.2.840.10008.5.1.4.1.1.501.2.2
    DICOS_ThreatDetectionReportStorage                   1.2.840.10008.5.1.4.1.1.501.3
    DICOS_2DAITStorage                                   1.2.840.10008.5.1.4.1.1.501.4
    DICOS_3DAITStorage                                   1.2.840.10008.5.1.4.1.1.501.5
    DICOS_QuadrupoleResonanceStorage                     1.2.840.10008.5.1.4.1.1.501.6
    DICONDE_EddyCurrentImageStorage                      1.2.840.10008.5.1.4.1.1.601.1
    DICONDE_EddyCurrentMultiframeImageStorage            1.2.840.10008.5.1.4.1.1.601.2
    DICONDE_ThermographyImageStorage                     1.2.840.10008.5.1.4.1.1.601.3
    DICONDE_ThermographyMultiFrameImageStorage           1.2.840.10008.5.1.4.1.1.601.4
    DICONDE_UltrasoundWaveformStorage                    1.2.840.10008.5.1.4.1.1.601.5
    DRAFT_RTBeamsDeliveryInstructionStorage              1.2.840.10008.5.1.4.34.1
    RTBeamsDeliveryInstructionStorage                    1.2.840.10008.5.1.4.34.7
    RTBrachyApplicationSetupDeliveryInstructionStorage   1.2.840.10008.5.1.4.34.10

    PrivateShutdownSOPClass                              1.2.276.0.7230010.3.4.1915765545.18030.917282194.0

The dcmqrscp application will accept presentation contexts for all of the above mentioned supported SOP Classes using any of the transfer syntaxes:

    LittleEndianImplicitTransferSyntax                   1.2.840.10008.1.2
    LittleEndianExplicitTransferSyntax                   1.2.840.10008.1.2.1
    BigEndianExplicitTransferSyntax                      1.2.840.10008.1.2.2

The dcmqrscp application will prefer transfer syntaxes having an explicit encoding over the default implicit transfer syntax. If dcmqrscp is running on big-endian hardware it will prefer BigEndianExplicit to LittleEndianExplicit transfer syntax (and vice versa). This behavior can be changed with the –prefer options (see above). Depending on these options, the following transfer syntaxes are supported:

    LittleEndianImplicitTransferSyntax                   1.2.840.10008.1.2
    LittleEndianExplicitTransferSyntax                   1.2.840.10008.1.2.1
    DeflatedExplicitVRLittleEndianTransferSyntax         1.2.840.10008.1.2.1.99
    BigEndianExplicitTransferSyntax                      1.2.840.10008.1.2.2
    JPEGProcess1TransferSyntax                           1.2.840.10008.1.2.4.50
    JPEGProcess2_4TransferSyntax                         1.2.840.10008.1.2.4.51
    JPEGProcess14SV1TransferSyntax                       1.2.840.10008.1.2.4.70
    JPEGLSLosslessTransferSyntax                         1.2.840.10008.1.2.4.80
    JPEGLSLossyTransferSyntax                            1.2.840.10008.1.2.4.81
    JPEG2000LosslessOnlyTransferSyntax                   1.2.840.10008.1.2.4.90
    JPEG2000TransferSyntax                               1.2.840.10008.1.2.4.91
    MPEG2MainProfileAtMainLevelTransferSyntax            1.2.840.10008.1.2.4.100
    MPEG2MainProfileAtHighLevelTransferSyntax            1.2.840.10008.1.2.4.101
    MPEG4HighProfileLevel4_1TransferSyntax               1.2.840.10008.1.2.4.102
    MPEG4BDcompatibleHighProfileLevel4_1TransferSyntax   1.2.840.10008.1.2.4.103
    MPEG4HighProfileLevel4_2_For2DVideoTransferSyntax    1.2.840.10008.1.2.4.104
    MPEG4HighProfileLevel4_2_For3DVideoTransferSyntax    1.2.840.10008.1.2.4.105
    MPEG4StereoHighProfileLevel4_2TransferSyntax         1.2.840.10008.1.2.4.106
    HEVCMainProfileLevel5_1TransferSyntax                1.2.840.10008.1.2.4.107
    HEVCMain10ProfileLevel5_1TransferSyntax              1.2.840.10008.1.2.4.108
    RLELosslessTransferSyntax                            1.2.840.10008.1.2.5

The dcmqrscp application does not support extended negotiation.

Presentation contexts for other SOP Classes and Transfer Syntax may be configured via the –assoc-config-file option by selecting an appropriate profile for incoming associations. The selected profile will override only the above mentioned storage SOP classes, dcmqrscp will accept contexts with the above mentioned FIND, GET, MOVE and private shutdown SOP Classes additionally to the ones defined in the selected profile. Please note that an appropriate profile for role negotiation must be defined and used for enabling GET support.

### Query Keys

The dcmqrscp application supports the following attributes as query keys.

Query/Retrieve Level: PATIENT (or STUDY for the Study Root Q/R model)

    (0010,0010) PatientName
    (0010,0020) PatientID
    (0010,0021) IssuerOfPatientID
    (0010,0030) PatientBirthDate
    (0010,0032) PatientBirthTime
    (0010,0040) PatientSex
    (0010,1000) OtherPatientIDs (retired)
    (0010,1001) OtherPatientNames
    (0010,2160) EthnicGroup (retired)
    (0010,4000) PatientComments

Query/Retrieve Level: STUDY

    (0008,0020) StudyDate
    (0008,0030) StudyTime
    (0008,0050) AccessionNumber
    (0008,0090) ReferringPhysicianName
    (0008,1030) StudyDescription
    (0008,1060) NameOfPhysiciansReadingStudy
    (0008,1080) AdmittingDiagnosesDescription
    (0010,1010) PatientAge
    (0010,1020) PatientSize
    (0010,1030) PatientWeight
    (0010,2180) Occupation
    (0010,21B0) AdditionalPatientHistory
    (0020,000D) StudyInstanceUID
    (0020,0010) StudyID
    (0020,1070) OtherStudyNumbers (retired)

Query/Retrieve Level: SERIES

    (0008,0060) Modality
    (0020,000E) SeriesInstanceUID
    (0020,0011) SeriesNumber

Query/Retrieve Level: IMAGE

    (0008,0018) SOPInstanceUID
    (0020,0013) InstanceNumber

## Configuration

The dcmqrscp program uses the same configuration file as the dcmqrti program. See the documentation on configuration for more information.

## Access Control

When compiled on Unix platforms with TCP wrapper support, host-based access control can be enabled with the –access-control command line option. In this case the access control rules defined in the system's host access control tables for dcmqrscp are enforced. The default locations of the host access control tables are /etc/hosts.allow and /etc/hosts.deny. Further details are described in hosts_access(5).

# LOGGING

The level of logging output of the various command line tools and underlying libraries can be specified by the user. By default, only errors and warnings are written to the standard error stream. Using option –verbose also informational messages like processing details are reported. Option –debug can be used to get more details on the internal activity, e.g. for debugging purposes. Other logging levels can be selected using option –log-level. In –quiet mode only fatal errors are reported. In such very severe error events, the application will usually terminate. For more details on the different logging levels, see documentation of module "oflog".

In case the logging output should be written to file (optionally with logfile rotation), to syslog (Unix) or the event log (Windows) option –log-config can be used. This configuration file also allows for directing only certain messages to a particular output stream and for filtering certain messages based on the module or application where they are generated. An example configuration file is provided in <etcdir>/logger.cfg.

# COMMAND LINE

All command line tools use the following notation for parameters: square brackets enclose optional values (0-1), three trailing dots indicate that multiple values are allowed (1-n), a combination of both means 0 to n values.

Command line options are distinguished from parameters by a leading '+' or '-' sign, respectively. Usually, order and position of command line options are arbitrary (i.e. they can appear anywhere). However, if options are mutually exclusive the rightmost appearance is used. This behavior conforms to the standard evaluation rules of common Unix shells.

In addition, one or more command files can be specified using an '@' sign as a prefix to the filename (e.g. @command.txt). Such a command argument is replaced by the content of the corresponding text file (multiple whitespaces are treated as a single separator unless they appear between two quotation marks) prior to any further evaluation. Please note that a command file cannot contain another command file. This simple but effective approach allows one to summarize common combinations of options/parameters and avoids longish and confusing command lines (an example is provided in file <datadir>/dumppat.txt).

# ENVIRONMENT

The dcmqrscp utility will attempt to load DICOM data dictionaries specified in the DCMDICTPATH environment variable. By default, i.e. if the DCMDICTPATH environment variable is not set, the file <datadir>/dicom.dic will be loaded unless the dictionary is built into the application (default for Windows).

The default behavior should be preferred and the DCMDICTPATH environment variable only used when alternative data dictionaries are required. The DCMDICTPATH environment variable has the same format as the Unix shell PATH variable in that a colon (":") separates entries. On Windows systems, a semicolon (";") is used as a separator. The data dictionary code will attempt to load each file specified in the DCMDICTPATH environment variable. It is an error if no data dictionary can be loaded.

Depending on the command line options specified, the dcmqrscp utility will attempt to load character set mapping tables. This happens when DCMTK was compiled with the oficonv library (which is the default) and the mapping tables are not built into the library (default when DCMTK uses shared libraries).

The mapping table files are expected in DCMTK's <datadir>. The DCMICONVPATH environment variable can be used to specify a different location. If a different location is specified, those mapping tables also replace any built-in tables.

# FILES

<docdir>/dcmqrcnf.txt - configuration information
<docdir>/dcmqrset.txt - setup information
<etcdir>/dcmqrscp.cfg - example configuration file
<etcdir>/dcmqrprf.cfg - example configuration file for association profiles

# SEE ALSO

dcmqridx(1), dcmqrti(1)

# COPYRIGHT

Copyright (C) 1993-2025 by OFFIS e.V., Escherweg 2, 26121 Oldenburg, Germany.

Generated on Mon Dec 15 2025 for DCMTK Version 3.7.0 by Doxygen 1.9.1